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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal, State, Other


	Private Funding:
	No


	
	


Project Description: 
This project is located within Richfield Township, Lucas County, Ohio. The proposed work includes the resurfacing of US-20 from the Fulton-Lucas County Line to King Road. Storm sewers that are parallel to US-20 will be repaired or replaced. Bridge deck and culvert replacements will occur near Washburn Road. Turn lanes at Crissey and Herr Roads are also proposed. Additional right of way is needed at these turn lane locations. 
	STIP Reference #
	SLI 15,32


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(28) Bridge rehabilitation, reconstruction, or replacement or the construction of grade separation to replace existing at-grade railroad crossings, if the actions meet the constraints in 23 CFR 771.117(e). Examples include: Railroad projects that close or relocate at-grade crossings


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Not Present


	Endangered Species:
	No Impacts to Protected Species and Critical Habitat


	100-Year Floodplain:
	No Encroachment Within a Special Flood Hazard Area (SFHA)


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	Minimum Potential to Cause Effect - Appendix B


	Cultural Resources Coordination - ODOT Approval Date:
	02/13/2015


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Yes


	Hazardous Materials - OES Approval Date:
	04/29/2015


	Phase I ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes
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1. Access to adjacent properties will be maintained during construction by the contractor and ODOT. 
2. The contractor shall notify the project engineer a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including media outlets, local schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage by the contractor and ODOT.
4. If required by local ordinance, a construction noise plan note will be developed and implemented. 
5. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  
6. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut outside the construction limits shown on the plans, approval must be given by the District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized.  
7. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
8. Due to the known presence of Ohio threatened Bandings turtle and Ohio threatened spotted turtle within the project area, if any turtle is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.  
9. Due to the location of the project within the globally rare Oak Openings region, there shall be no earth disturbance starting 3 feet from the edge of the existing pavement from LUC-120-11.2 to LUC-20-5.1.  No work shall be done over 3 feet off the existing pavement and care shall be taken to not disturb the existing vegetation in this area. 
10. This project is located in or near the source of public drinking water supplies. Do not perform equipment fueling within the locations identified in the table below.  If refueling of immobile equipment is necessary within these limits, provide secondary containment with enough capacity to completely contain and collect all potential liquid wastes in the event of a spill.  Do not perform maintenance activities associated with any viscous material that has potential to contaminate the groundwater.  All equipment or liquid containers shall be regularly checked for leaks prior to entering the restricted areas.  Identify all areas of fuel storage, equipment maintenance and spill kits on the Stormwater Pollution Prevention Plan.  All areas utilized by the Contractor not included within the table below and not in the project limits shall be assessed for potential groundwater contamination and be indicated on the Stormwater Pollution Prevention Plan or Spill Prevention Control and Countermeasures Plan. The Contractor shall immediately take steps to mitigate any event, such as a spill of fuels, oils, or chemicals. Any such spill or event shall be reported immediately to the emergency contact listed below for each drinking water source.  If the spill is a reportable amount, the Contractor should contact Ohio EPA Environmental Response and Revitalization (419-373-3031 or 800-282-9378) for cleanup of the spill.

Drinking Water Source 	           Restricted Refueling and Maintenance Area 	Emergency Contact Information
Spuyten Duyval Golf Club 	Between Crissey Rd and Murd Rd	                         419-829-2891
The Roadhouse	           Between N Raab Rd and Richfield Center Rd	         419-829-2223
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1. Access to adjacent properties will be maintained during construction by the contractor and ODOT. 
2. The contractor shall notify the project engineer a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including media outlets, local schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage by the contractor and ODOT.
4. If required by local ordinance, a construction noise plan note will be developed and implemented. 
5. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  
6. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut outside the construction limits shown on the plans, approval must be given by the District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized.  
7. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
8. Due to the known presence of Ohio threatened Bandings turtle and Ohio threatened spotted turtle within the project area, if any turtle is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.  
9. Due to the location of the project within the globally rare Oak Openings region, there shall be no earth disturbance starting 3 feet from the edge of the existing pavement from LUC-120-11.2 to LUC-20-5.1.  No work shall be done over 3 feet off the existing pavement and care shall be taken to not disturb the existing vegetation in this area. 
10. This project is located in or near the source of public drinking water supplies. Do not perform equipment fueling within the locations identified in the table below.  If refueling of immobile equipment is necessary within these limits, provide secondary containment with enough capacity to completely contain and collect all potential liquid wastes in the event of a spill.  Do not perform maintenance activities associated with any viscous material that has potential to contaminate the groundwater.  All equipment or liquid containers shall be regularly checked for leaks prior to entering the restricted areas.  Identify all areas of fuel storage, equipment maintenance and spill kits on the Stormwater Pollution Prevention Plan.  All areas utilized by the Contractor not included within the table below and not in the project limits shall be assessed for potential groundwater contamination and be indicated on the Stormwater Pollution Prevention Plan or Spill Prevention Control and Countermeasures Plan. The Contractor shall immediately take steps to mitigate any event, such as a spill of fuels, oils, or chemicals. Any such spill or event shall be reported immediately to the emergency contact listed below for each drinking water source.  If the spill is a reportable amount, the Contractor should contact Ohio EPA Environmental Response and Revitalization (419-373-3031 or 800-282-9378) for cleanup of the spill.

Drinking Water Source 	           Restricted Refueling and Maintenance Area 	Emergency Contact Information
Spuyten Duyval Golf Club 	Between Crissey Rd and Murd Rd	                         419-829-2891
The Roadhouse	           Between N Raab Rd and Richfield Center Rd	         419-829-2223
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	May 17, 2016
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	May 17, 2016
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