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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
Perform repairs on three bridges including the US 6 bridge over the Maumee River in Henry County, a SR 2 bridge over a railroad in Ottawa County, and a SR 2 bridge over the Sandusky Bay in Ottawa County as described in more detail below: 
HEN-6-16.50 (over Maumee River): Replace Strip seals in both the rear and forward abutment expansion joints.
OTT-2-23.06 (over railroad): Replace bearings on both the rear and forward abutments. Realign all of the pier non-fixed bearings.
OTT-2-28.39 (over Sandusky Bay): Perform deck repairs along conduit running transversely through the bridge deck. Epoxy inject cracks and repair concrete parapets.
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	(3) No Historic Properties Affected


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. Access to adjacent properties will be maintained during construction by the contractor.
2. The contractor shall perform all work within the existing right of way. 
3. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
4. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
5. If required by local ordinance, a construction noise plan note will be developed and implemented.
6. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.
7. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream.
8. Work on the structures shall not be performed between the bridge deck and the water.  Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water. 
9. Coordination will be sent to the United States Coast Guard (USCG) at least 14 prior to starting work on the OTT-2-28.39 bridge over Sandusky Bay.
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10. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut, approval must be given by the District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized.  
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1. Access to adjacent properties will be maintained during construction by the contractor.
2. The contractor shall perform all work within the existing right of way. 
3. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
4. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
5. If required by local ordinance, a construction noise plan note will be developed and implemented.
6. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.
7. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream.
8. Work on the structures shall not be performed between the bridge deck and the water.  Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water. 
9. Coordination will be sent to the United States Coast Guard (USCG) at least 14 prior to starting work on the OTT-2-28.39 bridge over Sandusky Bay.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	December 17, 2015

	Stacy Schimmoeller PROGRAM ADMIN 3
	December 17, 2015
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[bookmark: _Toc256000009]General
Aerial Map.pdf
County Map.pdf
USGS Quadrangle Topographical Map.pdf
[bookmark: _Toc256000010]ESA
ESA Screening Map.pdf
Oil and Gas map.pdf
[bookmark: _Toc256000011]Cultural Resources
Buckeye Assets Mapping.pdf
OHPO Cultural Map.pdf
[bookmark: _Toc256000012]Ecological
OBD Ecological Map.pdf
Wetlands Map.pdf
[bookmark: _Toc256000013]Other Resources
Public Water Supply Map.pdf
Well Log Data.pdf
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Bellow Poverty .pdf
Minority .pdf
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FEMA.pdf
Floodplain Keys.pdf
Permit Determination Request.pdf
Coordination with USCG.msg
Waterway Permit Complete email.pdf
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