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[bookmark: _GoBack]The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
This project proposes to resurface United States Route 20 from the west corporation limit of Alvordton in Williams County to State Route 108 north in Fulton County. Bridge work includes replacing wearing surfaces, waterproofing, and retrofitting railings on all bridges within the construction limits. Deck edges will also be replaced on the bridge over Bean Creek and approach slabs and an abutment conversion will be done on the bridge over Iron Creek. No work will occur below OHWM. 
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	


	Cultural Resources Coordination Date:
	


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT  will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
6. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  
7. The following plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source: 

This project is located in or near the source of 3 public drinking water supplies. Do not perform equipment fueling within the locations identified in the table below. If refueling of immobile equipment is necessary within these limits, provide secondary containment with enough capacity to completely contain and collect all potential liquid wastes in the event of a spill.  Do not perform maintenance activities associated with any viscous material that has potential to contaminate the groundwater.  All equipment or liquid containers shall be regularly checked for leaks prior to entering the restricted areas.  The contractor shall develop a Spill Prevention Control and Countermeasure Plan (SPCC) which shall also include all areas of fuel storage, equipment maintenance, and spill kits.  All areas utilized by the Contractor not included within the table below and not in the project limits shall be assessed for potential groundwater contamination and be indicated on the Spill Prevention Control and Countermeasures Plan. The Contractor shall immediately take steps to mitigate any event, such as a spill of fuels, oils, or chemicals. Any such spill or event shall be reported immediately to the emergency contact listed below for each drinking water source.  If the spill is a reportable amount, the Contractor should contact Williams County Emergency Management (419-633-5001) or the Fulton County Emergency Management (419-337-9207) and Ohio EPA Environmental Response and Revitalization (419-373-3031 or 800-282-9378) for cleanup of the spill.

Drinking Water Source 	         Restricted Refueling and Maintenance Area 	                           Emergency Contact Information
D & L Town and Country
(Williams County) 	                         SLM 20.19 to 21.27	                                                             419-924-2932

Archbold Village PWS
(Fulton County)	                                  SLM 6.84 to 7.35
                                                          SLM 7.64 to 8.33                                                                   419-445-2506

US 20 Main Stop Valero
(Fulton County)	                                  SLM 10.62 to 10.84	                                                             419-337-9207
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8. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut, approval must be given by the District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized.  
[bookmark: _Toc256000002]Environmental Commitments
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Commitments
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT  will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
6. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  
7. The following plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source: 

This project is located in or near the source of 3 public drinking water supplies. Do not perform equipment fueling within the locations identified in the table below. If refueling of immobile equipment is necessary within these limits, provide secondary containment with enough capacity to completely contain and collect all potential liquid wastes in the event of a spill.  Do not perform maintenance activities associated with any viscous material that has potential to contaminate the groundwater.  All equipment or liquid containers shall be regularly checked for leaks prior to entering the restricted areas.  The contractor shall develop a Spill Prevention Control and Countermeasure Plan (SPCC) which shall also include all areas of fuel storage, equipment maintenance, and spill kits.  All areas utilized by the Contractor not included within the table below and not in the project limits shall be assessed for potential groundwater contamination and be indicated on the Spill Prevention Control and Countermeasures Plan. The Contractor shall immediately take steps to mitigate any event, such as a spill of fuels, oils, or chemicals. Any such spill or event shall be reported immediately to the emergency contact listed below for each drinking water source.  If the spill is a reportable amount, the Contractor should contact Williams County Emergency Management (419-633-5001) or the Fulton County Emergency Management (419-337-9207) and Ohio EPA Environmental Response and Revitalization (419-373-3031 or 800-282-9378) for cleanup of the spill.

Drinking Water Source 	         Restricted Refueling and Maintenance Area 	                           Emergency Contact Information
D & L Town and Country
(Williams County) 	                         SLM 20.19 to 21.27	                                                             419-924-2932

Archbold Village PWS
(Fulton County)	                                  SLM 6.84 to 7.35
                                                          SLM 7.64 to 8.33                                                                   419-445-2506

US 20 Main Stop Valero
(Fulton County)	                                  SLM 10.62 to 10.84	                                                             419-337-9207
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8. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut, approval must be given by the District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized.  
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:
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Aerial Map.gif
County Map.pdf
USGS Quadrangle Topographical Map.pdf
Stage 1 Design.pdf
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ESA Screening Map.pdf
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Buckeye Assets Mapping.PNG
OHPO Culutural Map.pdf
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OBD Ecological Map.pdf
Wetland Map.pdf
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SWAP map.pdf
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Notification Mailing List.xlsx
Property Owner Notification Map.pdf
Property Owner Notification Letter.docx
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