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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: The D02 Pile Encas/Slopes FY18 (PID101872) project proposes maintenance activities at 20 bridge locations inFulton, Henry, Seneca, Williams, and Wood Counties in ODOT District 2.  Detailed location maps are included in the project file.  At eachbridge site, ODOT proposes to repair the bridge pier piles by encasing the baseof the piles in concrete to fortify the supports and prevent corrosion of the metal pier pile.  Some excavation of sediments around each pier pile will be necessaryand limited slope stabilization may be required. In-stream excavation will not exceed3 feet in depth at any site. All construction activities will be limited to thefootprint of the bridge and 20 linear feet upstream and downstream of thestructure. 
The project sites are located in rural, primarily agricultural, areas in northwest Ohio. The majority of the study areas were dominated bydeveloped open space vegetative communities that are typical of disturbed andmaintained road right-of-way. Portions of some bridge study areas includedforested riparian corridors. Several bridges cross large streams and are located in mapped FEMA Special Flood Hazard Areas. Floodplain coordination can be found in the project file. Two of the work locations are within surface water drinking water corridor management areas which require a plan note for the protection of those drinking water resources. 
An ecological survey was performed ateach bridge site to determine potential impacts to aquatic resources.Twenty-one (21) streams and eight (8) wetlands were identified within the studyareas associated with the project. Permanent impacts to twenty-one (21) streamsand five (5) wetlands are required to complete the bridge maintenance.Temporary impacts to twenty-one (21) streams and six (6) wetlands are requiredfor construction access.  Please see the project file for the Wetland Determination. 
Based on coordination with the Ohio Department of Natural Resources (ODNR), Phase 1 mussel surveys and relocations will be conducted (prior to any in-waterwork) at the following sites:
· FUL-20A-0253
· HEN-109-0438
· HEN-109-0878
· HEN-109-1355
· WIL-15-0011
· WIL-15-0292
· WIL-20-1488
· WIL-20A-0866
· WIL-49-2002
· WIL-576-2011
· WOO-281-1418 
	STIP Reference #
	SLI 32


	Select the appropriate project type:
	(28) Bridge rehabilitation, reconstruction, or replacement or the construction of grade separation to replace existing at-grade railroad crossings, if the actions meet the constraints in 23 CFR 771.117(e). Examples include: Railroad projects that close or relocate at-grade crossings


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Regional General Permit


	Waterways Permit Approval Date
	12/14/2016


	Isolated Wetland Permit
	No


	Endangered Species:
	Present; No finding of May Affect, Likely to Adversely Affect


	Endangered Species - Coordination
	May Affect, Not Likely to Adversely Affect


	Endangered Species - Coordination Date
	11/03/2016


	Endangered Species - Critical Habitat Present/Impacted
	Indiana bat

	
	Northern long-eared bat


	Endangered Species - Other Critical Habitat Present/Impacted:
	No


	100-Year Floodplain:
	Encroachment Within the SFHA is a Functionally Dependent Use


	EO 11988/NFIP Coordination and Documentation Completed:
	Yes


	NFIP Local Floodplain Coordinator Notification Date:
	01/31/2017


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	Minimum Potential to Cause Effect - Appendix B


	Cultural Resources Coordination - ODOT Approval Date:
	09/02/2016


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Studies Not Required


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work of any major, disruptive, time-delaying traffic control changes or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior to the work.
2. The project requires a waterway permit for stream and wetland impacts which shall be attached to the plans as Special Provisions. No work below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by ODOT. All conditions of the permit shall be followed throughout construction by the contractor.
3. No impacts shall occur to Wetland D located within the study area of SEN-101-0810.
4. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat. If it is necessary to remove trees for site access, all tree removal must occur from October 1 through March 31. This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act. For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet.
5. Due to work in a Zone A floodplain, the letter of compliance (LD-51 Form) and calculations showing that the carrying capacity of the streams will not change due to the work. All floodplain regulations shall be followed throughout design and construction.
6. ODOT shall ensure that a mussel survey shall be performed at the following locations prior to any work below the Ordinary High Water Mark (OHWM) of the stream: 
FUL-20A-2.53
HEN-109-4.38
HEN-109-8.78
HEN-109-13.55 
WIL-15-0.11
WIL-15-2.92
WIL-20-14.88
WIL-20A-8.66
WIL-49-20.02
WIL-576-20.11
WIL-281-14.18

7. The contractor shall perform all work within the existing right of way. 
8. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
9. ODOT and the contractor shall ensure that traffic is maintained at all times. 
10. A note will be added to the construction plans in order to address the project's location in relation to the drinking water source. 
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1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work of any major, disruptive, time-delaying traffic control changes or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior to the work.
2. The project requires a waterway permit for stream and wetland impacts which shall be attached to the plans as Special Provisions. No work below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by ODOT. All conditions of the permit shall be followed throughout construction by the contractor.
3. No impacts shall occur to Wetland D located within the study area of SEN-101-0810.
4. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat. If it is necessary to remove trees for site access, all tree removal must occur from October 1 through March 31. This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act. For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet.
5. Due to work in a Zone A floodplain, the letter of compliance (LD-51 Form) and calculations showing that the carrying capacity of the streams will not change due to the work. All floodplain regulations shall be followed throughout design and construction.
6. ODOT shall ensure that a mussel survey shall be performed at the following locations prior to any work below the Ordinary High Water Mark (OHWM) of the stream: 
FUL-20A-2.53
HEN-109-4.38
HEN-109-8.78
HEN-109-13.55 
WIL-15-0.11
WIL-15-2.92
WIL-20-14.88
WIL-20A-8.66
WIL-49-20.02
WIL-576-20.11
WIL-281-14.18

7. The contractor shall perform all work within the existing right of way. 
8. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
9. ODOT and the contractor shall ensure that traffic is maintained at all times. 
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10. A note will be added to the construction plans in order to address the project's location in relation to the drinking water source. 
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	Form Preparer
	amy Allen

OH 

amy.allen@davey.com



	Supporting Form Preparer(s)
	Eli Barber, Phoenix Golnick, Stacy Schimmoeller, Gregory Snowden, Jeff Pettit
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	February 2, 2017

	Stacy Schimmoeller PROGRAM ADMIN 3
	February 2, 2017


	
	 Environmental Document Level: C2
PID 101872 D02 Pile Encas/Slopes FY18
Approved: February 2, 2017




[bookmark: _Toc256000007]Appendix
[bookmark: _Toc256000008]Uploaded Files by Report Section
[bookmark: _Toc256000009]Environmental Commitments
Drinking Water Protection Plan Note.pdf
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Aerial Map.pdf
Schematic Plan.pdf
Stage 2 Design.pdf
County Map.pdf
USGS Quadrangle Topographical Map.pdf
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Screening Map.pdf
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Section 106 Request for Review.pdf
OES Approval - Minimum Potential to Cause Effects - B.pdf
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Level 1 ESR HEN-65-1618 PID 101872.pdf
Level 1 ESR HEN-65-1671 PID 101872.pdf
Level 1 ESR HEN-109-1355 PID 101872.pdf
Level 1 ESR SEN-18-0569 PID 101872.pdf
Level 1 ESR SEN-67-0046 PID 101872.pdf
Level 1 ESR SEN-4-0239 PID 101872.pdf
Level 1 ESR HEN-6-2784 PID 101872.pdf
Level 1 ESR SEN-101-0810 PID 101872.pdf
Level 1 ESR WIL-20A-0866 PID 101872.pdf
Level 1 ESR HEN-6-0912 PID 101872.pdf
Coordination with USFWS.pdf
Coordination with ODNR.pdf
OES Approval.pdf
Level 1 ESR FUL-20A-0253 PID 101872.pdf
Level 1 ESR WIL-15-0011 PID 101872.pdf
Level 1 ESR WIL-15-0292 PID 101872.pdf
Level 1 ESR WIL-20-1488 PID 101872.pdf
Level 1 ESR WIL-49-2002 PID 101872.pdf
Level 1 ESR WIL-576-2011 PID 101872.pdf
Level 1 ESR HEN-6-2182 PID 101872.pdf
Level 1 ESR HEN-109-0438 PID 101872.pdf
Level 1 ESR HEN-109-0878 PID 101872.pdf
Level 1 ESR WOO-281-1418 PID 101872.pdf
Consult Form HEN-6-0912 PID 101872.pdf
Consult Form HEN-65-1618 PID 101872.pdf
Consult Form HEN-65-1671 PID 101872.pdf
Consult Form HEN-109-1355 PID 101872.pdf
Consult Form SEN-18-0569 PID 101872.pdf
Consult Form SEN-67-0046 PID 101872.pdf
Consult Form SEN-101-0810 PID 101872.pdf
Coordination with USFWS-2.pdf
Coordination with ODNR-2.pdf
ODNR Comments.pdf
Consult Form D2 VAR Combined PID 101872.pdf
ODNR Comments2.pdf
Wetland Determination .pdf
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Water Source Protection Area Map.pdf
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Census Mapping.pdf
C2 EJ Form.pdf
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Survey Letter.pdf
Response to Public Comments.pdf
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FEMA FIRM.pdf
Permit Determination Request.pdf
OES Permit Determination.pdf
Floodplain Impacts.pdf
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