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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
The proposed project will be on the Craig Bridge (SR 65) and the Veterans Glass City Skyway Bridge (I-280) in the City of Toledo, Lucas County, and the Port Clinton Bridge (SR 163) in the City of Port Clinton, Ottawa County, Ohio. 
The electrical maintenance work will be performed inside of the existing bridges, meaning inside of the Craig and Port Clinton bridges, and also inside of the VGCS bridge superstructure/pylon. There will be no work or activity below the deck outside of any of the bridges. 
Maintenance will also be performed on 4 storm water pump stations located at 
LUC-280-0220-Storm water pump station located at Starr Avenue and I-280, Toledo, OH
LUC-280-0564-Storm water pump station located at Manhattan Blvd. and I-280, Toledo, OH
OTT-51-0973- Storm water pump station located at the Woodville Rd. & NorfolkSouthern Railroad overpass, Allen Township, Ottawa County OH 
FUL-120-1265- Storm water pump station located at the Indiana & Ohio RR underpass,Amboy Township, Fulton OH).  
	STIP Reference #
	SLI 12


	Cultural Resources Coordination:
	(2) Minimum Potential Appendix B


	Cultural Resources Coordination Date:
	02/29/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way. 

2. The contractor shall take all precautions to prevent any materials, including but not limited to grease, epoxy, paint, concrete, grindings, asphalt, etc. from entering waterways during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. No equipment or staging shall be permitted in any streams, wetlands, or other waters.
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3. Work on the structures shall not be performed between the bridge deck and the water within the navigation channel. Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.
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Commitments
1. The contractor shall perform all work within the existing right of way. 

2. The contractor shall take all precautions to prevent any materials, including but not limited to grease, epoxy, paint, concrete, grindings, asphalt, etc. from entering waterways during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. No equipment or staging shall be permitted in any streams, wetlands, or other waters.
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3. Work on the structures shall not be performed between the bridge deck and the water within the navigation channel. Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	June 17, 2016
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