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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
This project proposes to repair and replace guardrail damaged during the term of the contract throughout all 8 counties in District 2 (Fulton, Henry, Lucas, Ottawa, Sandusky, Seneca, Williams, and Wood). 
	STIP Reference #
	SLI 12


	Cultural Resources Coordination:
	


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes
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1. Access to adjacent properties will be maintained during construction by the contractor.
2. The contractor shall perform all work within the existing right of way. 
3. The contractor shall notify ODOT as soon as it is known that the work will require lane restrictions, lane closures, and/or road closures. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices as soon as possible prior the work.
4. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage
5. If required by local ordinance, a construction noise plan note will be developed and implemented.
6. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project unless the tree poses a potential safety hazard for the traveling public.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut, approval must be given by the District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized. 
7. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
8. If cutting and/or clearing of any vegetation, earthwork, ditch maintenance, herbicidal spraying, painting, welding, sand and/or water blasting, dewatering, RCP, or use of toxic or hazardous materials such as but not limited to sealants, paint, solvents, cleaning agents, earthen materials, waste water, fuels, debris, etc. is needed within 1000 feet of the Scenic Maumee River and/or Sandusky River, then coordination is required with ODNR Scenic Rivers prior to any work within 1000 feet of a scenic river. The contractor shall notify the project engineer as soon as it is known that work must occur within 1000 feet of the Scenic Maumee River and/or Sandusky Rivers. The project engineer shall notify the District Environmental Coordinator as soon as it is known that work must occur within 1000 feet of the scenic river so that the ODNR Scenic River Coordinator can be notified. 
9. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  
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10. Due to the location of the project within the globally rare Oak Openings region, earth disturbance shall be a minimal as possible.  Work done off the existing pavement shall be as minimal as possible.  Care shall be taken to not disturb the existing vegetation. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
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