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[bookmark: _GoBack]The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
This is a District 2 contract to address lighting maintenance district-wide and includes various locations throughout District 2. No environmental impacts are associated with this contract and no right of way is needed.  
	STIP Reference #
	SLI 12


	Cultural Resources Coordination:
	


	Cultural Resources Coordination Date:
	


	Supporting documentation has been uploaded to Project File:
	No


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. Light pole replacement located in historic districts require in-kind replacements. Any diversion from the original design must be approved by the District Environmental Coordinator (DEC) prior to disposal of the existing. 
2. Construction of this project will be conducted such that it does not interfere with waterway traffic between April 1 and November 30 of any calendar year for Section 9 Waterways (Maumee River south up to I-75, Lake Erie, West Harbor, Sandusky Bay, Toledo Harbor, Toussaint River, Port Clinton Harbor, and Put-In Bay).  During this period the channel will be open to navigation per the schedule posted at the bridge. For all in-water construction work, including work that falls within the December 1 to March 31 construction window, the contractor must contact the United States Coast Guard Ninth District as noted below: The Ninth Coast Guard will need to be contacted at least 45 days prior to the start of work to coordinate the in-water work. Contact info: Scot Striffler, Bridge Project Manager, Ninth Coast Guard District PH: (216) 902-6087 FAX: (216) 902-6088 Scot.M.Striffler@USGC.MIL

3. Coordination with ODNR Scenic Rivers shall occur prior to any work within 1000 feet of a Scenic River. The contractor shall notify the Project Engineer 25 days prior to work within 1000 feet of the Scenic River so that the ODNR Scenic River Coordinator can be notified. 
4. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet.  
5. The contractor shall take all precautions to prevent any and all materials from going off the edges of the bridge deck or edge of a culvert during all operations. The contractor shall immediately remove any materials that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the Ordinary High Water Mark (OHWM) of any stream.
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6. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  
[bookmark: _Toc256000002]Environmental Commitments
[bookmark: _Toc256000003]C1
Commitments
1. Light pole replacement located in historic districts require in-kind replacements. Any diversion from the original design must be approved by the District Environmental Coordinator (DEC) prior to disposal of the existing. 
2. Construction of this project will be conducted such that it does not interfere with waterway traffic between April 1 and November 30 of any calendar year for Section 9 Waterways (Maumee River south up to I-75, Lake Erie, West Harbor, Sandusky Bay, Toledo Harbor, Toussaint River, Port Clinton Harbor, and Put-In Bay).  During this period the channel will be open to navigation per the schedule posted at the bridge. For all in-water construction work, including work that falls within the December 1 to March 31 construction window, the contractor must contact the United States Coast Guard Ninth District as noted below: The Ninth Coast Guard will need to be contacted at least 45 days prior to the start of work to coordinate the in-water work. Contact info: Scot Striffler, Bridge Project Manager, Ninth Coast Guard District PH: (216) 902-6087 FAX: (216) 902-6088 Scot.M.Striffler@USGC.MIL

3. Coordination with ODNR Scenic Rivers shall occur prior to any work within 1000 feet of a Scenic River. The contractor shall notify the Project Engineer 25 days prior to work within 1000 feet of the Scenic River so that the ODNR Scenic River Coordinator can be notified. 
4. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet.  
5. The contractor shall take all precautions to prevent any and all materials from going off the edges of the bridge deck or edge of a culvert during all operations. The contractor shall immediately remove any materials that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the Ordinary High Water Mark (OHWM) of any stream.
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6. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	April 1, 2016
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