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 317 E. POE RD. • BOWLING GREEN, OH 43402 • 614-995-7902 



The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION

	ODOT District
	2

	Funding Source
	State, Other

	Private Funding:
	No

	
	


Project Description: 
This is a proposed project to do deck sealing using gravity fed resin (GFR) on various bridges in Sandusky County listed below to: 
1. SAN-6- 14.70 over US 20
2. SAN-6-15.13 over a RR
3. SAN-6-15.38 over Muskellunge Creek
4. SAN-6-17.51 over the Sandusky River
5. SAN-20-3.18 over the Portage River
6. SAN-20-4.99 over Sugar Creek
7. SAN-20-10.35 over Muddy Creek
8. SAN-20-19.2 over unnamed tributary
9. SAN-20-21.69 over Green Creek
This work is proposed as a preventative measure to help extend the life of the bridge.  The GFR will seal the cracks in the concrete deck to prevent water in the cracks from freezing and thawing, which breaks up the concrete, deteriorating the deck.  
All work for the project shall be within the existing right of way.  No work shall occur below low steel.  
A letter was sent to emergency services for their input on the maintenance of traffic as shown in the project file. 
	STIP Reference #
	SLI 32

	Cultural Resources Coordination:
	(3) No Historic Properties Affected

	Cultural Resources Coordination Date:
	06/30/2016

	Supporting documentation has been uploaded to Project File:
	Yes

	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.

	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. Access to multi-use paths shall be maintained at all times during construction by ODOT and the contractor. 
2. The contractor shall perform all work within the existing right of way. 
3. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. Work on the structures over Section 10 waters (SAN-6-17.51 over the Sandusky River and SAN-20-3.19 over the Portage River) shall not be performed between the bridge deck and the water within the navigation channel.  Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.         
6. ODOT and the contractor shall ensure that full bridge closure shall not occur for vehicular and/or pedestrian traffic. 
7. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
8. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source
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9. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
[bookmark: _Toc256000002]Environmental Commitments
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Commitments
1. Access to multi-use paths shall be maintained at all times during construction by ODOT and the contractor. 
2. The contractor shall perform all work within the existing right of way. 
3. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. Work on the structures over Section 10 waters (SAN-6-17.51 over the Sandusky River and SAN-20-3.19 over the Portage River) shall not be performed between the bridge deck and the water within the navigation channel.  Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.         
6. ODOT and the contractor shall ensure that full bridge closure shall not occur for vehicular and/or pedestrian traffic. 
7. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
8. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source
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9. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
[bookmark: _Toc256000004]Preparers  & Approvals
[bookmark: _Toc256000005]Form Preparer(s)
	Form Preparer
	District 2

	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:

	Stacy Schimmoeller PROGRAM ADMIN 3
	July 1, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	July 1, 2016
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Stage 3 Design.pdf
[bookmark: _Toc256000010]Cultural Resources
Minimum Potential to Cause Effects - A.pdf
[bookmark: _Toc256000011]Ecological
Ecological Review Form - Documentation for an Ecologically Exempt Project .pdf
Eco Map.jpg
[bookmark: _Toc256000012]Other Resources
Water Source Protection Area Map.pdf
Community Water System Coordination.pdf
Community Water Coordination letter .pdf
[bookmark: _Toc256000013]Public Involvement
Emergency Services Notification.pdf
Notification Mailing List.xlsx
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Permit Determination Request.pdf
USCG Section 9 Letter Request.pdf
OES Permit Determination.pdf
Coordination with USCG.pdf
Floodplain Impacts.pdf
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