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[bookmark: _GoBack]The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
This project proposes to repair 3 bridges in Ottawa County including OTT-2-27.25 over NS Rail Road, OTT-2-25.33 over Lake Road/Gypsum Road, and OTT-2-27.57 over Sandusky Bay. The proposed work is to replace latex wearing surface with new micro-silica, remove and replace backwall and expansion joints, replace abutment bearings, replace end cross-frames, repair paint system. 
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	


	Cultural Resources Coordination Date:
	


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.
6. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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7. Coordination with the United States Coast Guard (USCG) shall be initiated at least 30 days prior to starting work above Sandusky Bay (OTT-2-27.57, SFN 6200753), a Section 9 water.  Contact info: Scot Striffler, Bridge Project Manager, Ninth Coast Guard District PH: (216) 902-6087 FAX: (216) 902-6088 Scot.M.Striffler@USCG.MIL
[bookmark: _Toc256000002]Environmental Commitments
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Commitments
1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.
6. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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7. Coordination with the United States Coast Guard (USCG) shall be initiated at least 30 days prior to starting work above Sandusky Bay (OTT-2-27.57, SFN 6200753), a Section 9 water.  Contact info: Scot Striffler, Bridge Project Manager, Ninth Coast Guard District PH: (216) 902-6087 FAX: (216) 902-6088 Scot.M.Striffler@USCG.MIL
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[bookmark: _Toc256000005]Form Preparer(s)
	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	March 21, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	March 21, 2016


	
	Categorical Exclusion Document CE Level: C1
PID 80735 OTT SR 2 25.33/27.25/27.57 brdg
Approved: March 21, 2016




[bookmark: _Toc256000007]Appendix
[bookmark: _Toc256000008]Uploaded Files by Report Section
[bookmark: _Toc256000009]General
Aerial Map.pdf
USGS Quadrangle Topographical Map.pdf
County Map.pdf
[bookmark: _Toc256000010]ESA
ESA Screening Map.gif
[bookmark: _Toc256000011]Cultural Resources
Buckeye Assets Mapping.PNG
Records Check.pdf
[bookmark: _Toc256000012]Ecological
OBD Ecological Map.pdf
[bookmark: _Toc256000013]Other Resources
Water Source Protection Area Map.pdf
[bookmark: _Toc256000014]Environmental Justice
Poverty OTT.gif
Minority OTT.gif
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FEMA Floodplain Map.pdf
Public Water Supply Map.pdf
Permit Determination request .pdf
USCG Comments.pdf
FEMA Floodplain Letter.pdf
Coordination with USCG.pdf
OES Permit Determination.pdf
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