	
	Categorical Exclusion Document CE Level: C2
PID 85271 WOO US 6 0.00 Resurf
Approved: February 12, 2016



 



Categorical Exclusion Document
for
 WOO US 6 0.00 Resurf PID 85271

CE Level: C2




Approved: February 12, 2016

Prepared by: District 2




	[image: odotsl_gr]
	Ohio Department of Transportation
[bookmark: _GoBack] 317 E. POE RD. • BOWLING GREEN, OH 43402 • 614-995-7902 








		Page 16 of 16
Contents
C2	3
Environmental Commitments, 	8
Environmental Commitments	11
C2	11
Preparers  & Approvals	13
Form Preparer(s)	13
Approvals & Electronic Signatures	13
Appendix	14
Uploaded Files by Report Section	14
Environmental Commitments	14
General	14
ESA	14
Cultural Resources	14
Ecological	14
Other Resources	15
Environmental Justice	15
Permits	15

	
	Categorical Exclusion Document CE Level: C2
PID 85271 WOO US 6 0.00 Resurf
Approved: February 12, 2016




[bookmark: _Toc256000000]C2	PID
	85271


	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
This project is located within Grand Rapids Township and Weston Township, Wood County, Ohio.  The proposed work includes the resurfacing of United State Route 6 from the Henry and Wood County Line to State Route 235. Two existing culverts at Straight Line Mileage (SLM) 2.93 and 3.04 respectively will be replaced and three crossover pipes at SLM 3.09, 3.86, and 4.43 respectively will be replaced. The addition of rock channel protection and the removal of existing catch basins will be included in the culvert replacements. The project also includes the replacement of deck edges, bridges railing, and approach slabs over the existing bridge over Beaver Creek. Additional right-of-way will be needed for the culverts at SLMs 2.93 and 3.04.
	STIP Reference #
	SLI 32


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(28) Bridge rehabilitation, reconstruction, or replacement or the construction of grade separation to replace existing at-grade railroad crossings, if the actions meet the constraints in 23 CFR 771.117(e). Examples include: Railroad projects that close or relocate at-grade crossings


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Regional General Permit


	Endangered Species:
	Present; No finding of May Affect, Likely to Adversely Affect


	Endangered Species - Coordination
	No Effect


	100-Year Floodplain:
	No Encroachment Within a Special Flood Hazard Area (SFHA)


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	Minimum Potential to Cause Effect - Appendix B


	Cultural Resources Coordination - ODOT Approval Date:
	07/24/2015


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Yes


	Hazardous Materials - OES Approval Date:
	10/08/2015


	Phase I ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Phase II ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. Access to adjacent properties will be maintained during construction by the contractor
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  
6. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor or store equipment and/or materials in any wetlands, streams, or other waters.  No work is permitted below the top of bank of any stream, except the culvert work at WOO-6-2.93, 3.01, and 3.86.
7. The following plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source: This project is located in or near the source of 1 public drinking water supply. Do not perform equipment fueling within the locations identified in the table below.  If refueling of immobile equipment is necessary within these limits, provide secondary containment with enough capacity to completely contain and collect all potential liquid wastes in the event of a spill.  Do not perform maintenance activities associated with any viscous material that has potential to contaminate the groundwater.  All equipment or liquid containers shall be regularly checked for leaks prior to entering the restricted areas.  The contractor shall develop a Spill Prevention Control and Countermeasure Plan (SPCC) which shall also include all areas of fuel storage, equipment maintenance, and spill kits.  All areas utilized by the Contractor not included within the table below and not in the project limits shall be assessed for potential groundwater contamination and be indicated on the Spill Prevention Control and Countermeasures Plan.  The Contractor shall immediately take steps to mitigate any event, such as a spill of fuels, oils, or chemicals. Any such spill or event shall be reported immediately to the emergency contact listed below for each drinking water source.  If the spill is a reportable amount, the Contractor should contact Wood County Emergency Management (419-354-9269) and Ohio EPA Environmental Response and Revitalization (419-373-3031 or 800-282-9378) for cleanup of the spill. 
Drinking Water Source 	Restricted Refueling and Maintenance Area 	Emergency Contact Information
City of Bowling Green PWS	SLM 4.00 to 5.00 (Weston Rd to Van Tassel Rd)	(419) 878-6986

8. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut, approval must be given by the District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized.  
9. The project requires a waterway permit for the culvert work at WOO-6-2.93, 3.01, and 3.86 which is attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
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Commitments
1. Access to adjacent properties will be maintained during construction by the contractor
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  
6. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor or store equipment and/or materials in any wetlands, streams, or other waters.  No work is permitted below the top of bank of any stream, except the culvert work at WOO-6-2.93, 3.01, and 3.86.
7. The following plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source: This project is located in or near the source of 1 public drinking water supply. Do not perform equipment fueling within the locations identified in the table below.  If refueling of immobile equipment is necessary within these limits, provide secondary containment with enough capacity to completely contain and collect all potential liquid wastes in the event of a spill.  Do not perform maintenance activities associated with any viscous material that has potential to contaminate the groundwater.  All equipment or liquid containers shall be regularly checked for leaks prior to entering the restricted areas.  The contractor shall develop a Spill Prevention Control and Countermeasure Plan (SPCC) which shall also include all areas of fuel storage, equipment maintenance, and spill kits.  All areas utilized by the Contractor not included within the table below and not in the project limits shall be assessed for potential groundwater contamination and be indicated on the Spill Prevention Control and Countermeasures Plan.  The Contractor shall immediately take steps to mitigate any event, such as a spill of fuels, oils, or chemicals. Any such spill or event shall be reported immediately to the emergency contact listed below for each drinking water source.  If the spill is a reportable amount, the Contractor should contact Wood County Emergency Management (419-354-9269) and Ohio EPA Environmental Response and Revitalization (419-373-3031 or 800-282-9378) for cleanup of the spill. 
Drinking Water Source 	Restricted Refueling and Maintenance Area 	Emergency Contact Information
City of Bowling Green PWS	SLM 4.00 to 5.00 (Weston Rd to Van Tassel Rd)	(419) 878-6986

8. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut, approval must be given by the District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized.  
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9. The project requires a waterway permit for the culvert work at WOO-6-2.93, 3.01, and 3.86 which is attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	February 12, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	February 12, 2016
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Drinking Water Protection Plan Note.pdf
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Aerial Map.GIF
County Map.pdf
USGS Quadrangle Topographical Map.pdf
NEPA Assignment Language for CEs .docx
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ESA Screening Map.GIF
Oil and Gas Map.PNG
OES Coordination IOC.pdf
ESA Screening .pdf
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OHPO Cultural Map.pdf
Section 106 Request for Review.pdf
Coordination with SHPO.pdf
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OBD Ecological Map.pdf
Wetland Map.GIF
ODNR Comments.pdf
Level 1 MOA Coordination .pdf
Response To ODNR Comments.pdf
Coordination with USFWS.pdf
Response to USFWS Comments.pdf
Level 1 Ecological Survey.pdf
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Residential Well Map.jpg
Public Water Supply Map.docx
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Minority WOO.GIF
Poverty WOO.GIF
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FEMA Floodplain Map.pdf
Permit Determination Request .pdf
Regional General Permit B.pdf
Special Provisions.pdf
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