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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.


		Page 12 of 12
Contents
C1	3
Environmental Commitments, 	6
Environmental Commitments	8
C1	8
Preparers  & Approvals	10
Form Preparer(s)	10
Approvals & Electronic Signatures	10
Appendix	11
Uploaded Files by Report Section	11
General	11
ESA	11
Cultural Resources	11
Ecological	11
Other Resources	11
Environmental Justice	11
Permits	11

	
	 Environmental Document Level: C1
PID 95717 LUC 20/2/120 10.35/9.10/10.86
Approved: January 23, 2017




[bookmark: _Toc256000000]C1	PID
	95717


	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This project proposes to resurface US Route 20 (US-20/Central Avenue) from Van Fleet Parkway to State Route 120 (SR-120/Reynolds Road); State Route 2 (SR-2/Airport Highway) from Holloway Road to Holland-Sylvania Road; State Route 120 (SR-120/Central Avenue) from Hasty to Corey Road due to poor pavement conditions. This project also includes signal replacements at Lincolnshire Boulevard and Central Avenue and bridge deck sealing and concrete patching at LUC-2-9.46 Over Wolf Creek and LUC-2-10.26 over Interstate 475. There will be no new right of way required and no work below the Ordinary High Water Mark (OHWM) of any stream. This project passes through a floodplain but it will have no impact, as shown in the documentation in the project file. A minimum of one vehicular lane in each direction will be maintained throughout construction.  Pedestrian access shall be maintained at all times. The ESA Screening was approved at the district level because all deep excavation will occur within existing right of way and is surrounded by historically residential areas. A portion of this project is located within the Oak Opening Region. There will be no work off of existing pavement for the portions located within Oak Openings. 
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required. 
4. Due to the known presence of Ohio threatened Blanding's Turtle within the project area (on US 20/120), if any turtle is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.


6. Due to the location of the project within the globally rare Oak Openings region, there shall be no earth disturbance between Van Fleet Pkwy (LUC-20-10.32) and the Ottawa River (LUC-120-11.28).  No work shall be done off the existing pavement and care shall be taken to not disturb the existing vegetation within these limits. 
7. Pedestrian access shall be maintained at all times.  
8. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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9. The project is located within an area (SR-2) where the federally threatened Eastern Massasauga snake has been found.  If any snake is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.
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5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	January 23, 2017

	Stacy Schimmoeller PROGRAM ADMIN 3
	January 23, 2017
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