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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
TheOhio Department of Transportation is currently proposing to resurface StateRoute 18 from State Route 19 to County Road 32 in Seneca County due to poor pavement conditions. Additionalwork includes replacing the deck edges and patching the abutments of thestructure that carries State Route 18 over Westerhouse Ditch. All work is within existing right of way and there will be no impacts to utilities. The bridge work will not require any US Army Corps of Engineers permit since the work is above the ordinary high water mark of Westerhouse ditch. This project does pass through a floodplain, however the district hydraulic engineer has determined that there will be no impacts. Plan notes will be added to the construction plans to ensure the protection of several drinking water sources within the project area. The bridge workwill require a 45 day road closure and all impacted property owners, local public safety agencies, and schools have been notified of the closure. Constructionis expected to begin in the summer of 2018 and last approximately 120 days.During construction, one lane of traffic will be maintained at all times withthe exception of the closure noted above. 
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	Minimal Potential to Cause Effect - Appendix A


	Cultural Resources Coordination Date:
	06/17/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101 that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,179,656.40 of Federal funds or with a total estimated cost of not more than $31,077,938.40 and with Federal funds that comprise less than 15 percent of the total estimated project cost (each amount adjusted annually by the Secretary to reflect any increases in the Consumer Price Index prepared by the Department of Labor, see www.fhwa.dot.gov or www.fta.dot.gov).


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way
2. Parts 642-8 and 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. No work (temporary or permanent) shall be performed below the Ordinary High Water Mark (OHWM 823.08) of Westerhouse Ditch.  Any work below the OHWM is a violation of the Federal Clean Water Act of 1972.   
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6. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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1. The contractor shall perform all work within the existing right of way
2. Parts 642-8 and 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. No work (temporary or permanent) shall be performed below the Ordinary High Water Mark (OHWM 823.08) of Westerhouse Ditch.  Any work below the OHWM is a violation of the Federal Clean Water Act of 1972.   
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6. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Eli Barber
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	August 18, 2017

	Phoenix Golnick Neal ENV SPEC 2
	August 18, 2017
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Drinking Water Protection Plan Note.pdf
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Aerial Map.pdf
County Map.pdf
USGS Quadrangle Topographical Map.pdf
Stage 2 Design.pdf
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ESA screening map.pdf
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OHPO map.pdf
Buckeye Assets Mapping.pdf
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Eco map.pdf
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Water Source Protection Area Map.pdf
Community Water System Coordination.pdf
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EMA and School Notification.pdf
Property Owner Notification Letter.pdf
Public Notification Mailing List.pdf
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FEMA FIRM.pdf
Floodplain Impacts.pdf
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