	
	 Environmental Document Level: C1
PID 104665 WOO/OTT 75/269 29.93/1.67 Br hit
Approved: March 13, 2017



 



[bookmark: _GoBack]Environmental Document
for
 WOO/OTT 75/269 29.93/1.67 Br hit PID 104665

Environmental Document Level: C1




Approved: March 13, 2017

Prepared by: District 2




	[image: odotsl_gr]
	Ohio Department of Transportation
 317 E. POE RD. • BOWLING GREEN, OH 43402 • 614-995-7902 





The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Non-Federal


	Private Funding:
	No


	
	


Project Description: 
This project proposes to repair two bridges (Lime City Road over Interstate 75 (I-75) in Wood County and State Route 269 (SR-269) over Bayshore Road in Ottawa County) that were damaged from being hit by oncoming traffic. These repairs will have no impact any waters of the US or floodplains so no permits are required. Construction is expected to begin in the summer of 2017. During construction, there will be no lane restrictions on SR-269 and there will be no lane restrictions on I-75 during peak hours. Flaggers will be used to maintain traffic on Lime City Road and Bayshore Road. 
	STIP Reference #
	SLI 7


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(1) Activities which do not involve or lead directly to construction, such as planning and technical studies; grants for training; engineering to define the elements of a proposed action or alternatives so that social, economic, and environmental effects can be assessed; and Federal-aid system revisions which establish classes of highways on the Federal-aid highway system. Examples include: Study type projects (i.e. feasibility studies, etc.); Projects that utilize no federal monies or require no federal actions (State-funded actions only); Land donations to ODOT associated with ROW permits (non-NHS/non-Limited Access right-of-way). (Environmental Site Assessment issues will require coordination with ODOT-OES) (State-funded actions only).


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. Vehicular and pedestrian traffic shall be maintained at all times. 
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6. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. Vehicular and pedestrian traffic shall be maintained at all times. 
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6. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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	Form Preparer
	District 2


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick ENV SPEC 2
	March 13, 2017

	Phoenix Golnick ENV SPEC 2
	March 13, 2017
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