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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Non-Federal


	Private Funding:
	No


	
	


Project Description: 
This project is a district wide lighting maintenance project. Actual work locations are not known as the repairs are requested by work order after damage has occurred. No right of way is needed and there are no expected impacts to utilities.  
	STIP Reference #
	SLI 12


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	01/20/2017


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(1) Activities which do not involve or lead directly to construction, such as planning and technical studies; grants for training; engineering to define the elements of a proposed action or alternatives so that social, economic, and environmental effects can be assessed; and Federal-aid system revisions which establish classes of highways on the Federal-aid highway system. Examples include: Study type projects (i.e. feasibility studies, etc.); Projects that utilize no federal monies or require no federal actions (State-funded actions only); Land donations to ODOT associated with ROW permits (non-NHS/non-Limited Access right-of-way). (Environmental Site Assessment issues will require coordination with ODOT-OES) (State-funded actions only).


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
4. The intent of the project is to not remove any trees.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should a tree be a safety hazard for the traveling public, the tree should be cut as soon as possible.
5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
6. Light pole replacement located in historic districts require in-kind replacements. Any diversion from the original design must be approved by the District Environmental Coordinator (DEC) prior to disposal of the existing.



7. Coordination with ODNR Scenic Rivers shall occur prior to any work within 1000 feet of a Scenic River (Maumee River and Sandusky River). The contractor shall notify the Project Engineer 25 days prior to work within 1000 feet of the Scenic River so that the ODNR Scenic River Coordinator can be notified. 
8. Construction of this project will be conducted such that it does not interfere with waterway traffic between April 1 and November 30 of any calendar year for Section 9 Waterways (Maumee River south up to I-75, Lake Erie, West Harbor, Sandusky Bay, Toledo Harbor, Toussaint River, Port Clinton Harbor, and Put-In Bay).  During this period the channel will be open to navigation per the schedule posted at the bridge. For all in-water construction work, including work that falls within the December 1 to March 31 construction window, the contractor must contact the United States Coast Guard Ninth District as noted below:
The Ninth Coast Guard will need to be contacted at least 45 days prior to the start of work to coordinate the in-water work. Contact info: Scot Striffler, Bridge Project Manager, Ninth Coast Guard District PH: (216) 902-6087 FAX: (216) 902-6088 Scot.M.Striffler@USGS.MIL
9. If any animals, snake, turtle, bird, salamander, etc. is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue. 
10. Any work within the globally rare Oak Openings region shall be limited to the very minimum of earth disturbance necessary to perform the work.  The very minimum amount work shall be done off the existing pavement.  Care shall be taken to not disturb the existing vegetation. 
11. Access to all multi-use paths shall be maintained at all times during construction by ODOT and the contractor.
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12. Pedestrian access shall be maintained at all times by ODOT and the contractor.  
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Commitments
1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
4. The intent of the project is to not remove any trees.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should a tree be a safety hazard for the traveling public, the tree should be cut as soon as possible.
5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
6. Light pole replacement located in historic districts require in-kind replacements. Any diversion from the original design must be approved by the District Environmental Coordinator (DEC) prior to disposal of the existing.



7. Coordination with ODNR Scenic Rivers shall occur prior to any work within 1000 feet of a Scenic River (Maumee River and Sandusky River). The contractor shall notify the Project Engineer 25 days prior to work within 1000 feet of the Scenic River so that the ODNR Scenic River Coordinator can be notified. 
8. Construction of this project will be conducted such that it does not interfere with waterway traffic between April 1 and November 30 of any calendar year for Section 9 Waterways (Maumee River south up to I-75, Lake Erie, West Harbor, Sandusky Bay, Toledo Harbor, Toussaint River, Port Clinton Harbor, and Put-In Bay).  During this period the channel will be open to navigation per the schedule posted at the bridge. For all in-water construction work, including work that falls within the December 1 to March 31 construction window, the contractor must contact the United States Coast Guard Ninth District as noted below:
The Ninth Coast Guard will need to be contacted at least 45 days prior to the start of work to coordinate the in-water work. Contact info: Scot Striffler, Bridge Project Manager, Ninth Coast Guard District PH: (216) 902-6087 FAX: (216) 902-6088 Scot.M.Striffler@USGS.MIL
9. If any animals, snake, turtle, bird, salamander, etc. is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue. 
10. Any work within the globally rare Oak Openings region shall be limited to the very minimum of earth disturbance necessary to perform the work.  The very minimum amount work shall be done off the existing pavement.  Care shall be taken to not disturb the existing vegetation. 
11. Access to all multi-use paths shall be maintained at all times during construction by ODOT and the contractor.
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12. Pedestrian access shall be maintained at all times by ODOT and the contractor.  
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	Form Preparer
	District 2
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	April 21, 2017
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