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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Non-Federal


	Private Funding:
	No


	
	


Project Description: 
This project is an electrical maintenance contract for three bridges within District 2. (1) LUC-280 (Veterans Glass City Skyway) Bridge over the Maumee River, (2) LUC-65 (Craig Street Bridge) over the Maumee, and (3) OTT-163 Bridge over the Portage River.  Maintenance will also be performed on 4 storm water pump stations located at: 
LUC-280- 0220-Storm water pump station located at Starr Avenue and I-280, Toledo, OH 
LUC-280- 0564-Storm water pump station located at Manhattan Blvd. and I-280, Toledo, OH 
OTT-51- 0973- Storm water pump station located at the Woodville Rd. & Norfolk Southern Railroad overpass, Allen Township, Ottawa County OH 
FUL-120- 1265- Storm water pump station located at the Indiana & Ohio RR underpass, Amboy Township, Fulton OH).
The work on these structures does not require any US Army Corps of Engineer permit since there is no work below the deck of any bridge and not work which impacts waterways.
The bald eagle nest shown on the ecological map is over 1,000 feet away from the bridge and therefore is outside the 660 feet range in which USFWS requires timing restrictions.  This project is located within a special flood hazard area, however there will be no impacts to the floodplain, as shown in the coordination in the project file. 
All work is within the existing right of way and there will be no utility impacts. The contract begins in January of 2018 and lasts one calendar year (until 12-31-18). During maintenance activities, lane closures on the bridges are possible; however, a minimum of one lane of traffic will be maintained at all times and the notification dates within the Traffic Engineering Manual shall be followed.
	STIP Reference #
	SLI 12


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(1) Activities which do not involve or lead directly to construction, such as planning and technical studies; grants for training; engineering to define the elements of a proposed action or alternatives so that social, economic, and environmental effects can be assessed; and Federal-aid system revisions which establish classes of highways on the Federal-aid highway system. Examples include: Study type projects (i.e. feasibility studies, etc.); Projects that utilize no federal monies or require no federal actions (State-funded actions only); Land donations to ODOT associated with ROW permits (non-NHS/non-Limited Access right-of-way). (Environmental Site Assessment issues will require coordination with ODOT-OES) (State-funded actions only).

	
	(29) Purchase, construction, replacement, or rehabilitation of ferry vessels (including improvements to ferry vessel safety, navigation, and security systems) that would not require a change in the function of the ferry terminals and can be accommodated by existing facilities or by new facilities which themselves are within a CE.


	Environmental Commitments:
	Yes
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1. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
2. Work on the structures over Section 10 waters (LUC-280 and LUC-65 over the Maumee River and OTT-163 over the Portage River) shall not be performed between the bridge deck and the water within the navigation channel.  Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.            
3. Due to the known presence of Ohio endangered blue spotted salamander within the project area, if any salamander is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
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4. If at any time there may be a delay in opening the LUC-65-5.35 (Craig Memorial) bridge or OTT-163-24.11 (Monroe Street) bridge for vessels to pass, the US Coast Guard shall be notified by the contractor as soon as it is known that a delay is possible in order for the USCG to alert users. 
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2. Work on the structures over Section 10 waters (LUC-280 and LUC-65 over the Maumee River and OTT-163 over the Portage River) shall not be performed between the bridge deck and the water within the navigation channel.  Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.            
3. Due to the known presence of Ohio endangered blue spotted salamander within the project area, if any salamander is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
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4. If at any time there may be a delay in opening the LUC-65-5.35 (Craig Memorial) bridge or OTT-163-24.11 (Monroe Street) bridge for vessels to pass, the US Coast Guard shall be notified by the contractor as soon as it is known that a delay is possible in order for the USCG to alert users. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick Neal
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	May 15, 2017

	Stacy Schimmoeller PROGRAM ADMIN 3
	May 15, 2017
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