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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	LUCAS COUNTY ENGINEER


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The Lucas County Engineer is proposing to resurface Old State Line Road (County Road 34) from Wilkins Road to Fulton-Lucas Road in Harding Township, Lucas County. Additional work includes full depth pavement repairs in certain areas, replacing raised pavement markers, and restriping the pavement markings. All work is within the existing right of way and no utility impacts are anticipated. There are several streams within the project area, however there will be no work within these streams. No waterway permit from the US Army Corps of Engineers is required. Construction is expected to begin in the spring of 2018 and last approximately 60 days. During construction, one lane of traffic will be maintained at all times.   
	STIP Reference #
	SLI 16


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. Notes shall be placed in the plans by ODOT directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-8 and 642-58 to ensure compliance with Federal notification requirements.  
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and the Lucas Count Engineer, as required.
6. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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7. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
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	Form Preparer
	District 2
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	June 2, 2017

	Phoenix Golnick Neal ENV SPEC 2
	June 2, 2017
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