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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	WOOD COUNTY ENGINEER


	ODOT District
	2


	Funding Source
	Federal, State, Other


	Private Funding:
	No


	
	


Project Description: 
The proposed project consists of one bridge located within Lake Township in Wood County, Ohio.  The bridge crosses over Cedar Creek at Latcha Road (T065B-0001). The project area is primarily agricultural with homes relatively close to the culvert crossings.  The proposed work is part of the Ohio Bridge Partnership Program which includes replacing the bridge and additional right of way is needed for a temporary structure used to maintain traffic.  
This bridge was originally included in the project WOO-CR321/TR102-Var Gp5FY15 (PID 97642), but after challenges arose with the maintenance of traffic that would have occurred during construction, the bridge was moved into the current project and PID.  This allowed for additional right of way to be acquired to allow for a temporary bridge to be constructed and used while the new permanent bridge construction will occur. 
	STIP Reference #
	SLI 16


	Select the appropriate project type:
	(28) Bridge rehabilitation, reconstruction, or replacement or the construction of grade separation to replace existing at-grade railroad crossings, if the actions meet the constraints in 23 CFR 771.117(e). Examples include: Railroad projects that close or relocate at-grade crossings


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Permit Determination and/or Permit Application Approval Pending


	Isolated Wetland Permit
	No


	Endangered Species:
	Present; No finding of May Affect, Likely to Adversely Affect


	Endangered Species - Coordination
	No Effect


	100-Year Floodplain:
	Encroachment Within the SFHA is a Functionally Dependent Use


	EO 11988/NFIP Coordination and Documentation Completed:
	Yes


	NFIP Local Floodplain Coordinator Notification Date:
	12/16/2014


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Not Present


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Yes


	Hazardous Materials - OES Approval Date:
	09/30/2015


	Phase I ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall notify ODOT a minimum of 18 days prior to beginning any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  If an Ohio Environmental Protection Agency (OEPA) Notice of Intent (NOI) is required, the required post construction BMPs shall be included in the design and the NOI form shall be submitted as required.
3. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
4. A mussel survey and relocation in accordance with ODNR and USFWS protocols shall be performed at the project site prior to any in-stream work.
5. Due to work in a Zone A floodplain, the contracted designer must submit a letter of compliance (LD-51 Form) and calculations showing that the carrying capacity of Cedar Creek will not change after work is complete. All floodplain regulations shall be followed throughout design and construction. 
6. The project requires a waterway permit for work within Cedar Creek which is attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
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1. The contractor shall notify ODOT a minimum of 18 days prior to beginning any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. The specifications set forth in the most current version of ODOT's Construction and Material Specifications, Location and Design Manual and Standard Drawings will be used to ensure adequate erosion and sediment control during construction.  Disturbed areas will be reseeded.  If an Ohio Environmental Protection Agency (OEPA) Notice of Intent (NOI) is required, the required post construction BMPs shall be included in the design and the NOI form shall be submitted as required.
3. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
4. A mussel survey and relocation in accordance with ODNR and USFWS protocols shall be performed at the project site prior to any in-stream work.
5. Due to work in a Zone A floodplain, the contracted designer must submit a letter of compliance (LD-51 Form) and calculations showing that the carrying capacity of Cedar Creek will not change after work is complete. All floodplain regulations shall be followed throughout design and construction. 
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6. The project requires a waterway permit for work within Cedar Creek which is attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
[bookmark: _Toc256000004]Preparers  & Approvals
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	September 8, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	September 8, 2016
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[bookmark: _Toc256000009]General
Aerial.GIF
County.doc
USGS Topo.bmp
[bookmark: _Toc256000010]ESA
ESA Screening.pdf
OES Coordination IOC.pdf
ESA map.GIF
Asbestos Survey.pdf
[bookmark: _Toc256000011]Cultural Resources
OHPO Map.pdf
Section 106 RFR.pdf
Coordination with SHPO.pdf
[bookmark: _Toc256000012]Ecological
NHDB Map.pdf
NWI Map.GIF
ESR Level 1.pdf
USFWS Comments.pdf
ODNR Comments.pdf
Coordination Sent to Agencies.pdf
USACE Preliminary Jurisdictional Determination.pdf
Level 1 ESR WOO-Latch Rd PID 100386.pdf
Coordination with USFWS.pdf
Consult Form WOO-Latch Rd PID 100386.pdf
ODNR Comments 2.pdf
Mussel Survey Relocation.pdf
Mussel Survey Submittal to ODNR.pdf
[bookmark: _Toc256000013]Other Resources
Well Logs.pdf
Wood County SWAP.docx
[bookmark: _Toc256000014]Environmental Justice
Below Poverty.GIF
Minority Population.GIF
[bookmark: _Toc256000015]Public Involvement
Property Owner Notification Letter.pdf
Public Comments Received.pdf
Response to Public Comments.pdf
Website Packet.pdf
[bookmark: _Toc256000016]Permits
FEMA map.pdf
Floodplain Coordination.pdf
Temporary Fill Checklist.pdf
Permit Determination Request.pdf
PD IOC.pdf
Pre Construction Notification.pdf
PCN Attachments.pdf
Special Provisions.pdf
USACE 404 Approval.pdf
Regional General Permit B.pdf
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Approved CE.docx
image1.jpeg




