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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
This project proposes to resurface State Route 67 (SR 67) from State Route 101 (SR 101) to State Route 18 (SR 18) in Seneca County due to low pavement condition ratings (PCR).  Bridge maintenance work (waterproofing, upgrading bridge guardrail (GR), deck edges, drip edge, sealing, wing wall repairs, and approach work) is also proposed on 5 structures listed below. The specific work for each bridge is shown on the footprints in the project file.  There is no work outside of right of way (R/W) and there is no work below the Ordinary High Water Mark (OHWM). No floodplains will be impacted by this project.
1. SEN-67-0243 over Honey Creek - Traffic will be maintained with flaggers
2. SEN-67-0713 over East Branch of Rock Creek - 5 day closure
3. SEN-67-0737 over East Branch of Rock Creek - 45 day closure 
4. SEN-67-0834 over East Branch of Rock Creek - 30 day closure
5. SEN-67-0984 over Rock Creek -  45 day closure 
Detour routes will be posted and public involvement letters were sent to residents that would be effected by the closures.  Emergency services and schools were also notified of the project and to gather comments on the maintenance of traffic. All the public involvement can be found in the project file.  No comments have been received at this time; however, if any are received they shall be responded to. 
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	(3) No Historic Properties Affected


	Cultural Resources Coordination Date:
	04/19/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
4. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the Ordinary High Water Mark (OHWM) of any stream and/or within a wetland.  Any work below the OHWM is a violation of the Federal Clean Water Act of 1977.  
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6. A plan note will be added to the construction plans in order to address the project's location in the karst region of Northwest Ohio. 
[bookmark: _Toc256000002]Environmental Commitments
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Commitments
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
4. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the Ordinary High Water Mark (OHWM) of any stream and/or within a wetland.  Any work below the OHWM is a violation of the Federal Clean Water Act of 1977.  
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6. A plan note will be added to the construction plans in order to address the project's location in the karst region of Northwest Ohio. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Eli Barber, Phoenix Golnick


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	September 22, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	September 22, 2016
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Drinking Water Protection Plan Note.pdf
[bookmark: _Toc256000010]General
USGS Quadrangle Topographical Map.pdf
Schematic Plan.pdf
Bridge Footprints.pdf
Aerial Map.pdf
County Map.pdf
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Asbestos Report SEN-67-0713.pdf
Asbestos Survey Report SEN-67-0834.pdf
Asbestos Survey Report SEN-67-0984.pdf
Asbestos Survey SEN-67-0737.pdf
EPA DemoReno Form SEN-67-0713.doc
EPA DemoReno Form SEN-67-0737.doc
EPA DemoReno Form SEN-67-0834.doc
EPA DemoReno Form SEN-67-0984.doc
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OHPO Cultual Map.pdf
Buckeye Assets Mapping.pdf
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Eco map.pdf
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Water Source Protection Area Map.pdf
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Minority Map.PNG
Poverty Map.PNG
[bookmark: _Toc256000016]Public Involvement
Property Owner Notification Letter.pdf
Notification Mailing List.xlsx
EMA and School Notification.pdf
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FEMA FIRM.pdf
Floodplain Impacts.pdf
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