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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Non-Federal


	Private Funding:
	No


	
	


Project Description: 
The proposed project includes bridge maintenance on the State Route 295 bridge over the Maumee River in Grand Rapids, Wood County, Ohio.  Work involves replacing the bridge parapets, sidewalks, deck overlay, and converting the abutments to semi-integral due to a low bridge rating. Catch basins and guardrails near the ends of the bridges will also be fixed/replaced and the pavement at the bridge approaches will be repaired/replaced as noted on the plans. 
No work will be performed below the Ordinary High Water Mark (OHWM) of the Maumee River so no waterway permits are needed.  Coordination with the US Coast Guard (USCG) was completed which confirmed this and is included in the project file. The approach work is located within a special flood hazard area however there will be no impact to the floodplain, as shown in the project file.  The coordination completed with the Ohio Department of Natural Resources (ODNR) Scenic Rivers is included in the project file and all their comments have been addressed either through commitments or additional coordination.  Coordination was done with the City of Toledo Metroparks and ODNR for the adjacent Providence Metropark and General Store which is a Section 4(f) and 6(f) resource.  The coordination is shown in the project file and addressed all their comments.   Alternate access to the Ludwig Mill and corresponding Historic District will be maintained and clearly signed.  In addition, the work falls withinAppendix A for undertakings with Minimal Potential to Cause Effect.   A closure detour will be posted for 60 days during construction. Coordination was completed with the public, local emergency services, police, and schools, as shown in the project file.
	STIP Reference #
	SLI 32


	Select the appropriate project type:
	(28) Bridge rehabilitation, reconstruction, or replacement or the construction of grade separation to replace existing at-grade railroad crossings, if the actions meet the constraints in 23 CFR 771.117(e). Examples include: Railroad projects that close or relocate at-grade crossings


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Not Present


	Endangered Species:
	No Impacts to Protected Species and Critical Habitat


	100-Year Floodplain:
	No Encroachment Within a Special Flood Hazard Area (SFHA)


	Section 4(f):
	Present; No Programmatic Evaluation or Individual Evaluation Required


	Section 4(f) Determination:
	Temporary No Use Exception - 774.13(d)


	Section 4(f) Determination Date - 774.13(d)
	11/17/2016


	Section 6(f):
	Present; No 6(f) Conversion Required


	Section 6(f) Determination:
	Temporary Non-Conforming Use


	Section 6(f) Determination Date:
	07/31/2015


	Cultural Resources:
	Not Present


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Studies Not Required


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland, including the Maumee River and canal.  
5. Access to the Providence Metropark General Store will be maintained at all times, except for the time needed for temporary occupancy of the property and/or temporary access restrictions and/or closures needed to facilitate construction activities.  Closure of the park access shall be less than 6 months in duration. 

6. Temporary construction fencing will be installed along proposed construction limits prior to the start of construction activities to protect the 4(f) property and the public.  This includes entrances to the Providence Metropark General Store parking lot north of the Maumee River on the east side of SR 295 and the entrance for maintenance vehicles on the west side of SR 295. 

7. Appropriate signage will be installed along the roadways, within the park, and along the Towpath Trail to alert users of temporary access restrictions and/or closures, in order to direct users to the main Providence Metropark parking lot and Towpath Trail along the canal in order to access the General Store.

8. The staging and/or storage of construction equipment will not take place outside proposed construction limits, within Providence Metropark property boundaries. 

9. The contractor will closely coordinate the construction schedule and signage needs within the park with Metroparks of the Toledo Area.

10. Closure of the park entrances shall occur after school ends but before the Village of Grand Rapids Apple Butter Festival and last approximately 4 weeks.
11. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
12. No material shall be disposed of within 1000 feet of the top of bank of the Maumee State Scenic River. 
13. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
14. The vertical and horizontal clearances for the navigational channel of the bridge shall not change and shall remain open at all times during construction. 
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Commitments
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland, including the Maumee River and canal.  
5. Access to the Providence Metropark General Store will be maintained at all times, except for the time needed for temporary occupancy of the property and/or temporary access restrictions and/or closures needed to facilitate construction activities.  Closure of the park access shall be less than 6 months in duration. 

6. Temporary construction fencing will be installed along proposed construction limits prior to the start of construction activities to protect the 4(f) property and the public.  This includes entrances to the Providence Metropark General Store parking lot north of the Maumee River on the east side of SR 295 and the entrance for maintenance vehicles on the west side of SR 295. 

7. Appropriate signage will be installed along the roadways, within the park, and along the Towpath Trail to alert users of temporary access restrictions and/or closures, in order to direct users to the main Providence Metropark parking lot and Towpath Trail along the canal in order to access the General Store.

8. The staging and/or storage of construction equipment will not take place outside proposed construction limits, within Providence Metropark property boundaries. 

9. The contractor will closely coordinate the construction schedule and signage needs within the park with Metroparks of the Toledo Area.

10. Closure of the park entrances shall occur after school ends but before the Village of Grand Rapids Apple Butter Festival and last approximately 4 weeks.
11. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
12. No material shall be disposed of within 1000 feet of the top of bank of the Maumee State Scenic River. 
13. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
	
	 Environmental Document Level: C2
PID 96225 WOO SR 295 0.02 Bridge
Approved: December 29, 2016



14. The vertical and horizontal clearances for the navigational channel of the bridge shall not change and shall remain open at all times during construction. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	December 29, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	December 29, 2016
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General Plan Note.pdf
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Coordination with ODNR - Temporary Non-Conforming Use.pdf
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Aerial Map.png
Stage 2 Design.pdf
USGS Quadrangle Topographical Map.pdf
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Asbestos Survey Report WOO-295-0002.pdf
EPA Demo Reno form WOO-295-0002.doc
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Minimum Potential to Cause Effects - A.pdf
Buckeye Assets Mapping.PNG
Project Study Area Map.pdf
[bookmark: _Toc256000015]Ecological
ODNR Scenic Rivers Comments.pdf
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Eco Map.pdf
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Water Source Protection Area Map.pdf
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WOO-295-0.02 Bridge PID (96225) Section 6(f) Determination.pdf
Correspondence with OWJ.pdf
LWCF Grant Listing.pdf
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EJ Documentation.pdf
Census Mapping.pdf
[bookmark: _Toc256000019]Public Involvement
Trustee Notification.pdf
Trustee Notification List.xlsx
Village Admin Notification.pdf
School Comment and Response.pdf
Fire Department Comment and Response.pdf
Press Release Recipients.pdf
News Articles.pdf
Press Release.pdf
Chamber of Commerce Comment and Response.pdf
Response to Public Comments.pdf
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