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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
This project proposes to resurface US Route 6 (US-6) from County Road P-3 (CR P-3) to the Henry-Wood County line and State Route 65 (SR-65) from State Route (SR-110) to the Henry-Wood County Line due to poor pavement conditions.  (Since the CE was opened the project name has changed to HEN-6/65-17.81/17.09.)  Bridge work is included in the project due to low bridge ratings; however, no work will occur below the Ordinary High Water Mark (OHWM) of any stream. Detours for bridge closures will be posted.  The local public, emergency services, and schools have been notified and requested for comments, as shown in the project file.
Mary Jane Thurston State Park, a 4(f) resources, is located at the eastern end of the project along SR-65; however, access to the park shall be maintained at all times. 
The work on SR-65 is within 1000 feet of the State Scenic Maumee River.  Coordination with the Scenic River Coordinator was conducted and included in the project file. 
Work within floodplains will have no impact to the floodplain, as documented in the project file. 
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	08/11/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, the public, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by ODOT and the contractor, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the Ordinary High Water Mark (OHWM) of any stream and/or within a wetland. Any work below the OHWM or within a wetland is a violation of the Federal Clean Water Act of 1977.   
5. A plan note will be added to the construction plans in order to address the project's location in relation to a public drinking water source.
6. Access to Mary Jane Thurston State Park, located along State Route 65 between County Road 2 and County Road 1 (the Wood County and Henry County Line), shall be maintained at all times by ODOT and the contractor. 
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7. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, the public, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by ODOT and the contractor, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the Ordinary High Water Mark (OHWM) of any stream and/or within a wetland. Any work below the OHWM or within a wetland is a violation of the Federal Clean Water Act of 1977.   
5. A plan note will be added to the construction plans in order to address the project's location in relation to a public drinking water source.
6. Access to Mary Jane Thurston State Park, located along State Route 65 between County Road 2 and County Road 1 (the Wood County and Henry County Line), shall be maintained at all times by ODOT and the contractor. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	October 13, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	October 13, 2016
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Drinking Water Plan Note.pdf
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Aerial Map.pdf
County Map.pdf
USGS Quadrangle Topographical Map.pdf
Stage 3 Design.pdf
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Screening Map.pdf
NESHAP Asbestos Report for HEN-65-1828.pdf
Demo-Reno Form for HEN-65-1828.doc
EPA DemoReno Form for HEN-6-2072.doc
EPA DemoReno Form for Hen-6-2182.doc
EPA DemoReno Form for HEN-6-2521.doc
EPA DemoReno Form for HEN-6-2784.doc
EPA DemoReno Form for Hen-65-1828.doc
NESHAP asbestos Report for HEN-6-2072 .pdf
NESHAP Asbestos Report for HEN-6-2182.pdf
NESHAP Asbestos Report for HEN-6-2521.pdf
NESHAP Asbestos Report for HEN-6-2784.pdf
Asbestos Survey.pdf
Asbestos Survey.doc
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Buckeye Assets Mapping.pdf
Records Check.pdf
Minimum Potential to Cause Effects - A.pdf
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Eco Map.pdf
ODNR Scenic River Field Review Form.pdf
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Water Source Protection Area Map.pdf
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Property Owner Notification Letter.pdf
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