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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
ODOT District 2 is proposing to improve State Route-109 (SR-109, South Madison Street) in Delta and York Township, Fulton County as FUL-109-3.21, Project Identification Number (PID) 95726. The project will include the resurfacing of SR-109 from County Road D north to US Route-20A (US-20A, West Main Street) and the replacement of a culvert at Straight Line Mile (SLM) 5.26, which is between County Road F and Township Road EF.  The culvert replacement was originally programmed under PID 95855, FUL-109-5.26, which was combined into this project.  The previous identification information will be seen on some documents in the project file, but refers to the culvert and this project.  A section of US-20A was also proposed for resurfacing, but this section has since been removed from the project.  

Land use within the project corridor is predominantly agricultural, with a mix of older farmsteads and modern single-family homes scattered throughout. As SR-109 approaches US-20A at the north end of the project corridor, agricultural land use makes a transition to dense residential housing associated with the Village of Delta.
The project corridor was evaluated for the presence of cultural resources, including: properties listed on (or potentially eligible for listing on) the National Register of Historic Places (NRHP), Ohio Archaeological Inventory (OAI) sites, and Ohio Historic Inventory (OHI) buildings and structures. There are no records for NRHP or OAI properties within the project corridor. A previously recorded OHI property (King Cemetery) is located adjacent to the project corridor; however, this property will not be impacted by the proposed construction activities required for the completion of this project.
Project construction will be limited to the road right-of-way, with the exception of the culvert replacement located at SLM 5.26. New right-of-way will be required in this area in order to replace the deteriorated stone box culvert with 100 feet of new pipe, associated concrete headwall, and necessary grading. The area surrounding the new culvert and headwall will be graded to promote drainage along SR-109. Work associated with culvert replacement in this portion of the project site will occur within the 100-year floodplain (Zone AE) associated with Bad Creek.
A small, unnamed tributary (Stream 1) originates at the existing culvert on the west side of SR-109. Stream 1 flows east under SR-109 through the culvert and continues east where it drains into Bad Creek (approximately 0.20 mile from the project area). In order to complete the culvert replacement and grading, it will be necessary to remove a small area of successional woods (approximately 0.034 acre). One tree is located within the construction limits that provides potential habitat for the federally endangered Indiana bat (Myotis sodalis) and/or the federally threatened northern long-eared bat (Myotis septentrionalis); in order to protect these species during their summer roosting and brood-rearing period, tree removal for this project will only occur between October 1 and March 31. Roadway ditches within the project limits lack an Ordinary High Water Mark and are not jurisdictional.
The ecological coordination and responses to ODNR comments state, "ODOT commits to following SS832 to minimize impacts to existing riparian habitat zones," and "ODOT commits to following ODOT CMS (107.10) in order to ensure staging, storage, waste and borrow areas are appropriately sited."  Both SS832 and CMS 107.10 are standard in every project contract and are therefore not included as environmental commitments. 
The project is expected to award in June 2017.
	STIP Reference #
	SLI 32


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(28) Bridge rehabilitation, reconstruction, or replacement or the construction of grade separation to replace existing at-grade railroad crossings, if the actions meet the constraints in 23 CFR 771.117(e). Examples include: Railroad projects that close or relocate at-grade crossings


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Permit Determination and/or Permit Application Approval Pending


	Isolated Wetland Permit
	No


	Endangered Species:
	Present; No finding of May Affect, Likely to Adversely Affect


	Endangered Species - Coordination
	May Affect, Not Likely to Adversely Affect


	Endangered Species - Coordination Date
	11/24/2015


	Endangered Species - Critical Habitat Present/Impacted
	Indiana bat

	
	Northern long-eared bat


	Endangered Species - Other Critical Habitat Present/Impacted:
	No


	100-Year Floodplain:
	Encroachment Within the SFHA is a Functionally Dependent Use


	EO 11988/NFIP Coordination and Documentation Completed:
	No


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	No Historic Properties Affected


	Cultural Resources Coordination - SHPO Concurrence Date:
	01/21/2016


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	11/03/2015


	Hazardous Materials - ESA Screening Conducted
	Yes


	Hazardous Materials - OES Approval Date:
	11/03/2015


	Phase I ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, the public, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
3. If required by local ordinance, a construction noise plan note will be developed and implemented.
4. The project is located within the known ranges of the federally endangered Indiana bat (Myotis sodalis) and the federally threatened northern long-eared bat (Myotis septentrionalis). No trees shall be removed under this project from April 1 through September 30. All necessary tree removal shall occur from October 1 through March 31. This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act. For the purposes of this note: a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter (at a height of 4.5 feet above the ground surface), and a minimum height of 13 feet.
5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except the FUL-109-5.26 culvert over an Unnamed Tributary to Bad Creek.
6. The project requires a waterway permit for the culvert replacement located on SR-109 at SLM 5.26 over the Unnamed Tributary to Bad Creek which will be attached to the plans as Special Provisions. No work below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by ODOT. All conditions of the permit shall be followed throughout construction by the contractor.  
7. Work associated with the culvert replacement located on SR-109 at SLM 5.26 is within a mapped 100-year floodplain (Zone AE) associated with Bad Creek. Coordination to document compliance with Executive Order 11988 will be completed prior to project construction.
8. The waterway permit will be submitted to the appropriate agencies prior to any tree clearing for the project.
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1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, the public, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
3. If required by local ordinance, a construction noise plan note will be developed and implemented.
4. The project is located within the known ranges of the federally endangered Indiana bat (Myotis sodalis) and the federally threatened northern long-eared bat (Myotis septentrionalis). No trees shall be removed under this project from April 1 through September 30. All necessary tree removal shall occur from October 1 through March 31. This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act. For the purposes of this note: a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter (at a height of 4.5 feet above the ground surface), and a minimum height of 13 feet.
5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except the FUL-109-5.26 culvert over an Unnamed Tributary to Bad Creek.
6. The project requires a waterway permit for the culvert replacement located on SR-109 at SLM 5.26 over the Unnamed Tributary to Bad Creek which will be attached to the plans as Special Provisions. No work below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by ODOT. All conditions of the permit shall be followed throughout construction by the contractor.  
7. Work associated with the culvert replacement located on SR-109 at SLM 5.26 is within a mapped 100-year floodplain (Zone AE) associated with Bad Creek. Coordination to document compliance with Executive Order 11988 will be completed prior to project construction.
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8. The waterway permit will be submitted to the appropriate agencies prior to any tree clearing for the project.
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	Form Preparer
	Jeff Pettit
Davey Resource Group
1500 North Mantua Street, Kent OH 44240
330-673-5685
jeff.pettit@davey.com



	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick, Gregory Snowden, Jeff Pettit
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	June 1, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	June 1, 2016
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Aerial Map.pdf
USGS Quadrangle Topographical Map.pdf
County Map.pdf
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Screening.pdf
OES Recommendations - Screening.pdf
ESA Site Map.png
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Section 106 Request for Review.pdf
OHPO Map.pdf
Consulting Parties Comments.pdf
OES Approval - No Historic Properties Affected.pdf
Project Related Correspondence.pdf
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Level 1 Ecological Survey.pdf
Coordination Sent to Agencies.pdf
ODNR Comments.pdf
Response to ODNR Comments.docx
USFWS Comments.pdf
Response to USFWS Comments.pdf
NHBD Map.pdf
Auto Cad Drawings.dwg
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Water Source Protection Area Map.docx
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Low Income Mapping.pdf
Minority Mapping.pdf
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Property Owner Notification Letter.pdf
Notification Mailing List.csv
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