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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This project proposes to resurface State Route 64 (SR-64) from US Route 24 (US-24) to County Road 109 (CR-109) in Lucas County due to poor pavement conditions. This project also includes bridge work (replace wearing surface and seal joints) due to poor conditions. There are no closures or detours anticipated for this work. All work will occurs within the existing right of way and above OHWM. This project is located within a special flood hazard area but there will be no impacts to the floodplain, as shown in the project file. An ecological field review was performed by ODOT OES and D2 environmental staff on 10/18/2016 to determine if any state listed plant species were located within the right of way as this project is located within the globally rare Oak Opening Region. No listed plants were found.
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	05/03/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. Due to the known presence of Ohio threatened Blanding's and Spotted turtles within the project area, if any turtle is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
6. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source 
7. Due to the location of the project within the globally rare Oak Openings region, there shall be no earth disturbance starting 3 feet from the edge of the existing pavement from LUC-64-2.68 to LUC-64-8.91.  No work shall be done over 3 feet off the existing pavement and care shall be taken to not disturb the existing vegetation in this area.
8. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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9. Access to the Wabash-Cannonball South Fork Trail shall be maintained at all times.
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1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. Due to the known presence of Ohio threatened Blanding's and Spotted turtles within the project area, if any turtle is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
6. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source 
7. Due to the location of the project within the globally rare Oak Openings region, there shall be no earth disturbance starting 3 feet from the edge of the existing pavement from LUC-64-2.68 to LUC-64-8.91.  No work shall be done over 3 feet off the existing pavement and care shall be taken to not disturb the existing vegetation in this area.
8. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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9. Access to the Wabash-Cannonball South Fork Trail shall be maintained at all times.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick ENV SPEC 2
	January 4, 2017

	Phoenix Golnick ENV SPEC 2
	January 4, 2017
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Drinking Water Protection Plan Note.pdf
[bookmark: _Toc256000010]General
Stage 2 Design.pdf
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