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	Project Sponsor
	PORT CLINTON


	ODOT District
	2


	Funding Source
	Federal, State, Other


	Private Funding:
	No


	
	


Project Description: 
This City of Port Clinton project proposes to add a sidewalk within the right of way on the south side of State Route 163 (West Lakeshore Drive) from Ritchy Road to the existing sidewalk near the bridge over the Portage River in Port Clinton, Ottawa County.
 
	STIP Reference #
	SLI 16


	Cultural Resources Coordination:
	


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. Access to adjacent properties will be maintained during construction by the contractor
2. The contractor shall perform all work within the existing right of way. 
3. The contractor shall notify the City of Port Clinton a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, the City of Port Clinton will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work
4. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
5. If required by local ordinance, a construction noise plan note will be developed and implemented.
6. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
7. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut outside the construction limits shown on the plans, approval must be given by the ODOT  District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized.  
8. The contractor shall take all precautions to prevent any and all material from going into Lake Erie, roadside ditches, streams, wetlands, or other waters during all construction operations. The contractor shall immediately remove any material that falls into the Lake Erie, roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any Lake Erie, wetlands, streams, or other waters. No work or staging is permitted below the top of bank of Lake Erie, any stream, and/or within a wetland.
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9. A floodplain permit has been obtained and requirements have been incorporated into the plans.  Changes to the plans during construction shall be coordinated with the engineer who will determine if the floodplain permit needs updated. 
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Commitments
1. Access to adjacent properties will be maintained during construction by the contractor
2. The contractor shall perform all work within the existing right of way. 
3. The contractor shall notify the City of Port Clinton a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, the City of Port Clinton will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work
4. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
5. If required by local ordinance, a construction noise plan note will be developed and implemented.
6. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
7. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should any tree need to be cut outside the construction limits shown on the plans, approval must be given by the ODOT  District Environmental Coordinator (DEC) prior to tree cutting. Notice must be given to the DEC a minimum of 2 weeks prior to requested tree removal.  There is no guarantee that tree clearing above what is shown in the plans will be authorized.  
8. The contractor shall take all precautions to prevent any and all material from going into Lake Erie, roadside ditches, streams, wetlands, or other waters during all construction operations. The contractor shall immediately remove any material that falls into the Lake Erie, roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any Lake Erie, wetlands, streams, or other waters. No work or staging is permitted below the top of bank of Lake Erie, any stream, and/or within a wetland.
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9. A floodplain permit has been obtained and requirements have been incorporated into the plans.  Changes to the plans during construction shall be coordinated with the engineer who will determine if the floodplain permit needs updated. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	February 10, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	February 10, 2016
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Ottawa County Map.doc
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