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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This project proposes to resurface State Routes 65 and 18 in Henry County from the Putnam County line to State Route 110 due to poor pavement conditions. This project will also include work over several bridges. No work will occur below the Ordinary High Water Mark (OHWM) and no waterway or floodplain permits are required. The work on the structures will require road closures and detours, which have been coordinated with the local emergency services and schools, as shown in the project file.  The Maumee Scenic River is located at the northern end of the project, but is approximately 1,200 feet from the project area; therefore coordination with the Ohio Department of Natural Resources (ODNR) Scenic River section is not required. 
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	11/04/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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6. Due to the known presence of Ohio endangered Upland Sand Piper (Bartramia longicauda) within the project area, if any bird is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
[bookmark: _Toc256000002]Environmental Commitments
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Commitments
1. The contractor shall perform all work within the existing right of way.
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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6. Due to the known presence of Ohio endangered Upland Sand Piper (Bartramia longicauda) within the project area, if any bird is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick, Stacy Schimmoeller


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	November 4, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	November 4, 2016
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[bookmark: _Toc256000009]Environmental Commitments
Drinking Water Protection Plan Note.pdf
[bookmark: _Toc256000010]General
Aerial Map.pdf
County Map.pdf
USGS Quadrangle Topographical Map.pdf
Stage 3 Design.pdf
[bookmark: _Toc256000011]ESA
NESHAP Asbestos Report for HEN-65-1692.pdf
Demo-Reno Form for HEN-65-1692.doc
ESA Screening map.pdf
EPA DemoReno Form for HEN-65-0135.doc
EPA DemoReno Form for HEN-65-1692.doc
EPA DemoReno Form for HEN-65-0586.doc
EPA DemoReno Form for HEN-65-1618.doc
EPA DemoReno Form for HEN-65-1671.doc
NESHAP Asbestos Report for HEN-18-1698.pdf
NESHAP Asbestos Report for HEN-65-0135.pdf
NESHAP Asbestos Report for HEN-65-0586.pdf
NESHAP Asbestos Report for HEN-65-1618.pdf
NESHAP Asbestos Report for HEN-65-1671.pdf
EPA DemoReno Form for HEN-18-1698.doc
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Buckeye Assets Mapping.pdf
OHPO cultural map.pdf
Minimum Potential to Cause Effects - A.pdf
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Eco map.pdf
[bookmark: _Toc256000014]Other Resources
Water Source Protection Area Map.pdf
Well Log Data.pdf
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EMA and School Notification.pdf
Property Owner Notification Letter.pdf
Notification Mailing List.xlsx
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FEMA FIRM.pdf
Floodplain Impacts.pdf
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