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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
This project proposes to resurface United States Route 20 (US 20) in Fulton County from State Route 108 (SR-108) south to the Lucas County line. The Pavement Condition Rating (PCR) for this segment of US-20 is 72 on a scale of 1 to 100 with 100 being the highest.  District 2 was directed to resurface this section by the Pavement Management System (PMS).  Additional work includes replacing a culvert at Straight Line Mileage (SLM) 25.10 due to a culvert rating of 4 on a scale of 1 to 9 with 9 being the highest. A rating of 4 requires the structure to either be repaired or replaced.
ESA screening was approved by D2 (not OES) on 12-28-15. 
This project occur within a floodplain but has no adverse impacts to the floodplain (documentation in project file).
Notification information was sent to the one property owner/tenants effected by the closure, the local school district, and local emergency services. 
The proposed project will have no disproportionately high and adverse impacts to minority or low-income populations based upon the table above, the attached mapping, and the answers to the questions in the EJ Form and Memo. No Environmental Justice issues were raised as a result of public involvement activities conducted as part of the proposed project. Therefore, in accordance with the protections of Executive Order 12898 and FHWA Order 6640.23A, no further Environmental Justice analysis is required. 

  
	STIP Reference #
	SLI 32


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Regional General Permit


	Waterways Permit Approval Date
	04/04/2016


	Isolated Wetland Permit
	No


	Endangered Species:
	No Impacts to Protected Species and Critical Habitat


	100-Year Floodplain:
	Encroachment Within the SFHA is a Functionally Dependent Use


	EO 11988/NFIP Coordination and Documentation Completed:
	Yes


	NFIP Local Floodplain Coordinator Notification Date:
	03/10/2016


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	Minimum Potential to Cause Effect - Appendix B


	Cultural Resources Coordination - ODOT Approval Date:
	07/29/2016


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Yes


	Hazardous Materials - OES Approval Date:
	12/28/2015


	Phase I ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except the FUL-20-25.10 culvert.
5. Work associated with the culvert replacement located on US-20 at SLM 25.10 is within a mapped 100-year floodplain (Zone A). Coordination to document compliance with Executive Order 11988 will be completed prior to project construction.
6. The project requires a waterway permit for work within an unnamed tributary to Ai Creek (STA 1322+00) which is attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
7. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source. 
8. Due to the known presence of Ohio threatened Blandings Turtle within the project area, if any turtle is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
9. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except the FUL-20-25.10 culvert.
5. Work associated with the culvert replacement located on US-20 at SLM 25.10 is within a mapped 100-year floodplain (Zone A). Coordination to document compliance with Executive Order 11988 will be completed prior to project construction.
6. The project requires a waterway permit for work within an unnamed tributary to Ai Creek (STA 1322+00) which is attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
7. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source. 
8. Due to the known presence of Ohio threatened Blandings Turtle within the project area, if any turtle is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
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9. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	August 1, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	August 1, 2016
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Aerial Map.PNG
County Map.pdf
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OBD Ecological Map.gif
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Water Source Protection Area Map.pdf
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Census Mapping.pdf
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Emergency Management Notification.pdf
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Website Packet.pdf
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Coordination with Local Floodplain Administrator.pdf
Letter of Compliance - ODOT Form LD-51.pdf
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Special Provisions.pdf
image1.jpeg




