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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This project proposes to resurface State Route 579(SR 579) in Wood County from State Route 51 (SR 51) to the Ottawa County line (Fostoria Road) due to poor pavement conditions. Additional work includes replacing the decks, repairing the abutments, encasing piles, and placing rock channel protection on the slopes of the structures that carry State Route 579 over Dry Creek and Cedar Creek.  A US Army Corps permit is required for the work within the water of Dry and Cedar Creeks. Several portions of this project are located within a floodplain. All National Flood Insurance Program (NFIP) and Executive Order 11098 regulations regarding floodplain impact notifications have been followed and are included in the project file.  All work is within existing right of way and there will be no impacts to utilities.  Construction is expected to begin in the summer of 2018 and the resurfacing will last approximately 150 days. During construction, one lane of traffic will be maintained on State Route 579 with the exception of a 60 closure for the bridge work, which will require a detour. Coordination was completed with the local emergency services and school as well as with the public that will be most effected by the closure, as shown in the project file.  
	STIP Reference #
	SLI 32


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Regional General Permit


	Waterways Permit Approval Date
	03/21/2017


	Isolated Wetland Permit
	No


	Endangered Species:
	No Impacts to Protected Species and Critical Habitat


	100-Year Floodplain:
	Encroachment Within the SFHA is a Functionally Dependent Use


	EO 11988/NFIP Coordination and Documentation Completed:
	Yes


	NFIP Local Floodplain Coordinator Notification Date:
	03/28/2017


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	Minimum Potential to Cause Effect - Appendix A


	Cultural Resources Coordination - ODOT Approval Date:
	06/07/2016


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Studies Not Required


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except the WOO-579-1.04 bridge over Dry Creek and the WOO-579-1.91 bridge over Cedar Creek.
6. The project requires a waterway permit for work within Dry Creek (STA 51+21) and Cedar Creek (STA 97+41) which shall be attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
	
	


	
	 Environmental Document Level: C2
PID 97012 WOO SR 579 0.00 Resurf/Bridge
Approved: April 24, 2017




[bookmark: _Toc256000002]Environmental Commitments
[bookmark: _Toc256000003]C2
Commitments
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except the WOO-579-1.04 bridge over Dry Creek and the WOO-579-1.91 bridge over Cedar Creek.
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6. The project requires a waterway permit for work within Dry Creek (STA 51+21) and Cedar Creek (STA 97+41) which shall be attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick Neal, Stacy Schimmoeller
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	April 24, 2017

	Stacy Schimmoeller PROGRAM ADMIN 3
	April 24, 2017


	
	 Environmental Document Level: C2
PID 97012 WOO SR 579 0.00 Resurf/Bridge
Approved: April 24, 2017




[bookmark: _Toc256000007]Appendix
[bookmark: _Toc256000008]Uploaded Files by Report Section
[bookmark: _Toc256000009]General
Aerial Map.pdf
USGS Quadrangle Topographical Map.pdf
Stage 2 Design.pdf
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Water Source Protection Area Map.pdf
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Permit Determination Request.pdf
OES Permit Determination.pdf
Pre-Construction Notification.pdf
FEMA FIRM.pdf
USACE 404 Approval.pdf
Special Provisions.pdf
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Statement of Findings.pdf
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