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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
This project proposes to repair the fire damage to the IR-280 Bridge over the Maumee River in Lucas County. Work includes power washing, grinding, patching and replacing parapets, replacing and repainting sections of railing, replacing light fixtures, hydro and overlay damaged deck areas, cleaning underside, and replacing wire and conduit in necessary areas. There are no plans for this project. This project will not have impacts below ordinary high water.  In order to clean and repair the underside of the bridge deck, a snooper truck will be utilized. The vertical clearance between low steel and the top of the water surface will be temporarily changed. 
As shown on the NHDB mapping, the project is within the half mile buffer of a bald eagle nest and is approximately 1,200 feet from the nest, which does not warrant a plan note or specific work restriction dates. 
	STIP Reference #
	SLI 7


	Cultural Resources Coordination:
	


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. Access to adjacent properties will be maintained during construction by the contractor
2. The contractor shall perform all work within the existing right of way. 
3. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
4. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
5. If required by local ordinance, a construction noise plan note will be developed and implemented.
6. The contractor shall take all precautions to prevent any and all material from going into the Maumee River during all construction operations. This includes but is not limited to paint, wash water, sand/water blasting, hydrodemolition materials, etc. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. 
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7. ODOT will continue to coordinate with the United States Coast Guard (USCG) and determine their requirements and notifications for this project. 
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7. ODOT will continue to coordinate with the United States Coast Guard (USCG) and determine their requirements and notifications for this project. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:
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