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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	
	


Project Description: 
The proposed project is a contract to perform maintenance activities on the IR-280 (Veterans Glass City Skyway) including deck patching at various locations on the top of the bridge deck, replacement of torn expansion strip seals and broken gaskets, reconstruction of concrete plinths at abutment bearings, and painting metal light poles. 
	STIP Reference #
	SLI 12


	Cultural Resources Coordination:
	


	Cultural Resources Coordination Date:
	


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way. 


2. The contractor shall take all precautions to prevent any materials, including but not limited to grease, epoxy, paint, concrete, grindings, asphalt, etc. from entering waterways. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. No equipment shall be permitted in any waters.
3. Work on the structures shall not be performed between the bridge deck and the water within the navigation channel. Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.
4. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, the public, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
5. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
6. If required by local ordinance, a construction noise plan note will be developed and implemented.
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7. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
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1. The contractor shall perform all work within the existing right of way. 


2. The contractor shall take all precautions to prevent any materials, including but not limited to grease, epoxy, paint, concrete, grindings, asphalt, etc. from entering waterways. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. No equipment shall be permitted in any waters.
3. Work on the structures shall not be performed between the bridge deck and the water within the navigation channel. Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.
4. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, the public, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
5. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
6. If required by local ordinance, a construction noise plan note will be developed and implemented.
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7. Adequate erosion and sediment controls shall be implemented and maintained throughout construction, as required.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Josiah Allen, Phoenix Golnick
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	June 16, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	June 16, 2016
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