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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	WOOD COUNTY ENGINEER


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The WoodCounty Engineer proposes to upgrade two intersections and a segment of roadway in theCity of Rossford and Perrysburg Township, Ohio. The project will include the construction of two modern roundabouts, one each atthe intersections of Lime City Road/Buck Road and Buck Road/Penta CenterDrive. The roadway improvements include street widening, paved shoulders, street lighting,traffic signs, and pavementmarkings. A sidewalk/path with ADA-compliant ramps is also proposed to beconstructed along Buck Road and the project area intersections.  
Theproject is the result of a traffic study first performed by Mannik & Smith,Inc. in 2005, that showed the traffic generated by the Penta Career Centerwould result in poor traffic operations at the intersections and along Buck Road. A subsequent traffic and feasibilitystudy by DLZ beginning in 2007 resulted in four (4) alternatives beingdeveloped and studied to determine which would best meet the project's Purposeand Need. The study resulted in Wood Countyselecting a single lane roundabout alternative at both intersections and widening of Buck Road from east of BatesRoad to Penta Center Drive.
The project will be constructed in four phases, all of which will require a local detour.  The first and second phases builds the southern portion of Buck Road, west of Lime City Road and the western portion of Lime City Road, south of Buck Road.  The third phase builds a portion of the north side of Buck Road and a portion of Lime City Road, north of Buck Road.  The fourth and final phase, builds the remainder of the north side of Buck Road and the remainder of Lime City Road, north of Buck Road.  One direction of traffic, on either Buck or Lime City Roads, will need to be detoured during Phases 1, 2 and 3.  These detours will utlize local county roads Mandell Road, Bates Road, and Shreier Road.  During the fourth phase, both directions of traffic will need to be detoured for a short duration (approximately two weeks).  This detour will utilize Bates Road and Shreier Road. 
The initial Ecological Survey Report (ESR) coordination from December 30, 2015 did not include the entire project area.  In May 2016 it was realized that the project area had expanded, so the ESR was updated and submitted to the ODOT Office of Environmental Services (OES) to review.  In the May 19, 2016 email located in the project file, OES states that, "The only jurisdictional resource in the project area is Grassy Creek, which will not be impacted.  The impacts (in the updated ESR) are less than it was originally coordinated so we will not need to re-coordinate the report."  
Location mapping can be found under General/Project Information/ County Map.doc; and USGS Topographical Quadrangle Map.pd.Stage 2 Design Plans can be found under General/Project Information/Stage 2 Plans.pdf.
	STIP Reference #
	2016stipID0062FDCO


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Not Present


	Endangered Species:
	Present; No finding of May Affect, Likely to Adversely Affect


	Endangered Species - Coordination
	May Affect, Not Likely to Adversely Affect


	Endangered Species - Coordination Date
	01/27/2016


	Endangered Species - Critical Habitat Present/Impacted
	Indiana bat

	
	Northern long-eared bat


	Endangered Species - Other Critical Habitat Present/Impacted:
	No


	100-Year Floodplain:
	Encroachment Within the SFHA is a Functionally Dependent Use


	EO 11988/NFIP Coordination and Documentation Completed:
	Yes


	NFIP Local Floodplain Coordinator Notification Date:
	05/02/2016


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	No Historic Properties Affected


	Cultural Resources Coordination - SHPO Concurrence Date:
	04/18/2016


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Yes


	Hazardous Materials - OES Approval Date:
	08/03/2016


	Phase I ESA Warranted Based on Coordination with OES:
	Yes


	Phase II ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Hazardous Materials - Coordination Results
	Limited to Petroleum Related Underground Storage Tanks (USTs) and/or Releases


	Hazardous Materials - OES Approval Date - Phase I:
	08/09/2016


	Farmland:
	Urbanized Area; No Impacts in Accordance With the Farmland MOU and 7 CFR 658


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall notify ODOT and the Wood County Engineer a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. ODOT, the Wood County Engineer, and the contractor shall ensure that a National Pollution Discharge Elimination System (NPDES) permit shall be acquired prior to the start of construction.
3. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
4. The required floodplain permit and/or coordination shall be acquired by the Wood County Engineer from the City of Rossford prior to any work within the floodplain and the conditions shall be followed throughout construction by the contractor.
5. No work (temporary or permanent) shall be performed below the Ordinary High Water Mark (OHWM) elevation of 601 of Grassy Creek.  Any work below the OHWM is a violation of the Federal Clean Water Act of 1977.   
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Commitments
1. The contractor shall notify ODOT and the Wood County Engineer a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. ODOT, the Wood County Engineer, and the contractor shall ensure that a National Pollution Discharge Elimination System (NPDES) permit shall be acquired prior to the start of construction.
3. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
4. The required floodplain permit and/or coordination shall be acquired by the Wood County Engineer from the City of Rossford prior to any work within the floodplain and the conditions shall be followed throughout construction by the contractor.
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5. No work (temporary or permanent) shall be performed below the Ordinary High Water Mark (OHWM) elevation of 601 of Grassy Creek.  Any work below the OHWM is a violation of the Federal Clean Water Act of 1977.   
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	Form Preparer
	Vickie Wildeman
DLZ Ohio Inc.
614 West Superior Avenue Suite 1000, Cleveland OH 44113
216-771-1090
vwildeman@dlz.com



	Supporting Form Preparer(s)
	Natalie Dingledine, Stephen Metzer, Vickie Wildeman
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	December 29, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	December 29, 2016
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County Map.doc
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Stage 2 Plans.pdf
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Traffic Impact Study 2005.pdf
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Screening.pdf
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Site Specific Resource Mapping.pdf
Project Related Correspondence.pdf
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Eco Map .gif
Coordination Sent to Agencies.pdf
ODNR Comments.pdf
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OES Approval.pdf
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Water Source Protection Area Map.pdf
[bookmark: _Toc256000015]Environmental Justice
Census Mapping.gif
Census Mapping 2.gif
[bookmark: _Toc256000016]Public Involvement
Website Packet Post.PNG
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Public Meeting all documentation.pdf
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