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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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[bookmark: _Toc256000002]Project, Cost Schedule and Work Limits	Environmental Document Level
	D2


	PID
	92088


	Project Name
	WOO/LUC SR 64 12.03/0.00 Bridge


	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	State, Other


	Private Funding:
	No


	Local Public Funding:
	Yes


	STIP Reference #:
	2016stiplD0065FDCO


	The next phase of the proposed project is listed on the STIP
	Yes


	The current cost estimate is in line with existing federal procedures for Ohio STIP Amendments and Administration Modifications
	Yes


	Planning and Engineering
	$2,027,424.00


	Right of Way
	$631,000.00


	Construction
	$24,607,500.00


	Other
	$0.00


	An Interchange Modification / Interchange Justification Study (IMS/IJS) was completed
	No


	
	


Project Description: 
The proposed project involves the replacement of an existing bridge that carries State Route (SR) 64 over the Maumee River in order to meet current design standards and maintain access for both motorized and non-motorized users. The bridge connects the City of Waterville in Lucas County on the west side of the river to rural Wood County on the east side of the river and is designated as a pedestrian and bike connectivity route in both the Toledo Metropolitan Area Council of Governments (TMACOG) 2035 Regional Transportation Plan as well as in the current Waterville Comprehensive Plan. 
The proposed structure will be a nine-span concrete pre-stressed I-Beam with composite superstructure and reinforced concrete deck on typical reinforced concrete abutments (founded on drilled shafts) and reinforced concrete wall type piers (founded on drilled shafts). The proposed cross section will have the following characteristics: two 12-foot through lanes; 4-foot outside shoulders; 12-foot shared use path located on the left (downstream) side of the bridge with two observation platforms; and a 7-foot sidewalk located on the right (upstream) side of the bridge. The intersection of SR 64 at River Road on the Lucas County (City of Waterville) side of the bridge will involve a full signal upgrade with turning radii improvements, and the intersection of SR 64 at SR 65 on the Wood County side of the bridge will be constructed as a roundabout.
The existing structure was built in 1904, with a truss installed in 1946 and a major rehabilitation in 1988. The existing structure is a through truss structure nearing the end of its service life and is considered Functionally Obsolete with narrow lane widths (11-feet) and is inadequate for non-motorized purposes. The bridge is considered to be "fracture critical" due to its truss style design whereas it contains Fracture Critical Members (FCM).  
There are wetland and river impacts associated with the proposed project. Permanent and temporary right-of-way will be required. 
· Detailed information regarding existing bridge conditions can be found in the Alternatives Evaluation Report located in the project file under Alternatives/Reports/Alternatives Evaluation Report.pdf.
	Limits of Proposed Work
	Waterville Bridge over Maumee River


	Start (SLM):
	12.007-12.206 WOO


	End (SLM):
	0.000-0.180 LUC


	Total Work Length (Miles):
	0.711


[bookmark: _Toc256000003]Roadway Character	
	


Tab Number: SR00064
	Functional Classification:
	Collector (Urban)


	Current Average Daily Traffic:
	11900


	Current Average Daily Traffic Year:
	2018


	Design Year Average Daily Traffic:
	15500


	Design Average Daily Traffic Year:
	2038


	Daily Hourly Volume:
	1560


	Truck %:
	3


	Setting:
	Urban


	Topography:
	Level


	
	Existing
	Proposed

	Design Speed (MPH):
	55
	35

	Legal Speed (MPH):
	50
	35

	Number of Lanes:
	2
	2

	Type of Lanes:
	Through
	Through

	Pavement Width (ft):
	20
	24

	Shoulder Width (ft):
	4
	8

	Median Width (ft):
	N/A
	N/A

	Sidewalk Width (ft):
	4.6
	19


	 


[bookmark: _Toc256000004]Design Criteria For BridgesTab Number: 8702462
	Sufficiency Rating:
	044.6


	General Rating:
	5


	Date Built:
	07/01/1904


	Bridge Location:
	2.0 mi. South of USR24 


	
	Existing
	Proposed

	Bridge Type:
	344
	232

	Bridge Length (ft):
	846
	966

	Number of Main Spans:
	5
	9

	Max Span Length (ft):
	167
	112

	Load Restrictions (TON):
	120
	N/A

	Curb to Curb Width (ft):
	23.60
	32

	Shoulder Width(ft):
	2
	8

	Under Clearance (ft):
	10.54
	4.53


	 


	Bridge Type Description:
	Nine (9) span concrete pre-stressed I-Beam with reinforced concrete substructures on drilled shaft foundations.



	Load Restrictions Description:
	None, outside of Ohio legal loads for new bridge design.



	Will the structure be rehabilitated or replaced as part of the project?
	Yes


	If this bridge is a historic bridge, what type is it?
	N/A


	Remarks:
	A Structure Type Study was completed by The Mannik & Smith Group, Inc. in August 2015 as part of the Alternatives Evaluation Report. The report evaluated four bridge design options including Steel Plate Girder; Steel Haunch Plate Girder; Concrete Haunch I-Girder; and Prestressed Concrete I-Beam. Further design studies concludedthe preferred appropriate design would be a nine (9) span concrete prestressed I-Beam.  The study can be found in Chapter 6.0 of the Alternatives Evaluation Report, which is located in the project file under Alternatives/Reports/Alternatives Evaluation Report.pdf.



[bookmark: _Toc256000005]Maintenance of Traffic During Construction	A roadway, bridge or ramp closure is required
	Yes


	A temporary bridge or roadway is proposed
	No


	A detour is required for the proposed project
	Yes


	Access for local through traffic will be provided with appropriate signage
	Yes


	Provisions for through-traffic dependent businesses will be incorporated into project design
	No


	Provisions to accommodate any local special events or festivals will be incorporated into project design
	Yes


	The proposed MOT substantially impacts sensitive environmental resources
	No


	Substantial controversy is associated with the proposed MOT
	No


	Coordination has been initiated and/or completed with local emergency services, schools, public institutions/facilities, etc.
	Yes


	
	


Remarks: 
Construction of the new structure can be substantially completedwhile the existing bridge remains in service. A short-term closure of thebridge crossing (approximately 2 months) will be required toreconstruct the roadway approaches to the new bridge from at the tie ins to the current roadway. The detour will beapproximately 17-22 miles depending on which detour route is used for the nearest adjacent bridge. The two adjacent bridges that would likely be utilized for the detour routes involve the bridge in Maumee (17 mile detour) or the bridge in Grand Rapids (22 mile detour) over the Maumee River. The closure will beclosely coordinated with local emergency, law enforcement and schoolofficials. Initial coordination with agencies was made through the public involvement portion of the project via use of notifications to local governmental agencies and officials with Press Releases of public meetings and decisions, notification letters of public meetings, direct mailings to property owners along the corridor, elected officials, and local governments, and through a public comment period. All documentation of the public involvement process can be found in the Project File within the Public Involvement/Project Information section.
The specifics of the Maintenance of Traffic (MOT) plans will be developed asdetailed construction plans are completed with input from local officials. 
Marine recreational traffic/activities would be maintained during construction, but may berestricted during specific construction activities. The contractor will berequired to coordinate marine impacts with ODNR Scenic Rivers and the Division of Watercraft.
The contractor willbe required to coordinate the restricted period with ODOT and localofficials, who will notify local EMS and schools as necessary.Detour information can be found in the project file under General/Maintenance of Traffic/Detour Plan.pdf and Detour Mapping.pdf
	Are there any Environmental Commitments?
	Yes


[bookmark: _Toc256000006]Environmental Commitments, Maintenance of Traffic During Construction
1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Meetings will be held with the City of Waterville, Wood County, ODOT, and the project team following the completion of Stage 2 plans and MOT plans to confirm impacts and notify appropriate public services and facilities prior to the start of construction. 
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.  This includes the annual Roche de Boeuf Parade and Festival that occurs typically on the last Saturday in September.
[bookmark: _Toc256000007]Right of Way and Utility Involvement	The project requires Permanent Right-of-Way
	Yes


	The project requires Permanent easement(s)
	Yes


	The project requires Temporary Right-of-Way
	Yes


	Number of parcels impacted by Permanent Right-of-Way:
	9


	Number of parcels impacted by Temporary Right-of-Way:
	3


	Approximate acreage of Permanent Right-of-Way needed:
	3.99


	Approximate acreage of Temporary Right-of-Way needed:
	0.31


	Electrical lines, gas lines, water lines, sewer lines, phone lines or other utilities exist in the project area
	Yes


	Large scale transmission facilities are located within the project area
	No


	Private utility easements are located within the project area
	Yes


	The existing private utility easement will be impacted by the project
	Yes


	Coordination with identified utilities has been initiated and/or completed
	Yes


	
	


Remarks: 
Coordination with utilities has been initiated, and Stage 1 Plans were provided to the known utilities within the project area along with correspondence that requested they review the plans to confirm the accuracy of their facilities being shown on the design plans and provide feedback with any comments or corrections they have regarding their facilities.
The following utilities were provided Stage 1 Plans along with correspondence on 1/13/16:
1) Buckeye Cable (c/o Doug Hartford); 4818 Angola Road; Toledo, OH 43615; (419)-724-9820; dhartford@cablesystem.com 
2) Frontier Communications (c/o Paul Hamaker); 3126 N. McCord Road; Toledo, OH 43617; (419)-841-8675; paul.haymaker@ftr.com 
3) Time Warner Cable (c/o Don Kurtz); 205 Crystal Avenue; Findlay, OH 45840; (419)-340-0339; Donald.kurtz@twcable.com 
4) Waterville Gas & Oil (c/o Todd Black); 700 Farnsworth Road; Waterville, OH 43566; (419)-878-4972; tblack@watervillegas.com 
5) Northwestern Water and Sewer (c/o Tom Stalter); 12560 Middleton Pike; Bowling Green, OH 43402; (419)-354-9090 ext. 174; tstalter@nwwsd.org 
6) Lucas County Engineer (c/o Brian Miller); 1049 S. McCord Road; Holland, OH 43528; (419)-213-4541 ext. 4539; bwmiller@co.lucas.oh.us 
7) Lucas County Sanitary Engineer (c/o Jim Shaw); 1111 S. McCord Road; Holland, OH 43528; (419)-213-2926; jshaw@co.lucas.oh.us 
8) Ohio Gas (c/o Greg Nofiger); 1460 Quality Drive; Bryan, OH 43506; (800)-331-7396; gregnofiger@ohiogas.com 
9) Toledo Edison (c/o Randy Swope); 300 Madison Avenue; Toledo, OH 43562; (419)-249-5218; rrswope@firstenergycorp.com 
Coordination and correspondence will continue throughout the detailed design process as construction plans are finalized.
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Project History: 
Originally built in 1904 with a truss installed in 1946, and a major rehabilitation in 1988, the existing Waterville Bridge (carrying State Route 64 over the Maumee River) is a through truss structure nearing the end of its service life and is considered Functionally Obsolete with insufficient lane widths and lack of adequate non-motorized facilities. The bridge connects the City of Waterville in Lucas County on the west side of the river to rural Wood County on the east side of the river.  The bridge is currently inspected annually (once each calendar year) per the Ohio Revised Code. The non-redundant structure has two main load carrying members (trusses), and failure of one (1) truss can cause a catastrophic bridge collapse. In regard to fracture critical, the failure of one (1) load carrying tension member can cause partial or full collapse (does not matter what type of steel or fabrication process was originally used). Given the characteristics of the bridge and its existing condition, the Ohio Department of Transportation (ODOT) identified the rehabilitation or replacement of the bridge as a project on the TIP/STIP for 2017/2018 with preliminary engineering and detailed design occurring in 2014/2015. Several sources of funding are being utilized including Federal, State, and local MPO Congestion Mitigation and Air Quality (CMAQ) funds. Furthermore, the river crossing is part of a planned pedestrian and bike connectivity route in the Waterville Comprehensive Plan and a network street bike facility in the TMACOG 2035 Regional Transportation Plan.
	
	


Purpose Statement: 
The purpose of the proposed project is to improve bridge and roadway conditions, mobility and access for motorized and non-motorized users.
	
	


Need Element(s): 
The identified needs listed below have been documented as contributing to the existing mobility and traffic flow issues along State Route 64 in the City of Waterville:
· The existing Waterville Bridge has sub-standard lane widths (11 feet) and shoulder widths (1 foot), whereas current design standards per the ODOT Location & Design Manual indicate standard lane widths are lanes of 12 feet and shoulders of 4 feet. The existing roadway has a functional classification of Urban Collector and carries 360 commercial vehicles per day, or approximately 3 percent of the Average Daily Traffic (ADT). The existing structure provides insufficient lane widths for its functional use based on the expected commercial vehicle activity.
· The most recent bridge inspection performed in May 2014 indicated a general rating and operational status of 5A (out of 9) meaning fair condition with no load posting required. Per the latest inventory report, the bridge has a Sufficiency Rating (SR) of 44.7 and is considered Functionally Obsolete, meaning the existing bridge is not designed to current geometric standards. The bridge is scheduled for replacement due to the SR being under 50.
· The bridge is considered to be "fracture critical" due to its truss style design whereas it contains Fracture Critical Members (FCM).  The FCM's on the existing bridge consist of the truss diagonals, gusset plates, low chords, floor beams, floor beam connections, and sidewalk connections.  The failure of one (1) load carrying tension member can cause partial or full collapse of the structure. Inspection reports indicate these members are experiencing deterioration including section loss (some severe), pack rust, pitting, and loose rods.  Repairs were done to the floor beams and floor beam connections in 2004/2005.  In addition, the pier concrete truss seats that support the primary load carrying members are deteriorating.
· The current structure only provides a narrow pedestrian pathway (4') on one side of the structure and no bike path facility. However, this river crossing has been designated a pedestrian and bike connectivity route in the Waterville Comprehensive Plan and a network street bike facility in the TMACOG 2035 Regional Transportation Plan. Therefore this corridor and the river crossing require improved accommodation for bicycle and pedestrian activity. The ODOT Location & Design Manual indicates the standard sidewalk width is 7 feet and a minimum width for a bike path is 10 feet with a 1 foot buffer to a barrier.
	
	


Goals and Objectives: 
N/A
	
	


Summary Statement: 
The purpose of the proposed project is to improve bridge and roadway conditions, mobility and access for motorized and non-motorized users. The identified needs included sub-standard roadway geometrics, facility deficiencies, and limited access for non-motorized activities. 
	
	


Logical Termini and Independent Utility: 
The proposed project study area incorporates the existing Waterville Bridge (State Route 64) over the Maumee River which borders Lucas and Wood counties, and includes portions of the City of Waterville, Ohio on the western side of the river in Lucas County.
The proposed project has independent utility in that it will address the transportation needs to improve mobility and traffic flow along the corridor and structural functionality. This does not preclude other improvements to State Route 64 outside of the bridge area to enhance continuity, remove conflict points, and address traffic flow concerns. No other improvements outside of the State Route 64 corridor are necessary to address the purpose and need of the proposed project.
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Discuss No Build Alternative: 
The No Build Alternative maintains the current condition of the bridge and existing roadwaygeometrics, with no improvements other than planned routine maintenance. The existing structure over the Maumee River originally built in 1904 with a truss installed in 1946, and a major rehabilitation in 1988, is nearing the end of its service life and is considered Functionally Obsolete with insufficient lane widths and lack of adequate non-motorized facilities. The non-redundant structure has two main load carrying members (trusses) and failure of one (1) truss can cause a catastrophic bridge collapse. In regard to fracture critical, the failure of one (1) load carrying tension member can cause partial or full collapse (does not matter what type of steel or fabrication process was originally used). The No Build will not address any of the functionally obsolete design issues; fracture critical issues; and does not provide adequate non-motorized facilities. Therefore, the No Build does not meet the Purpose & Need for the proposed project.
	Was a Feasibility Study completed?
	No


	Was an Alternative Evaluation Report (AER) completed?
	Yes


	Date AER was approved:
	08/25/2015


	Name
	Description
	Reason Dismissed
	Included in the AER
	Preferred Alternative

	No Build
	No improvements other than routine maintenance.
	Does not meet the Purpose and Need.
	Yes
	No

	Existing Alignment
	Replace the structure utilizing the existing alignment.
	Lengthy bridge closure of approximately 12 months that would require a detour of 17 miles or 22 miles depending on detour route, which would create burden on user costs. Project requires decommission of utilities on bridge for entire year during construction.
	Yes
	No

	Parallel Alignment
	Replace the structure by constructing a new structure on a new alignment parallel to the existing bridge.
	Not dismissed.
	Yes
	Yes

	Angled Alignment
	Replace the structure by constructing a new structure on a new angled alignment from Farnsworth Road on west side of the river in the City of Waterville to the existing SR64/SR65 intersection the east side of the river in Wood County.
	Higher construction cost from longer structure length; location does not comply with Waterville Comprehensive Plan as it place bridge through future park property; potential adverse (indirect) effects on National Register Historic Places on western bridge approach; alignment could impact fishing and recreational access to Maumee River (Scenic/Recreational River) by impacting Memorial Park; and potential proximity impacts to the Toledo Metroparks-owned Granger Island.
	Yes
	No


	 


	
	


Discuss Reasons Alternative Identified as Preferred was selected: 
The Parallel Alignment alternative was selected in the Alternatives Evaluation Report as the preferred alternative because this option:Meets the Purpose and Need of the project.Allows traffic to be maintained while new structure is built, which minimizes user costs associated with an extended closure period.Consistent with both the Waterville Comprehensive Plan and the TMACOG 2035 Regional Transportation PlanDoes not require lengthy decommission of utilities on existing bridge during construction of the new structureMinimizes impacts to recreational 4(f) properties and the State Scenic/Recreational designated Maumee River
As part of the decision making process, ODOT, the City of Waterville, and the design team evaluated the build and no build alternative based on the Purpose and Need, environmental impacts, operational analyses, stakeholder input, public involvement comments, and long term future needs of the facility. Also considered was the Waterville Comprehensive Plan and the TMACOG 2035 Regional Transportation Plan. The public provided input, specifically during a public meeting that was held on March 27, 2014 at the Waterville Primary School in Waterville. The meeting had a total of 233 people sign in officially and a total of 141 comment sheets were submitted. The majority of respondents preferred either the existing alignment or parallel alignment instead of the angled alignment, and comments also indicated a desire to limit river crossing closure time, thus the parallel alignment would best satisfy the minimal closure time of these two options. Given all of this information and the evaluation process, the parallel alignment option was selected as the preferred alternative.Analysis of alternatives and structure types can be found in the Project File under Alternatives/Reports/Alternatives Evaluation Report.pdf The Alternatives Evaluation Matrix can be found in the Project File under Alternatives/Project Information/Alternatives Evaluation Matrix.pdf
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	Sensitive Areas are located within approximately 500' of the proposed project area
	Yes


	The proposed project is listed as a C1 in ODOT's CE Guidance and/or falls under 40 CFR 93.126
	No


	The proposed project involves adding capacity, a new interchange, relocating thru lanes significantly closer to sensitive areas, or expanding an intermodal center
	Yes


	Design Year ADT is 
	No


	Qualitative MSAT prepared
	Yes


	OES Concurrence Date
	12/07/2015


	OEPA Approval Date
	02/01/2016


	
	


Remarks: 
A Qualitative Mobile Source Air Toxics (MSAT) Analysis, dated December 14, 2015, was prepared by Lawhon & Associates, Inc.  On February 1, 2016, the Ohio Environmental Protection Agency (OEPA) determined the proposed project qualifies as a project of "Low Potential for Meaningful MSAT Effects". This determination was made in accordance with the Federal Highway Administrations (FHWA) Interim Guidance Update on MSATs in NEPA. 
· The Qualitative MSAT Analysis can be found in the Project File under Air/Reports/Qualitative MSAT Analysis.pdfThe OEPA Approval can be found in the Project File under Air/Coordination/OEPA Approval - Qualitative MSAT.pdf
[bookmark: _Toc256000014]Particulate Matter 2.5 (PM2.5)
	The proposed project is in an air quality non-attainment or maintenance area
	No


	
	


Remarks: 
Lucas and Wood Counties are designated as being in attainmentfor PM2.5, therefore, no additional air quality investigations arenecessary.Relevant mapping can be found in the Project File under Air/Project Information/PM2.5 Nonattainment Area Map.pdf
[bookmark: _Toc256000015]Carbon (CO)
	The State of Ohio is in attainment for CO at this time and no coordination or analysis is required
	


[bookmark: _Toc256000016]Ozone
	The proposed project is in an Ozone non-attainment or maintenance area
	No


	The proposed project is listed on the TIP
	Yes


	
	


Remarks: 
Lucas and Wood Counties are designated as being in attainment for Ozone. Furthermore, theproposed project is listed on the STIP (#2016stiplD0065FDCO) and TIP. Therefore, ozone is addressed.Relevant mapping can be found in the Project File under Air/Project Information/Ozone Nonattainment Area Map.pdf
[bookmark: _Toc256000017]Environmental Commitments
	Are there any environmental commitments?
	No
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	Noise Sensitive Areas located within approximately 500' of the proposed project area
	Yes


	Noise Analysis conducted
	Yes


	ODOT Approval Date
	12/09/2015


	The proposed project is a Type I project
	Yes


	The proposed project constructs a roadway on new location
	Yes


	The proposed project significantly changes the existing roadway's horizontal or vertical alignment
	Yes


	The proposed project adds capacity (thru travel lanes) 
	No


	The proposed project adds an auxiliary lane(s)
	No


	The proposed project negatively affects shielding of an existing roadway
	Yes


	The proposed project restripes existing pavement for an added thru lane or auxiliary lane
	No


	The proposed project adds or substantially alters an existing weigh station, rest stop, rideshare lot, or toll plaza
	No


	The proposed project causes a major change in vehicle mix
	No


	A design year noise impact was predicted
	No


	All noise attenuation measures were considered and are consistent with existing policy
	Yes


	Noise barriers proposed
	No


	The proposed project impacts identified NSAs
	No


	
	


Remarks: 
A noise analysis and subsequent report was conducted and prepared by Lawhon and Associates. Based on analysis results, traffic generated noise levels were predicted at eighteen (18) Noise SensitiveReceptor sites representing 22 residential dwelling units and one park usingthe FHWA Traffic Noise Modeling (TNM) Version 2.5 for AM and PM Peak hour traffic for Existing Year2018 and Design Year 2038 Build Alternative 2. The TNM predicted traffic noiselevels range from approximately 50 to 65 dBA within the proposed project area with anaverage increase in traffic noise of about 1.5 dBA. None of the identified receptor sites were predicted to experience peak hourtraffic noise levels in excess of the Noise Abatement Criteria (NAC) of 67 dBA for Category B (residences) or CategoryC (e.g. parks, sport areas, playgrounds). In accordance with 23 CFR 772 and ODOT's Noise Manual, and based on correspondence from the ODOT-OES Noise and Air Quality Coordinator dated December 9, 2016, all appropriate noise abatement measures were considered, no noise impacts will occur, and no additional analysis is required.The Noise Analysis Report can be found in the Project File under Noise/Reports/Noise Analysis.pdfThe ODOT-OES correspondence can be found in the Project File under Noise/Coordination/OES Approval_Noise Analysis. pdf
[bookmark: _Toc256000020]Environmental Commitments
	Are there any environmental commitments?
	No
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	Does the project require any Permanent ROW or easement?
	Yes


	ESA Screening Report was completed by District Staff
	No


	Date of ESA Screening IOC from OES:
	01/23/2014


	Do any sites require a Phase 1 ESA, Phase 2 ESA, or plan note according to the IOC from OES?
	Yes


	Site Name
	Address
	Phase 1 Required?
	Phase 2 Required?
	Plan Note Required?

	Kam Wah Restaurant (Site No. 20)
	38 N. River Road, Waterville, OH 43566
	Yes
	Yes
	No

	Waterville Import Services (Site No. 29)
	37 N. River Road, Waterville, OH 43566
	Yes
	Yes
	Yes

	Slaske Building Company (Site No. 47)
	103 N. River Road, Waterville, OH 43566
	Yes
	Yes
	No

	Vacant (industrial land use) (Site No. 53)
	127 N. Second Street, Waterville, OH 43566
	Yes
	No
	No

	Vacant (industrial land use) (Site No. 54)
	125 N. Second Street, Waterville, OH 43566
	Yes
	No
	No

	Vacant (industrial land use) (Site No. 55)
	202 Mechanic Street, Waterville, OH 43566
	Yes
	No
	No

	Roger's Dance Center (former automotive repair) (Site No. 56)
	208 Mechanic Street, Waterville, OH 43566
	Yes
	No
	No

	Digital Dish Offices (former automotive repair) (Site No. 57)
	210 Mechanic Street, Waterville, OH 43566
	Yes
	No
	No

	Valero Filling Station (former filling station) (Site No. 58)
	214 Mechanic Street, Waterville, OH 43566
	Yes
	No
	No

	Allstates Refractory Contractors (industrial land use) (Site No. 60)
	218 Mechanic Street, Waterville, OH 43566
	Yes
	No
	No

	Vacant (former auto body shop in 2000's) (Site No. 61)
	129 N. Second Street, Waterville, OH 43566
	Yes
	No
	No

	Cooper and Mill Race Antiques (former metal drum warehouse) (Site No. 80)
	215 N. Mechanic Street, Waterville, OH 43566
	Yes
	No
	No

	Smedlaps Smithy (former rubber plant) (Site No. 85)
	205 Farnsworth Road, Waterville, OH 43566
	Yes
	No
	No

	Pucci (former rubber plant warehouse) (Site No. 91)
	209 Farnsworth Road, Waterville, OH 43566
	Yes
	No
	No


	 


	Date of Phase 1 ESA IOC from OES:
	02/04/2016


	Date of Phase 2 ESA IOC from OES:
	03/30/2016


	
	


Remarks: 
An Environmental Site Assessment(ESA) Screening Report (December 2013) was performed by the Mannik and Smith Group (MSG). The Screening was prepared in accordance with ODOT's Office ofEnvironmental Services (ODOT-OES) 2009 Guidance.Based on the results of the Screening, in correspondence from ODOT-OES dated January 23,2014, the ESA staff recommended a Phase I ESA be conducted on14 properties. However, based on selection of the preferred alternative and discussions with ODOT at the onset of the detailed design phase, only three (3) sites were recommended for Phase I ESA investigations out of the original 14. Based on the results of the Phase I ESA Report (December 2015) conducted by MSG, in correspondence from ODOT-OES dated February 4, 2016, the ESA staff recommended a Phase II ESA was warranted for three properties. 
Field activities for the Phase II ESAwere completed on February 18, 2016 and the Phase II ESA Report was submittedin March 2016. Based on the results of the Phase II ESAs, no further actions were recommended for the two properties located at 38 N. River Road and 103 N. River Road, and ODOT-OES in an email correspondence on March 30, 2016 agreed with these findings of no further action for these two properties. However, due to theexceedance of the BUSTR Re-Use Action Level at the property located at 37 N. River Road, excavated soil fromthis site should only be spoiled where it can be controlled for non-residentialland use or characterized as a solid waste and properly disposed.  The ODOT-OES email correspondence on March 30, 2016 agreed with this finding for the property at 37 N. River Road, and thus an environmental commitment plan note was developed that states the contractor is required to dispose of any excavated soils as a solid waste in a licensed solid waste landfill, and that the soils from 37 N. River Road cannot be re-used on the project.
· Reports can be found in the Project File under ESA/Reports/Screening.pdf; Phase I.pdf and Phase II.pdf
· The ODOT-OES correspondence can be found in the Project File under ESA/Coordination/OES Recommendations - Screening.pdf and OES Recommendations - Phase I.pdf
	According to the IOC from OES does the project require any Environmental Commitments (plan notes and/or other coordination)?
	Yes


[bookmark: _Toc256000023]Environmental Commitments, ESA
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1. A solid waste management plan note will be included in the plans for 37 North River Road requiring the contractor to dispose of any excavated soils as a solid waste in a licensed solid waste landfill.  The soils from 37 North River Road cannot be re-used on the project. 
[bookmark: _Toc256000024]Cultural Resources
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Please describe all of the efforts made to identify Historic Properties (including lit review, field investigation, etc.): 
A Phase I History/Architecture Report was prepared by the Mannik & Smith Group (MSG) in August 2013. Within a one (1) mile study area, the literature review identified the following: Twelve (12)archaeological sites listed in the Ohio Archaeological Inventory (OAI); 140properties listed in the Ohio Historic Inventory (OHI); five (5) individual propertiesand one (1) historic district listed in the National Register of Historic Places (NRHP), two (2) properties determined eligiblefor NRHP listing, one (1) locally-designated historic district, and three (3) cemeterieslisted in the Ohio Genealogical Society (OGS) files. Three Cultural ResourceManagement (CRM) surveys were conducted within the proposed project area. Theexisting bridge (SFN 8702462) is listedin the ODOT Historic Bridge Inventory, but wasdetermined not eligible for NRHP listing in 2008.
Aboveground investigations were conducted in July andAugust 2013 within the APE (defined by the ODOT-OESCultural Resource Staff as the construction footprint and an area of sufficientgeographical size to include all feasible alternatives and associatedimpacts). Within the APE, abovegroundreconnaissance identified 26 properties over 50 years of age, including 10 OHIsites. Two(2) OHI sites (Columbian House and Morehouse-Downes House) are individually listed in the NRHP and are located within a locally-designatedhistoric district. Field investigations determined OHI site LUC-00882-18is no longer extant. None of the historic properties are located within the APE of the preferred alternative (Alternative 2).


A Phase I Archaeological report was prepared by the Archaeological Staff of ODOT-OES in September 2014. As part of their investigations, OES conducted a literature review and locational survey within the APE that encompassed the three feasible alternatives, but focused mainly on the preferred (Alternative 2). The literature review determined cultural resource investigations were infrequently conducted and that the proposed project area had not been previously surveyed. The literature review did not identify previously known archaeological resources. Various field methods were used to document disturbances and the presence or absence of archaeological remains across the survey area. No prehistoric resources were identified. 
In January 2016, Stage 1 Design Plans were submitted to ODOT District 2, which introduced minor changes to the proposed project footprint. On January 7, 2016, MSG visited the proposed project area to determine if historic properties were present within the expanded project limits. No historic properties were identified and based on the level of ground disturbance, no potential exists for intact archaeological deposits. The results of the field investigations were included in a Phase I History Architecture Addendum that was submitted to ODOT-OES Cultural Resources Staff on January 14, 2016.
· Reports can be found in the Project File under Cultural Resources/Reports/Phase I History Architecture.pdf; Phase I Archaeology.pdf; and Phase I History Architecture Addendum.pdf
	Based on the letter or IOC you received from OES, is there an eligible or listed NRHP Historic Property in the Area of Potential Effects Pursuant to 36 CFR part 800?
	No


	OES/OSHPO Concurrence Date:
	01/05/2015


	
	


Remarks: 
Results of the Phase I History/Architecture and Archaeological Surveys were coordinated with the State Historic Preservation Office (SHPO) on October 27, 2014. In accordance with 36 CFR Part 800.4(d)(1), the Cultural Resources Staff of ODOT-OES determined "No Historic Properties Affected" was the appropriate finding based on the following:Two individually-listed NRHP properties (Columbian House [3 North River Road] and the Morehouse-Downs House [4 South River Road]) are located outside the APE for the preferred alternative. No land from these sites will be required and their contributing features will not be altered or removed by the proposed undertakingPhase II investigations are not required to evaluate the NRHP eligibility of three properties based on their potential as contributing components of a historic district: 23 South River Road (LUC-00851-18); 112 Farnsworth Road (LUC-04638-18); and 128 North River Road (LUC-04639-18). These properties are located outside the APE for the preferred alternative and no impacts to the properties are anticipated.The Waterville Gas & Oil Company building located at 9-11 North River Road (LUC-00838-18) is individually eligible for listing in the NRHP, but is located outside the APE of the preferred alternative, and no impacts to the property are anticipatedNo historic properties of an archaeological nature will be impacted by the proposed project, and no further archaeological investigations are recommended unless an alternative not considered as part of the studies is selected for construction
The SHPO concurred with the recommended finding on January 5, 2015.
Section 106 of the National Historic Preservation Act of 1966 requires federal agencies to consider the effect of their actions on properties listed on or eligible for listing on the NRHP and, to provide the public and consulting parties an opportunity to participate in the Section 106 consultation process. In November 2014, ODOT District 2 sent invitation requests to individuals/groups within the vicinity of the proposed project that demonstrated interest in being a consulting party. Individuals responding via applications to be part of the process included Mr. and Mrs. John and Verna Rose (members of the Waterville Historical Society) and Mr. James Bagdonas (Administrator - City of Waterville). The consulting parties were considered to be a part of the project development process and provided comments.Coordination and concurrence documents can be found in the Project File under Cultural Resources/Coordination/Coordination with SHPO - NHPA.pdf and SHPO Concurrence - NHPA.pdfConsulting Party information can be found in the Project File under Cultural Resources/Project Information/Section 106 Consulting Party Application.pdf and Section 106 Consulting Party Request Acknowledgement
	What is the Section 106 effect determination in the OES letter or IOC?
	No Historic Properties Affected
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	Are there any Environmental Commitments?
	No


	
	 Environmental Document Level: D2
PID 92088 WOO/LUC SR 64 12.03/0.00 Bridge
Approved: June 16, 2016




[bookmark: _Toc256000029]Ecological
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	Has an ESR been completed?
	Yes


	Date ESR was completed:
	05/06/2015


[bookmark: _Toc256000031]Wetlands 
	Are Wetlands Present?
	Yes


	Are Any Wetlands impacted?
	Yes


	Has a Wetland Delineation been made?
	Yes


	Has the wetland Jurisdictional Determination been made?
	Yes


	Wetland ID
	ORAM Category
	Type
	Est Total Size (Acres)
	Est Impact (Acres)

	Wetland A
	2
	Non-Isolated
	0.075
	0.000

	Wetland B
	2
	Non-Isolated
	0.029
	0.000

	Wetland C
	2
	Non-Isolated
	0.012
	0.000

	Wetland D
	2
	Non-Isolated
	0.099
	0.062

	Wetland E
	2
	Non-Isolated
	0.237
	0.072

	Wetland F
	3
	Non-Isolated
	1.945
	0.263

	Wetland G
	3
	Non-Isolated
	0.500
	0.030

	Wetland H
	2
	Non-Isolated
	0.030
	0.000

	Wetland I
	2
	Non-Isolated
	0.026
	0.000


	 


	Est. Total Size (Acres) of for Project
	2.953


	Est. Total Impacted (Acres) of for Project
	0.427


	Total Acres of Non-Isolated Wetlands impacted
	0.427


	Total Acres of Isolated Wetlands impacted
	0


	
	


Remarks: 
A Level 2 EcologicalSurvey Report (ESR) dated May 6, 2015, was prepared by the Mannik & Smith Group, based on field investigations conducted in May and June 2013, and December2014. The report identified nine non-isolated wetlands within theproposed project area. The wetland impact acreages from the table above reflect totals based on the Stage 1 Plans and the alignment/construction footprint of the proposed project. A total of 2.953 acres of Category 2 (moderate quality) and Category 3 (high quality) wetlands were identified in the proposed project area. Construction of the new bridge will result in permanent impacts to 0.4277 acres of wetlands, of which 0.2933 acres is Category 3 wetland impacts. These impacts have been reduced preferred alternative since the original Level 2 ESR was conducted based on modifications to the proposed project design plans.

The Level 2 ESR can be found in the Project File under Ecological/Reports/Level 2 Ecological Survey.pdf
[bookmark: _Toc256000032]Streams & Rivers 
	
	Present
	Impacted

	Streams and Rivers:
	Yes
	Yes

	National Scenic River:
	No
	

	State Scenic River:
	Yes
	Yes

	Sec 9:
	No
	

	Sec 10:
	Yes
	Yes


	 


	Stream Name
	Total Linear feet Impacted
	QHEI
	Aquatic Life Use Designation

	Maumee River
	75
	74
	Warm Water Habitat (WWH) 


	 


	Total Linear feet Impacted
	75


	
	


Remarks: 
Based on the results of the Level 2 ESR, the Maumee River (a State Scenic River) is located in the proposed projectarea, and no other streams or waterways wereidentified. The proposed project will permanently impactapproximately 75 feet of the Maumee River to accommodate placement ofbridge piers and Rock Channel Protection (RCP). The Maumee River is a Section10 waterway, which is protected by the Rivers and Harbors Act of 1899 toregulate the placement of any material in navigable waters of the United States.The impacts are anticipated to consist of excavation of streambedmaterials (although the proposed project area is bedrock with only a smallamount of cobble), placement of fill materials within the stream channel of theriver, and placement of materials on the river banks to prepare for demolitionof the existing bridge and construction of the replacement bridge. Theplacement of fill material will likely consist of rock channel protection, andother various clean non-erodible fill materials necessary for the constructionof temporary work pads, support abutments, and stream bank protection in thevicinity of construction activities.
[bookmark: _Toc256000033]Other Surface Waters 
	
	Present
	

	Reservoirs:
	No
	

	Lakes:
	No
	

	Ponds:
	No
	

	Storm Water Management Facility:
	No
	

	Jurisdictional Ditch:
	No
	

	Other (If selected please explain in remarks):
	No
	


	 


	
	


Remarks: 
Based on the results of the Level 2 ESR, no other surface waters were identified within the proposed project area.
[bookmark: _Toc256000034]Terrestrial Habitat 
	
	Present
	Impacted

	Terrestrial Habitat:
	Yes
	Yes

	Unique or high Quality:
	Yes
	Yes


	 


	Please Check All types of Unique or high Quality Terrestrial habitat that are present:
	Any other habitat that has a prevalence of state or federally listed species. ¿ 


	
	


Remarks: 
Based on the results of the Level 2 ESR, terrestrial habitat in the proposed project areaconsists of vegetative communities that experience low to high levels ofdisturbance. The following vegetative communities and land cover were identified within the proposed project area: Open Water, Cultivated Crops, Developed Open Space, Developed Low Intensity, Developed Medium Intensity, Floodplain Forest and Herbaceous Riverine Community. Impacts are expected to occur within two high quality vegetative communities (open water and herbaceous riverine community). 
[bookmark: _Toc256000035]Threatened or Endangered Species 
	
	Present
	Impacted

	Within the known range of a Federal Species?
	Yes
	No

	Federal Species/habitat found within the project area? 
	Yes
	Yes

	Within the known range of a State Species? 
	Yes
	No

	State Species/habitat found within the project area? 
	Yes
	Yes


	 


	
	


Remarks: 
All threatened and endangered species surveys were conducted in accordance with the Endangered Species Act of 1973 (ESA). The purposes of the ESA are to protect federally endangered and threatened species and to provide a means to conserve their habitats. The Act requires that all federal agencies protect species and preserve their habitats. The law is administered by the USFWS and the National Marine Fisheries Services.
The proposed project is withinthe known range of ten (10) federally listed species and two (2) state listedspecies were observed within or known to be within one mile ofthe proposed project area. 
The proposed project is within theknown summer breeding range of the federally endangered Indiana Bat (Myotis sodalis) and federally threatenednorthern long-eared bat (Myotisseptentrionalis). Five trees possessing potentially suitable roostinghabitat (PRT) for each species will be removed. 
In addition to the Indianaand northern long-eared bat, the proposed project lies within the known range of Kirtland'swarbler (Setophaga kirtlandii),piping plover (Charadrius melodus),karner blue butterfly (Lycaeides Melissasamuelis), rayed bean mussel (Villosafabalis), all federally endangered species; eastern prairie fringed orchid(Platanthera leucophaea) and rufa redknot (Calidris canutus rufa), bothfederally threatened species; eastern massasauga (Sistrurus catenaus), a federal candidate species; and bald eagle (Haliaeetus leucocephalus), a federalspecies of concern protected under the Bald and Golden Eagle Protection Act andMigratory Bird Treaty Act. ODOT has determined the proposed project will have no effect on the aforementioned species. Therefore, consultation under section 7(a) (2) of the Endangered Species Act is not required.
Review of ODNR's Ohio NaturalHeritage Database revealed the eastern cricket frog (Acris crepitans), a state species of concern, was identified withinone mile of the proposed project area. Suitable habitat for the easterncricket frog consists of shores of vegetated permanent pools and streams. Basedon the results of field investigations, suitablehabitat exists within the proposed project area, however, this species was not observed. Dueto the small area of impact to the shoreline of the Maumee River, the proposed projectwill have minimal or no impact on this species.
Based on results of the Level 2 ESR, the threehorn wartyback (Obliquaria reflexa) was identified within the proposed projectarea. Based on email correspondence with ODOT-OES dated January 19, 2016, a mussel survey is not required as the portion of the Maumee River within the proposed project area is bedrock with a small amount of cobble (not suitable mussel habitat).
· OES correspondence regarding a mussel survey can be found in the  Project File under Ecological/Coordination/OES Approval_No Mussel Survey Required.pdf
[bookmark: _Toc256000036]Agency Coordination 
	
	Coordination Required
	Comments Received Date

	Ohio Department of Natural Resources (ODNR):
	Yes
	02/27/2015

	United States Fish and Wildlife Service (USFWS):
	Yes
	02/04/2015

	Ohio Environmental Protection Agency (OEPA):
	Yes
	04/22/2015

	United States Army Corps of Engineers (USACE):
	Yes
	07/30/2015

	ODNR State Scenic River:
	Yes
	02/09/2015

	National Park Service (NPS) National Scenic River:
	No
	


	 


	
	


Remarks: 
Based on coordination with the US Fish and Wildlife Service (USFWS) and ODNR, specific comments regarding wetland and stream impacts were not provided by either agency. 
USFWS recommended that unavoidable impacts to streamsand other important habitats be mitigated. In addition, staging areas should bekept well away from streams and all disturbed areas in the project vicinityshould be mulched and re-vegetated with native plant species. USFWS concurswith ODOT that the proposed project mayaffect but is not likely to adversely affect the Indiana bat and northernlong-eared bat. All tree clearing for this project must be conducted onlybetween October 1 and March 31. In addition, the project will have no effect on the Kirtland's warbler (Setophaga kirtlandii), piping plover (Charadrius melodus), karner bluebutterfly (Lycaeides Melissa samuelis),rayed bean mussel (Villosa fabalis),eastern prairie fringed orchid (Platantheraleucophaea), rufa red knot (Calidriscanutus rufa), eastern massasauga (Sistruruscatenaus) and bald eagle (Haliaeetusleucocephalus).
Comments  from ODNR Scenic Rivers have been received and are included in the Ecological section of the Project File.  ODOT has committed to work with ODNR Scenic Rivers to address their commentsand concerns to the satisfaction of both agencies, and develop plan notesand/or special provisions to assure Scenic River's concerns are adequatelyimplemented.  ODOT will receive approval form the Director ofODNR  in accordance with ORC, Section1547.82 prior to construction.
An approved jurisdictional determination was issued bythe USACE on July 30, 2015. It was determined that Wetlands A through I areadjacent to the Maumee River. Therefore, Wetlands A through I within theproject construction limits are subject to regulation under Section 404 of theClean Water Act. 
USACE recommends the number of in-stream piers bereduced to the lowest number technically feasible to minimize potential adverseeffects on navigation and aquatic resources.
Division of Wildlife recommended habitat avoidance dates for the habitats listed in the table below. None of these habitats are found in the project construction limits as noted in the table, thus no environmental commitment notes are needed for avoiding these dates during construction.
ODNR Division of Wildlife also indicate the project is within the range of the western banded killifish (Fundulus diaphananus menona), a state endangered fish. The DOW recommends no in-water work in perennial streams from April 15 to June 30 to reduce impacts to indigenous aquatic species and their habitat.
	Are there any environmental commitments?
	Yes


[bookmark: _Toc256000037]Environmental Commitments, Agency Coordination 

1. ODOT shall work with ODNR Scenic Rivers to address their comments and concerns to the satisfaction of both agencies, and develop plan notes and/or special provisions to assure Scenic River's concerns are adequately implemented.  In accordance with ORC Section 1547.82, ODOT must receive approval form the Director of ODNR prior to the start of construction.
2. No in-water work shall occur from April 15 to June 30 to reduce impacts to indigenous aquatic species and their habitat, including the western banded killifish (Fundulus diaphananus menona), a state endangered fish. 
3. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet.   
4. The contractor shall notify the U.S. Coast Guard (USCG) Ninth District at least 30 days prior to the start of construction. Contact info: Scot Striffler, Bridge Project Manager, Ninth Coast Guard District PH: (216) 902-6087 FAX: (216) 902-6088 Scot.M.Striffler@USGS.MIL
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5. ODOT shall provide documentation required by the U.S. Coast Guard (USCG) once the bridge replacement is completed. Complete drawings are not required but a single page showing an overhead and side view of the bridge with clearance information from International Great Lakes Datum 1985/Low Water Datum (IGLD85/LWD) would be adequate for documentation for the USCG.
[bookmark: _Toc256000038]Other Resources
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	The proposed project is located within an Urbanized Area
	No


	The proposed project is located within a Non-Urbanized Area
	Yes


	The proposed project involves new permanent right-of-way (ROW)
	Yes


	The proposed project involves temporary ROW
	Yes


	The proposed project is a type of action listed below and meets allowable ROW thresholds: 
· Bridge replacement requiring ROW of three (3) acres or less to accommodate bridge piers, wingwalls, and/or approach work
· Widening requiring linear strip ROW of 10 acres or less per linear mile
· Intersection improvement requiring ROW of three (3) acres or less

	Yes


	Undeveloped land being used for construction purposes is protected by a conservation easement
	No


	Undeveloped land being used for temporary ROW will be returned to equal or greater productive capability upon completion of the proposed project
	Yes


	Based on the scope and type of work, the proposed project is in compliance with the executed Farmland Memorandum of Understanding (MOU), the FPPA, and 7 CFR 658. Completion of the Farmland Conversion Impact Rating (FCIR) Form is not warranted. No further coordination is required.
	


	OES Concurrence Date
	03/24/2016


	NRCS Approval Date
	03/24/2016


	Land being used for the proposed project is part of an Agricultural District
	No


	
	


Remarks: 
The proposed project islocated in a non-urbanized area.  Based upon review of the USDA Urban-Built Up Area Soils Maps, prime farmland is located on the eastern portion of the proposed project area.  Two parcels in this portion that will require right-of-way acquisition are 54.22 acres and 201.74 acres in size. However, the total amount of right-of-way (0.4728 acres) from both parcels (0.2496 from the 54.22 acre parcel and 0.2232 from the 201.74 acre parcel) does not exceed the conditions of the Farmland Memorandum of Understanding (MOU) between the NRCS and ODOT.  Furthermore, the proposed project is notlocated in an agricultural district and the acres do not exceed the regulations listed in Ohio Revised Code (ORC) 929.05. Based on the scope and type of the proposedproject, along with the amount of right-of-way needed, the proposed projectmeets the criteria/conditions the MOU executed on 3/15/2016.  No further coordinationis required. 
· Farmland and Census mapping can be found in the Project File under Other Resources/Farmlands/US Census Urbanized Area Map.pdf and USDA Urban-Built Up Area Soils Map.pdf


	Are there any environmental commitments?
	No


[bookmark: _Toc256000040]Drinking Water
	The proposed project is wholly or partially located within the USEPA designated boundaries of a Sole Source Aquifer
	No


	
	Present
	

	The proposed project is wholly or partially located within the OEPA designated boundaries of a Source Water Protection Area
	No
	


	 


	Coordination with the Local Public Water Administrator is required
	No


	
	Present
	

	Residential Wells are present
	No
	


	 


	
	


Remarks: 
A review of drinking water resourceprotection areas from OEPA and of drinking water wells from ODNR Division of Soil and Water Resources revealed no known drinking water source areas locatedwithin the proposed project limits in Lucas and Wood Counties. The literature and mapping reviewed for drinking water resources for this CE document are provided as reference material attachments located at Project File/OtherResources/Drinking Water.
No additional research or coordination is required as there are no drinking water sources within the project limits.
	Are there any environmental commitments?
	No
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[bookmark: _Toc256000041]Section 4(f)[bookmark: _Toc256000042]Section 4(f) Determination
	Section 4(f) properties are within and/or adjacent to the proposed project area
	Yes


	Concurrence received from the OWJ
	Yes


	Were there multiple OWJs?
	Yes


	Name
	Date concurrence received

	City of Waterville
	02/23/2016

	Ohio Department of Natural Resources (ODNR) Scenic Rivers
	04/05/2016


	 


	
	Present
	Impacted

	Publicly owned Park(s):
	Yes
	Yes

	Publicly owned recreation facility(ies) and/or area(s):
	Yes
	Yes

	Wildlife and Waterfowl refuge(s):
	No
	

	Historic Site(s):
	Yes
	No


	 


[bookmark: _Toc256000043]Identified Section 4(f) Properties
	Property Name
	Type
	Permanent ROW/Easement Acres
	Temporary ROW/Easement  Acres
	4(f) finding
	Date

	Memorial Park
	Publicly owned Park
	0.307
	0.540
	Net Benefit
	06/01/2016

	Maumee River
	Publicly owned Recreational Facility and/or Area
	NA
	NA
	No Use
	04/05/2016

	Former Waterville Public School Property (Planned Park)
	Publicly owned Park
	0
	1.876
	Net Benefit
	06/01/2016

	Columbian House (3 North River Road)
	Historic Site
	N/A
	N/A
	No Use
	01/05/2016

	Morehouse-Downs House (4 South River Rd)
	Historic Site
	N/A
	N/A
	No Use
	01/05/2016

	Waterville Gas & Oil Co. (9-11 North River Rd)
	Historic Site
	N/A
	N/A
	No Use
	01/05/2016


	 


	
	


Remarks: 
Three recreational properties were identified within the proposed project area:
Maumee River
The designated State Scenic River is administered and maintained by the Ohio Department of Natural Resources (ODNR) and provides recreational opportunities, such as canoeing, kayaking and fishing. No permanent restrictions to recreational activities that occur on or along the Maumee River within the proposed project area are anticipated. Temporary impacts include limiting small watercraft access and existing egress/ingress access at Memorial Park for safety purposes during certain stages of construction. Recreational activities that require ingress/egress access will be diverted to Waterworks Park (which has a boat ramp and parking), located approximately 0.5-mile upstream. Although navigational closures of the Maumee River are not anticipated, a temporary work pad/causeway will be placed in the waterway to facilitate construction activities. Based on the scope of the proposed project and type of work, there will be no adverse effects to the protected recreational activities, features, or attributes associated with the Maumee River. 
Memorial Park

The park is owned and maintained by the City of Waterville and provides passive amenities, such as a memorial stone, grill, birdhouse, pet and concrete trash receptacles, and four benches. These park features will be removed to a safe storage location during construction activities and reinstalled upon completion of the proposed project. The park will be closed to public access for the duration of construction activities to facilitate construction equipment movement, provide direct access to the river, and to protect the public. Permanent (0.3072 acres) and temporary right-of-way (0.54 acres) impacts will be required, which includes existing public road right-of-way (Water Street) along the west side of the park. The permanent right-of-way will be required from along the north side of the park adjacent to the existing bridge and Mechanic Street. The temporary right-of-way is needed for the duration of construction in order to provide a staging and storage area for construction equipment and direct access to the Maumee River to launch the in-stream work pad. 
Former Waterville Public School Property
The property is owned and maintained by the City of Waterville and is identified as a planned park in the city's 2006 Downtown Revitalization Plan and 2012 Comprehensive Plan to enhance access to the Maumee River and return the property to its original function as a public square. A portion of the property was re-zoned from the east wall of the school building to the river as the Parks & Green Space District in 2014. The existing property comprises 1.876 acres, of which the north side of the property currently functions as public road right-of-way. Although not originally platted as public right-of-way, it is owned and maintained by the city. To facilitate construction activities, the property will be used as a staging and storage area for construction equipment. 
As part of previous and on-going project development, ODOT and the City of Waterville partnered to ensure the proposed project design complements existing and planned recreational activities. Furthermore, the proposed project will assist in the implementation of the City of Waterville's revitalization plans. Based upon the measures to minimize harm and assessment of impacts, the proposed project will result in a "Net Benefit" by enhancing recreational opportunities through the merger of Memorial Park and the former Waterville School Property, and providing better access to river recreation and better connect to existing and planned walkways/trails. 
Historic Sites
Results of the Phase I History/Architecture and Archaeological Surveys were coordinated with the State Historic Preservation Office (SHPO) on October 27, 2014. In accordance with 36 CFR Part 800.4(d)(1), the Cultural Resources Staff of ODOT-OES determined "No Historic Properties Affected" was the appropriate finding based on the following:Two individually-listed NRHP properties (Columbian House [3 North River Road] and the Morehouse-Downs House [4 South River Road]) are located outside the APE for the preferred alternative. No land from these sites will be required and their contributing features will not be altered or removed by the proposed undertakingThe Waterville Gas & Oil Company building located at 9-11 North River Road (LUC-00838-18) is individually eligible for listing in the NRHP, but is located outside the APE of the preferred alternative, and no impacts to the property are anticipated


	Are there any environmental commitments?
	Yes


[bookmark: _Toc256000044]Environmental Commitments, Identified Section 4(f) Properties

1. The contractor will be required to closely coordinate the construction schedule with ODOT, the ODNR Scenic River coordinator, ODNR Parks and Recreation, and the City of Waterville.  Christina Kuchle, Northwest Region-Scenic River Manager, office: (419) 429-8306, mobile: (419) 348-5073, Christina.kuchle@dnr.state.oh.us and the City of Waterville contact is James Bagdonas, Municipal Administrator, office: (419) 878-8100, jbagdonas@waterville.org and the ODOT District Environmental coordinator is Stacy Schimmoeller office: (419) 373-4319 or stacy.schimmoeller@dot.ohio.gov. The ODNR Division of Parks and Recreation contact person is Gary Obermiller at 614-265-6561 or ohiostateparks@dnr.state.oh.us

The contractor will notify ODOT, ODNR Scenic River coordinator, ODNR Parks and Recreation section, and City of Waterville 18 days prior to beginning construction so that the public can be informed 15 days prior to construction.
2. For watercraft safety, the contractor will coordinate with ODNR Division of Watercraft the installation of the appropriate warning signs and buoys in the water directing hand-powered watercraft to Waterworks Park, upstream of Memorial Park. The ODNR Division of Watercraft contact person is Chad German at 419-836-6003 or maumeebay.watercraft@dnr.state.oh.us 
3. Advance notice of the project's construction schedule and potential for users to encounter partial closures at the bridge (for the causeway and demolition) will be provided by the contractor no less than 48 hours prior to construction activities.  Notices shall be posted in an area that can be seen by users of the Maumee River, both upstream and downstream, and on the ODNR and ODOT website.

The contractor shall notify the ODOT District Environmental coordinator Stacy Schimmoeller at (419) 373-4319 or stacy.schimmoeller@dot.ohio.gov.; the ODNR Northwest Region-Scenic River Manager Christina Kuchle at (419) 429-8306 or mobile (419) 348-5073 or Christina.kuchle@dnr.state.oh.us; the City of Waterville administrator James Bagdonas at (419) 878-8100 or jbagdonas@waterville.org; and the ODNR Division of Parks and Recreation Chief Gary Obermiller at 614-265-6561 or ohiostateparks@dnr.state.oh.us

4. ODOT, the contractor, and the City of Waterville will cooperate prior to construction to remove for safekeeping the existing benches, memorial stone, grill, birdhouse, mutt receptacle, concrete trash receptacle, and flag pole associated with Memorial Park.  These items shall be reinstalled following completion of construction in a manner as good or better than which they existed prior to construction. 
5. All areas of Memorial Park disturbed by construction activities will be restored to a condition at least as good as or better than that which existed prior to the proposed project.
6. ODOT and the City of Waterville will coordinate for the demolition of the former Waterville Public School building prior to start of construction activities.
7. Following completion of construction, ODOT and the City of Waterville will coordinate to ensure, the former Waterville Public School property will be integrated with Memorial Park.
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8. Fencing will be installed around Memorial Park and the former Waterville Public School property, except for the boundary along the river.  This fencing can be the same fencing used to secure the equipment and materials as needed, so long as it is along the property boundary.
[bookmark: _Toc256000045]Section 6(f)
[bookmark: _Toc256000046]Section 6(f) Determination	
	Present
	

	6(f) Properties:
	No
	


	 


	
	


Remarks: 
The proposed project will not impact existing properties that received Land and Water Conservation Funds. Review of the LWCF Grant Listing did not indicate existing properties received LWCF Funds. Therefore, no further Section 6(f) coordination is required.
	Are there any environmental commitments?
	No
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[bookmark: _Toc256000047]Community Impacts
[bookmark: _Toc256000048]Community Impacts
	Will the proposed action comply with the local/regional development patterns for the area?
	Yes


	
	


Remarks: 
The proposed project, as planned, is designed to comply with local comprehensive plans and development patterns within the region. The proposed bridge will provide a pedestrian/bike facility which complies with both the City of Waterville Comprehensive Plan and the TMACOG 2045 Long Range Regional Transportation Plan for non-motorized projects. 
· The Waterville Comprehensive Plan can be found in the Project File under General/PDP/Transportation Plan or Visioning Documents.pdf
· The Regional Transportation Plan and the City of Waterville's Zoning Map can be found in the Project File under Community Impacts/Project Information/Regional Development Plan.pdf and Existing Land Use or Zoning Map.pdf
	Will the proposed action result in substantial negative impacts to community cohesion?
	No


	
	


Remarks: 
The proposed project will enhance community cohesion by providing a pedestrian/bike facility across the Maumee River to provide better access and improve safety for motorized and non-motorized traffic. Providing a pedestrian/bike facility complies with the City of Waterville Comprehensive Plan and TMACOG's Regional 2045 Long Range Transportation Plan as the SR 64 corridor is a designated non-motorized project that will provide connectivity to several bike routes in the region. Furthermore, the former Waterville Public School property is designated as a future parks & green space in the Comprehensive Plan. The demolition of the former elementary school as part of this project will provide a first step desired by the community to clear the site for future park area development once the bridge construction project is completed. 
	Will the proposed action result in indirect or cumulative impacts?
	No


	
	


Remarks: 
The proposed bridge will be constructed on essentially existing alignment, and no additional development is anticipated to occur as a result of the proposed project. The proposed project is not anticipated to result in negative cumulative impacts on the local or regional land use patterns. The proposed project will in fact provide compliance to the local and regional plans. In addition, the removal of the vacant elementary school will assist the City of Waterville in developing the former school site into a park & green space area once the construction of the bridge is completed. The provision of a safe and efficient pedestrian/bike facility on the new bridge will provide opportunities for increased non-motorized traffic which will reduce vehicle trips and thereby provided positive cumulative environmental impacts by reducing emissions, fuel consumption, and congestion.
	Will the proposed action result in substantial impacts on health and educational facilities, public utilities, fire, police, emergency services, religious institutions, public transportation, pedestrian and bicycle facilities?
	No


	
	


Remarks: 
No substantial impacts are anticipated, as the current bridge will remain open during the majority of construction period of the new bridge so that traffic, utilities, school traffic, pedestrian/bike traffic, emergency services, religious institutions, and police services can be maintained during the construction to allow for minimal impacts on the community. Once the new bridge is open and operational, the enhance river crossing will provide positive benefits to the health of the community by providing a new pedestrian/bike facility across the river; provide safe & efficient travel on a bridge constructed to current design standards; and provide more efficient intersections that will reduce congestion and improve traffic flow.
	Will the proposed action displace residents, businesses, institutions or farms?
	Yes


Number of Displacements
	Residences:
	1


	Businesses:
	1


	Institutions:
	0


	Farms:
	0


	
	


Remarks: 
The proposed project will displace one business and one residential property on the City of Waterville side where the re-aligned approach to the proposed bridge will be constructed from the intersection of North River Road and SR 64. No existing institutions or farms will be displaced. The Ohio Department of Transportation (ODOT) has been and will continue to be in discussions with the business and residential property owner to assist in coordinating project impacts.
	Are there any Environmental Commitments?
	No
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[bookmark: _Toc256000049]Environmental Justice
[bookmark: _Toc256000050]Environmental Justice
	Census Block Group #
	% Minority
	% Low Income

	390950089021
	4.36
	0.00

	390950089022
	23.69
	1.24

	391730212001
	10.54
	1.55


	 


	Are there block groups that have minority and/or low-income populations that are equal to or greater than 40%?
	No


	
	


Remarks: 
The USEPA EJView on-line tool was utilized to obtain minority and low-income population percentages within the proposed project area. The proposed project area is located in three (3) CensusBlock Groups. The minority populations range from 4.36% to 23.69% and low-income populations range from 0% to 1.55.
The proposed project will haveno disproportionately high and adverse impacts to minority or low-income populationsbased upon census mapping.  No EnvironmentalJustice issues were raised as a result of public involvement activitiesconducted as part of the proposed project. Therefore, in accordance with the protections of Executive Order 12898and FHWA Order 6640.23A, no further Environmental Justice analysis isrequired.  


	Are there any Environmental Commitments?
	No
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[bookmark: _Toc256000051]Public Involvement
[bookmark: _Toc256000052]Public Involvement
	
	


Please provide a summary of the Public Involvement activities that have been conducted for this project. (For example press releases, letters to affected property owners and residents, meetings, special purpose meetings, newspaper articles, etc) 
On Monday March 10, 2014, ODOT sent a public notification (Press Release) for the public meeting to be held Thursday March 27, 2014.  Additionally, notifications were sent to property owners, residents, businesses, and public officials. The public meeting notification was also posted on the ODOT and City of Waterville web page.
On Friday March 14, 2014, the Sentinel-Tribune posted an article regarding the public meeting.
On March 27, 2014, WTVG Channel 13 News provided information about the public meeting online as well as through a newscast.
On March 27, 2014, WTOL Channel 11 News provided an online story of the public meeting and how to provide comments on the project.
On March 27, 2014, a public meeting was held at the Waterville Primary School at 457 Sycamore Lane in Waterville, to provide project information and solicit public input. A total of 233 attendees signed into the meeting. A total of 141 comment sheets were submitted over the two-week comment period from March 27 to April 10, 2014.
On March 28, 2014, The Blade posted an article regarding the public meeting.
On March 28, 2014, the Sentinel-Tribune posted an article regarding the public meeting.
· All public involvement documentation can be found in the project file under Public Involvement/Project Information
	Was Public Involvement conducted in compliance with Title VI requirements?
	Yes


	Is there any substantial environmental controversy on environmental grounds?
	No


	
	


Please summarize the Public Involvement responses received. 
A review of the sign-in sheets from the meeting reveals that a total of 233 officially signed into the meeting, however a visual assessment of the meeting seems to indicate there were more in attendance. A total of 141 comment sheets were submitted over the two-week period from March 27 to April 10, 2014. A summary of the comments submitted is provided in tabular form herein, as well as a copy of each original comment sheet that was submitted. The tabular summary of comments also contains a column of data regarding how responses to each comment submitted were handled (ODOT provided responses to comments). A pie chart located on page 1 of the Executive Summary of the Public Meeting Summary Document (located in the Project File at Public Involvement/Project Information/Public Meeting Summary.pdf) provides a summary of which alternatives were mentioned in the comments, which shows a total of 43% desired either Alt. 1/Alt. 1 or 2/Alt. 2; and 39% listed Alt. 2 or 3/Alt. 3.
Several of the more common comments made on the comment sheets included the following:
· Concerns about extended period of river crossing closure and long detour involved
· Impacts to historic buildings if Alt-3 selected due to increased truck traffic on Farnsworth Rd.
· Desire to use old school property as future park/community square instead of a bridge
· Several comments on whether or not existing bridge even needs replaced yet
· Issues raised about roundabout and if it could accommodate very large farm equipment
· Concerns that roundabout would be confusing to drivers
· Long detour would negatively impact Anthony Wayne School District transportation
· Alt-3 would divide Waterville in half since Farnsworth Rd. would be heavy traffic
· Several comments Alt-3 would benefit businesses since more visible to traffic
· Desire to make bridge aesthetic with Waterville themes
· Desire that bridge allows for good view of river while driving on it
ODOT provided feedback to all comments received if the commenter provided contact information. A summary of the responses provided by ODOT to commenters included:
· The commenter was thanked for submitting comments on the project
· A link was provided on an FHWA video on how roundabouts operate
· Indicated that the design phase of the project will try to incorporate comments and suggestions into the design as much as possible
· Provided contact information for ODOT if commenter had further questions on the project
· Discussed roundabout concerns regarding trucks and farm machinery passing through a roundabout for those that asked about this subject
· Discussed the reasons why ODOT is replacing the bridge for those commenters that inquired why it needed replaced
· Discussed the sidewalk and multi-use path (bike facility) that would be part of a new bridge for those than inquired about the facility'
· Provided explanation on the cost of the new bridge for those that inquired
· Explained why a roundabout was recommended instead of an all-way stop and the benefits such provides in way of safety and efficiency
All public involvement documentation can be found in the Project File under Public Involvement/Project Information
	Are there any Environmental Commitments?
	No
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[bookmark: _Toc256000053]Permits
[bookmark: _Toc256000054]Waterway Permits
	Are Waterway Permits required?
	Yes


	Is the Waterway Permits Determination Complete?
	Yes


Army Corps of Engineers
	Regional General Permit (RGP):
	Yes


	Nationwide Permit (NWP):
	Yes


	Section 404 Individual Permit:
	No


	Section 10 Permit:
	No


Ohio EPA
	Section 401 Water Quality Certification:
	Yes


	Level 1 General Isolated Wetland Permit:
	No


	Level 2 Individual Isolated Wetland Permit:
	No


	Level 3 individual Isolated Wetland Permit:
	No


US Coast Guard
	Section 9 Coordination:
	Yes


	Section 9 Bridge Permit:
	No


ODNR
	Shore Structure Permit :
	No


	
	


Remarks: 
A Section 404 Regional General Permit (RGP) PCN (Pre Construction Notification) and Individual Section 401 OEPA Water Quality Certification arerequired. ODOT is coordinating obtaining all permits prior to construction. Final mitigation for impacts to the Maumee River andwetlands has not been determined yet, but the final mitigation plan will needto be approved by agencies prior to construction.
ODOT submitted a PCN for geotechnical drilling in the Maumee River and received a Section 404 NWP (Nationwide Permit) #6 on November 12, 2015.  ODOT also submitted a Scenic River Field Review Form to ODNR Scenic Rivers for coordination on the project.  Coordination was received from ODNR Scenic Rivers and the project was given waiver to drill in river after 10/31/15. The drilling took place in December 2015, and the USACE completion of activity form was signed and dated 1-25-2016 and returned to the ODOT District Environmental Coordinator.
ODOT-OES Permit Determination was received on2/26/16.  The project will result in 75linear feet of permanent impacts to  the Maumee River and 0.3254 acres of permanentimpacts to wetlands.  There will be0.2933 acres of permanent impact to Category 3 wetlands.  Mitigation for stream and wetland impacts hasyet to be determined by ODOT.  It islikely they will use a "pooled mitigation site" for the river impacts.  Impacts to Category 2 wetlands will likely bemitigated by purchasing credits at a wetland mitigation bank that serves thiswatershed.  ODOT is currently exploringoptions on where impacts to Category 3 wetlands can be mitigated.


	Are there any environmental commitments?
	Yes


[bookmark: _Toc256000055]Environmental Commitments, Waterway Permits

1. The project requires a waterway permit for work within wetlands and the Maumee River which shall be attached to the plans as Special Provisions. No work within wetlands and/or below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by ODOT. All conditions of the permit shall be followed throughout construction by the contractor. 

[bookmark: _Toc256000056]Storm Water Permits
	NPDES Construction General Permit for Stormwater (NOI):
	Yes


	Watershed Specific NPDES Construction General Permit for Stormwater (NOI):
	Yes


	
	


Remarks: 
The proposed project will require a National Pollutant Discharge EliminationSystem (NPDES) permit since the earth disturbed area is greater than one acre.  An NOI will be submitted by ODOT to the OEPA priorto plan file.  In accordance with ODOT Supplemental Specification 832, aStorm Water Pollution Prevention Plan (SWPPP) and an Erosion Control Plan will be developed by thecontractor and a NPDES permit will be finalized/acquired by the contractorprior starting any earth disturbing construction activities.
	Are there any environmental commitments?
	Yes


[bookmark: _Toc256000057]Environmental Commitments, Storm Water Permits

1. ODOT and the contractor shall ensure that an National Pollution Discharge Elimination System (NPDES) permit shall be acquired prior to the start of construction. 
[bookmark: _Toc256000058]Floodplains
	The proposed project involves encroachment within a Special Flood Hazard Area (SFHA)
	Yes


	EO 11988/NFIP Coordination and Documentation Completed
	No


	NFIP Local Floodplain Coordinator Notification Date
	01/14/2016


	
	


Remarks: 
Following a review of the current FEMA Flood Insurance Rate Maps (FIRM) by The Mannik & Smith Group, Inc., the proposed project area is partially located in aregulated floodplain based on the following panels:Lucas County Panel #:39095C0240ELucas County Panel #:39095C0405EWood County Panel #:39173C0150DWood County Panel #:39173C0015D
Coordination with the Local Floodplain Administrators was initiated for the proposed project on 1-14-2016, and will continue during the design process as detailed plans progress. The City of Waterville floodplain coordinator indicated all the city standards mirror the Federal standards and no coordination is needed as long as those standards are followed. The Lucas County flood plain coordinator indicated they do not have jurisdiction over the bridge and deferred to City of Waterville. The Wood County flood plain coordinator provided their standards (which have been uploaded as an attachment to this CE document), and if there are further questions feel free to contact them.The panels can be found in the project file under Permits/Floodplains/FEMA FIRM.pdf All correspondence can be found in the project file under Permits/Floodplains/Correspondence with Local Floodplain Administrator and Local Floodplain Administrator Response.pdf 
	Are there any environmental commitments?
	Yes


[bookmark: _Toc256000059]Environmental Commitments, Floodplains

1. If required, ODOT shall ensure that a floodplain permit is acquired prior to construction.  
[bookmark: _Toc256000060]Landfills
	Is a 2713 Permit required?
	No


	
	


Remarks: 
The proposed project will not have any impact on regulated land fills, and will not require any permits.
	Are there any environmental commitments?
	No
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[bookmark: _Toc256000061]Environmental Commitments
[bookmark: _Toc256000062]General, Maintenance of Traffic During Construction
Commitments
1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Meetings will be held with the City of Waterville, Wood County, ODOT, and the project team following the completion of Stage 2 plans and MOT plans to confirm impacts and notify appropriate public services and facilities prior to the start of construction. 
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.  This includes the annual Roche de Boeuf Parade and Festival that occurs typically on the last Saturday in September.
[bookmark: _Toc256000063]ESA
Commitments
1. A solid waste management plan note will be included in the plans for 37 North River Road requiring the contractor to dispose of any excavated soils as a solid waste in a licensed solid waste landfill.  The soils from 37 North River Road cannot be re-used on the project. 
[bookmark: _Toc256000064]Ecological, Agency Coordination 
Commitments
1. ODOT shall work with ODNR Scenic Rivers to address their comments and concerns to the satisfaction of both agencies, and develop plan notes and/or special provisions to assure Scenic River's concerns are adequately implemented.  In accordance with ORC Section 1547.82, ODOT must receive approval form the Director of ODNR prior to the start of construction.
2. No in-water work shall occur from April 15 to June 30 to reduce impacts to indigenous aquatic species and their habitat, including the western banded killifish (Fundulus diaphananus menona), a state endangered fish. 
3. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet.   
4. The contractor shall notify the U.S. Coast Guard (USCG) Ninth District at least 30 days prior to the start of construction. Contact info: Scot Striffler, Bridge Project Manager, Ninth Coast Guard District PH: (216) 902-6087 FAX: (216) 902-6088 Scot.M.Striffler@USGS.MIL
5. ODOT shall provide documentation required by the U.S. Coast Guard (USCG) once the bridge replacement is completed. Complete drawings are not required but a single page showing an overhead and side view of the bridge with clearance information from International Great Lakes Datum 1985/Low Water Datum (IGLD85/LWD) would be adequate for documentation for the USCG.
[bookmark: _Toc256000065]Section4f, Identified Section 4(f) Properties
Commitments
1. The contractor will be required to closely coordinate the construction schedule with ODOT, the ODNR Scenic River coordinator, ODNR Parks and Recreation, and the City of Waterville.  Christina Kuchle, Northwest Region-Scenic River Manager, office: (419) 429-8306, mobile: (419) 348-5073, Christina.kuchle@dnr.state.oh.us and the City of Waterville contact is James Bagdonas, Municipal Administrator, office: (419) 878-8100, jbagdonas@waterville.org and the ODOT District Environmental coordinator is Stacy Schimmoeller office: (419) 373-4319 or stacy.schimmoeller@dot.ohio.gov. The ODNR Division of Parks and Recreation contact person is Gary Obermiller at 614-265-6561 or ohiostateparks@dnr.state.oh.us

The contractor will notify ODOT, ODNR Scenic River coordinator, ODNR Parks and Recreation section, and City of Waterville 18 days prior to beginning construction so that the public can be informed 15 days prior to construction.
2. For watercraft safety, the contractor will coordinate with ODNR Division of Watercraft the installation of the appropriate warning signs and buoys in the water directing hand-powered watercraft to Waterworks Park, upstream of Memorial Park. The ODNR Division of Watercraft contact person is Chad German at 419-836-6003 or maumeebay.watercraft@dnr.state.oh.us 
3. Advance notice of the project's construction schedule and potential for users to encounter partial closures at the bridge (for the causeway and demolition) will be provided by the contractor no less than 48 hours prior to construction activities.  Notices shall be posted in an area that can be seen by users of the Maumee River, both upstream and downstream, and on the ODNR and ODOT website.

The contractor shall notify the ODOT District Environmental coordinator Stacy Schimmoeller at (419) 373-4319 or stacy.schimmoeller@dot.ohio.gov.; the ODNR Northwest Region-Scenic River Manager Christina Kuchle at (419) 429-8306 or mobile (419) 348-5073 or Christina.kuchle@dnr.state.oh.us; the City of Waterville administrator James Bagdonas at (419) 878-8100 or jbagdonas@waterville.org; and the ODNR Division of Parks and Recreation Chief Gary Obermiller at 614-265-6561 or ohiostateparks@dnr.state.oh.us

4. ODOT, the contractor, and the City of Waterville will cooperate prior to construction to remove for safekeeping the existing benches, memorial stone, grill, birdhouse, mutt receptacle, concrete trash receptacle, and flag pole associated with Memorial Park.  These items shall be reinstalled following completion of construction in a manner as good or better than which they existed prior to construction. 
5. All areas of Memorial Park disturbed by construction activities will be restored to a condition at least as good as or better than that which existed prior to the proposed project.
6. ODOT and the City of Waterville will coordinate for the demolition of the former Waterville Public School building prior to start of construction activities.
7. Following completion of construction, ODOT and the City of Waterville will coordinate to ensure, the former Waterville Public School property will be integrated with Memorial Park.
8. Fencing will be installed around Memorial Park and the former Waterville Public School property, except for the boundary along the river.  This fencing can be the same fencing used to secure the equipment and materials as needed, so long as it is along the property boundary.
[bookmark: _Toc256000066]Permits, Waterway Permits
Commitments
1. The project requires a waterway permit for work within wetlands and the Maumee River which shall be attached to the plans as Special Provisions. No work within wetlands and/or below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by ODOT. All conditions of the permit shall be followed throughout construction by the contractor. 

[bookmark: _Toc256000067]Permits, Storm Water Permits
Commitments
1. ODOT and the contractor shall ensure that an National Pollution Discharge Elimination System (NPDES) permit shall be acquired prior to the start of construction. 
[bookmark: _Toc256000068]Permits, Floodplains
Commitments
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1. If required, ODOT shall ensure that a floodplain permit is acquired prior to construction.  
[bookmark: _Toc256000069]Preparers  & Approvals
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	Form Preparer
	Patrick Etchie
The Mannik AND Smith Group Inc.
1800 Indian Wood Circle, Maumee OH 43537
419-891-2222
petchie@manniksmithgroup.com



	Supporting Form Preparer(s)
	Phoenix Golnick, Jessica Stratigakos, Libby Rushley, Maura Johnson, Mike Lehman, R. christopher Homan


[bookmark: _Toc256000071]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:
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	June 16, 2016
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	June 13, 2016
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[bookmark: _Toc256000072]Appendix
[bookmark: _Toc256000073]Uploaded Files by Report Section
[bookmark: _Toc256000074]Air
Qualitative MSAT Analysis.pdf
OEPA Approval - Qualitative MSAT.pdf
PM2.5 Nonattainment Area Map.pdf
Ozone Nonattainment Area Map.pdf
[bookmark: _Toc256000075]Noise
OES Approval_Noise Analysis.pdf
Noise Analysis.pdf
[bookmark: _Toc256000076]Section 4(f)
OES Section 106 Determination - No Use.pdf
Site Specific Property Map.pdf
Coordination with OWJ.pdf
Coordination with OWJ_2.pdf
Determination Request Form for Recreational Properties.pdf
OES Recreational Determination - No Use.pdf
OES Recreational Determination - Programmatic Evaluation.pdf
[bookmark: _Toc256000077]General
USGS Quadrangle Topographical Map.bmp
Stage 1 Design.pdf
Detour Plan.pdf
Detour Mapping.pdf
Aerial Map.bmp
County Map.pdf
Bridge Preliminary Design Report.pdf
Right of Way Plan Sheets.pdf
Known Utility Relocations.pdf
Signal Warrants Report.pdf
Roundabout Analysis.pdf
Transportation Plan or Visioning Documents.pdf
Project Initiation Package.pdf
Peer Review.pdf
[bookmark: _Toc256000078]Purpose and Need
OES Approval.pdf
Bridge Condition Rating.pdf
Bridge Inventory Information.pdf
[bookmark: _Toc256000079]Alternatives
Alternatives Evaluation Matrix.pdf
OES Approval - Alternatives Evaluation Report.pdf
Alternatives Evaluation Report.pdf
Certified Traffic Report.pdf
Certified Traffic Review Comments.pdf
Certified Traffic Review Comments_2.pdf
[bookmark: _Toc256000080]ESA
OES Recommendations - Phase I.pdf
OES Review Comments - Screening.pdf
Screening.pdf
Phase I .pdf
Phase II .pdf
OES Recommendations - Screening.pdf
OES Recommendations - Phase II.pdf
[bookmark: _Toc256000081]Cultural Resources
OES Scoping Guidance.pdf
Coordination with SHPO - NHPA.pdf
SHPO Concurrence - NHPA.pdf
Project Related Correspondence Containing an OES Decision.pdf
Section 106 Request for Review.pdf
Records Check.pdf
Site Specific Resource Mapping.pdf
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