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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
TheFUL-20-23.60 project proposes the replacement of a culvert, including an extension and minor realignment, carrying Stream 1 (an unnamed tributary to Tenmile Creek) under US-20 in Amboy Township, Fulton County.  Construction is expected to begin in August 2018 and conclude in November 2018. During this time, US-20 will be closed for approximately 30 days and a detour will be posted. Although there will be a temporary, short term access restriction during the construction detour, the proposed project will have no disproportionately high and adverse impacts to minority or low income populations based upon the census mapping review and Environmental Justice Questions.  A detour will be posted. 
Atotal of 523 linear feet of permanent impacts to Stream 1 are anticipated basedupon preliminary construction drawings.  A Permit Determination Request will be submitted and the appropriate waterway permit obtained before any construction will occur below the Ordinary High Water Mark (OHWM) of Stream 1.  
	STIP Reference #
	SLI 32


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Permit Determination and/or Permit Application Approval Pending


	Isolated Wetland Permit
	No


	Endangered Species:
	No Impacts to Protected Species and Critical Habitat


	100-Year Floodplain:
	No Encroachment Within a Special Flood Hazard Area (SFHA)


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	Minimum Potential to Cause Effect - Appendix B


	Cultural Resources Coordination - ODOT Approval Date:
	12/05/2016


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Yes


	Hazardous Materials - OES Approval Date:
	08/18/2016


	Phase I ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
3. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
4. The project requires a waterway permit for work within Stream 1 (unnamed tributary to Tenmile Creek) which will be attached to the plans as Special Provisions. No work below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by ODOT. All conditions of the permit shall be followed throughout construction by the contractor. 
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Commitments
1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
3. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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4. The project requires a waterway permit for work within Stream 1 (unnamed tributary to Tenmile Creek) which will be attached to the plans as Special Provisions. No work below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by ODOT. All conditions of the permit shall be followed throughout construction by the contractor. 
[bookmark: _Toc256000004]Preparers  & Approvals
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	Form Preparer
	Jeff Pettit
Davey Resource Group
1500 North Mantua Street, Kent OH 44240
330-673-5685
jeff.pettit@davey.com
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	January 6, 2017

	Stacy Schimmoeller PROGRAM ADMIN 3
	January 6, 2017
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Aerial Map.pdf
County Map.pdf
USGS Quadrangle Topographical Map.bmp
Schematic Plan.pdf
[bookmark: _Toc256000010]ESA
Screening Map.png
Screening.pdf
Asbestos Survey.pdf
OES Recommendations - Screening.pdf
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Section 106 Request for Review.pdf
OES Approval - Minimum Potential to Cause Effects - B.pdf
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NHDB Map.pdf
Level 2 ESR FUL-20-23.60 PID 91327.pdf
OES Approval.pdf
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Water Source Protection Area Map.pdf
[bookmark: _Toc256000014]Environmental Justice
Census Mapping.pdf
Environmental Justice Form.pdf
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