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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The project islocated on State Route 66 (SR 66)  in southeastern Williams County, southeast of the town of Bryan.  The project includes replacement of the slab deck, abutments, minor approach work, and installation of new rock channel protection on the existing bridge over Coon Creek at straight line mile (SLM) 0.63 due to the poor condition of the bridge.  Roadway resurfacing will also be conducted  from the intersection of SR 66 and County Road 1 at the Defiance County/Williams County line to the intersection of SR 66 and US Route 6 (Elm Grove Grange Road) to the north.  All work will be within the existing right of way.
Stage 2 plans and project mapping can be found in the Project file in the General section.
	STIP Reference #
	SLI 32


	Select the appropriate project type:
	(28) Bridge rehabilitation, reconstruction, or replacement or the construction of grade separation to replace existing at-grade railroad crossings, if the actions meet the constraints in 23 CFR 771.117(e). Examples include: Railroad projects that close or relocate at-grade crossings


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Regional General Permit


	Waterways Permit Approval Date
	11/30/2016


	Isolated Wetland Permit
	No


	Endangered Species:
	Present; No finding of May Affect, Likely to Adversely Affect


	Endangered Species - Coordination
	No Effect


	100-Year Floodplain:
	No Encroachment Within a Special Flood Hazard Area (SFHA)


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	Minimum Potential to Cause Effect - Appendix A


	Cultural Resources Coordination - ODOT Approval Date:
	11/01/2016


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	10/03/2016


	Hazardous Materials - ESA Screening Conducted
	Yes


	Hazardous Materials - OES Approval Date:
	08/29/2016


	Phase I ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except the WIL-66-0.63 bridge over Coon Creek.
6. The project requires a waterway permit for work within Coon Creek which will be attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
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1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project from April 1 through September 30.  All necessary tree removal shall occur from October 1 through March 31.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except the WIL-66-0.63 bridge over Coon Creek.
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6. The project requires a waterway permit for work within Coon Creek which will be attached to the plans as Special Provisions.  All conditions of the permit shall be followed throughout construction by the contractor. 
[bookmark: _Toc256000004]Preparers  & Approvals
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	Form Preparer
	Brian Metz
TranSystems Corporation
1105 Schrock Road Suite 400, Columbus OH 43229
614-433-7800
bsmetz@transystems.com
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	December 19, 2016

	Stacy Schimmoeller PROGRAM ADMIN 3
	December 19, 2016
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LWCF Grant Listing.pdf
[bookmark: _Toc256000010]General
Aerial Map.pdf
USGS Quadrangle Topographical Map.pdf
County Map.pdf
STIP Listing.pdf
Schematic Plan.pdf
Stage 2 Design.pdf
Bridge location map.pdf
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Screening map.pdf
Asbestos Survey.pdf
Screening.pdf
OES Recommendations - Screening.pdf
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Buckeye Assets Mapping.pdf
OHPO map.pdf
WILL 66 Scoping Request Form .pdf
Minimum Potential to Cause Effects - A.pdf
[bookmark: _Toc256000013]Ecological
Level 1 ESR WIL-66-0.63 PID 101344 .pdf
OES Approval.pdf
Ecological Map.pdf
[bookmark: _Toc256000014]Other Resources
Water Source Protection Area Map.pdf
[bookmark: _Toc256000015]Environmental Justice
Census Mapping.pdf
EJ Checklist.pdf
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EMA and School Notification.pdf
Property Owner Notification Letter.pdf
Notification Mailing List.pdf
Field work notification mailing list.pdf
Property Owner Field Work Letter.pdf
Public Comment and Response.pdf
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FEMA FIRM.pdf
Permit Determination Request Packet.pdf
OES Permit Determination.pdf
Special Provisions.pdf
Regional General Permit B.pdf
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