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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: This project is located in Toledo, Lucas County, Ohio and proposes to reconstruction of 0.25 miles of State Route 25/Anthony Wayne Trail (SR-25/AWT) and the ramps to/from AWT to Collingwood Boulevard.  The project is located from the railroad track bridge just west of the intersection with Emerald Avenue/City Park to the Swan Creek bridge, just west of where AWT goes under I-75. Pedestrian and vehicular traffic will not be impacted, as there are no sidewalks and no pedestrian paths in the limits of construction and there will be no changes in access during or after construction.  Swan Creek is within the project limits; however, there will be no impacts to it or other waterways, therefore a waterway permit is not required.
	STIP Reference #
	2016AM10ID0264FDCO 


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream (including Swan Creek) and/or within a wetland.
	
	 Environmental Document Level: C1
PID 102122 LUC SR 25 8.04 Reconstruct
Approved: January 10, 2017



6. Pedestrian access shall be maintained at all times.  
[bookmark: _Toc256000002]Environmental Commitments
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Commitments
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
4. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream (including Swan Creek) and/or within a wetland.
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6. Pedestrian access shall be maintained at all times.  
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	Form Preparer
	Valerie Jones
Parsons Brinckerhoff, Inc. 
312 Elm Street, Suite 2500 , Cincinnati OH 45202
513-639-2153
jonesv@pbworld.com



	Supporting Form Preparer(s)
	Steve Lane, Valerie Jones


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	January 10, 2017

	Stacy Schimmoeller PROGRAM ADMIN 3
	January 10, 2017
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LWCF Grant Listing.pdf
[bookmark: _Toc256000010]General
Project Study Area Map.pdf
USGS Quadrangle Topographical Map.pdf
County Map.pdf
Stage 1 Design.pdf
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Screening.pdf
Project Related Correspondence Containing an OES Decision.pdf
OES Recommendations - Screening.pdf
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Buckeye Assets Mapping.pdf
Site Specific Resource Mapping.pdf
Minimum Potential to Cause Effects - A.pdf
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Ecological Review Form - Documentation for an Ecologically Exempt Project .pdf
Field Investigation Notes.pdf
[bookmark: _Toc256000014]Other Resources
Water Source Protection Area Map.pdf
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Census Mapping.pdf
EJ C2 Form.pdf
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FEMA FIRM.pdf
Floodplain Impacts.pdf
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