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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This project proposes to upgrade several traffic signals located at State Route 51 and Wales road/I-280 northbound and State Route 51 and I-280 southbound in Wood County. All work will be performed within the public right of way and no utilities will be impacted. No work will take place within special flood hazard areas or waters of the US, therefor no permits are required. Construction is expected to being in spring of 2018 and last approximately 60 days. During construction, traffic is expected to be maintained. 
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	08/09/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(8) Installation of fencing, signs, pavement markings, small passenger shelters, traffic signals, and railroad warning devices where no substantial land acquisition or traffic disruption will occur. Examples include: The installation or maintenance of signs, pavement markings/raised pavement markers/sensors, traffic calming activities, and/or new or replacement fencing (right-of-way, vandal, etc.); General pavement marking or "line painting" projects.

	
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. Notes shall be placed in the plans by ODOT directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-8 and 642-58 to ensure compliance with Federal notification requirements.  
3. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should a tree be a safety hazard for the traveling public, the tree should be cut as soon as possible. 
	
	 Environmental Document Level: C1
PID 101147 D02 TSG FY2018
Approved: June 23, 2017



4. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
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2. Notes shall be placed in the plans by ODOT directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-8 and 642-58 to ensure compliance with Federal notification requirements.  
3. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should a tree be a safety hazard for the traveling public, the tree should be cut as soon as possible. 
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4. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Eli Barber, Phoenix Golnick Neal, Stacy Schimmoeller
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	June 23, 2017

	Phoenix Golnick Neal ENV SPEC 2
	June 23, 2017
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