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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
TheOhio Department of Transportation is proposing to resurface US Route 6 in SanduskyCounty from County Road 232 to the Erie County line. Additional work includesminor maintenance (replace deck edges and guardrail, waterproofing, pileencasements and patching) on several bridges which will require temporary closures/detours. Below is the list of bridge locations and the expected closure durations.
· SAN-6-22.72(between Schiets Rd and Jacobs Rd)- 30 days
· SAN-6-24.64(between Polter Rd and Minier Rd)- 21 days
· SAN-6-25.24(between Minier Rd and SR 510)- 30 days
· SAN-6-25.77(between SR 510 and CR 256)- 30 days
· SAN-6-27.18(between CR 260 and CR 268/N Vickery Rd)- 3 days
· SAN-6-29.65(between CR 290 and CR 294)- 3 days
All impacted property owners, local public safety agencies, and schools have been notified of these closures. The work on some of the bridges does require a permit from the US Army Corps of Engineers, which has already been acquired. This project also required coordination with the local floodplain administrator due to the work impacting several floodplains. All NFIP and EO 11988 regulations have been followed and all documentation is in the project file. Notes to project several state or federally listed species will be added to the plans to ensure that there will be no impacts. No historically significant resources will be impacted by this project. Construction is expected to begin in the summer of 2018 and the resurfacing will last approximately 160 days and all bridge closures will happen during those 160 days. A minimum of one lane of traffic will be maintained at all times with the exception of the bridge closures noted above. 
This document was approved using Stage 2 plans.
	STIP Reference #
	SLI 32


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(28) Bridge rehabilitation, reconstruction, or replacement or the construction of grade separation to replace existing at-grade railroad crossings, if the actions meet the constraints in 23 CFR 771.117(e). Examples include: Railroad projects that close or relocate at-grade crossings


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Permit Determination and/or Permit Application Approval Pending


	Isolated Wetland Permit
	No


	Endangered Species:
	Present; No finding of May Affect, Likely to Adversely Affect


	Endangered Species - Coordination
	May Affect, Not Likely to Adversely Affect


	Endangered Species - Coordination Date
	10/03/2016


	Endangered Species - Critical Habitat Present/Impacted
	Kirtland's warbler


	Endangered Species - Other Critical Habitat Present/Impacted:
	No


	100-Year Floodplain:
	Encroachment Within the SFHA is a Functionally Dependent Use


	EO 11988/NFIP Coordination and Documentation Completed:
	Yes


	NFIP Local Floodplain Coordinator Notification Date:
	06/15/2017


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Not Present


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	08/31/2017


	Hazardous Materials - ESA Screening Conducted
	Studies Not Required


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. Parts 642-8 and 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
4. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except for SAN-6-25.24 over Raccoon Creek (STA. 1328) and SAN-6-25.76 over Little Raccoon Creek (STA. 1356).

5. The project requires a waterway permit for work within the SAN-6-25.24 over Raccoon Creek (STA. 1328) and SAN-6-25.76 over Little Raccoon Creek (STA. 1356) which is attached to the plans as Special Provisions that shall be followed throughout construction by the contractor. 

6. A mussel survey and, if necessary, relocation shall occur at SAN-6-25.24 over Raccoon Creek in accordance with ODNR and USFWS protocols.  No in-stream work shall occur prior to the mussel survey/relocation.

The required mussel relocation was completed in August 2017.

7. If any turtles are found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue. 
8. To minimize impacts to the Kirtland's warbler during migration, the contractor shall not remove trees and brush located within 3 miles of the Lake Erie shoreline between April 22nd and June 1st or between August 15th and October 15th. If this species is encountered within the construction limits during construction operations, all construction operations will cease and the USFWS Columbus Field Office be notified immediately (614-416-8993). Activity will not resume until coordination with USFWS has been concluded.
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1. The contractor shall perform all work within the existing right of way. 
2. Parts 642-8 and 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
4. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge deck(s) and edge of the culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work is permitted below the top of bank of any stream, except for SAN-6-25.24 over Raccoon Creek (STA. 1328) and SAN-6-25.76 over Little Raccoon Creek (STA. 1356).

5. The project requires a waterway permit for work within the SAN-6-25.24 over Raccoon Creek (STA. 1328) and SAN-6-25.76 over Little Raccoon Creek (STA. 1356) which is attached to the plans as Special Provisions that shall be followed throughout construction by the contractor. 

6. A mussel survey and, if necessary, relocation shall occur at SAN-6-25.24 over Raccoon Creek in accordance with ODNR and USFWS protocols.  No in-stream work shall occur prior to the mussel survey/relocation.

The required mussel relocation was completed in August 2017.

7. If any turtles are found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue. 
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8. To minimize impacts to the Kirtland's warbler during migration, the contractor shall not remove trees and brush located within 3 miles of the Lake Erie shoreline between April 22nd and June 1st or between August 15th and October 15th. If this species is encountered within the construction limits during construction operations, all construction operations will cease and the USFWS Columbus Field Office be notified immediately (614-416-8993). Activity will not resume until coordination with USFWS has been concluded.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick Neal
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	October 5, 2017

	Phoenix Golnick Neal ENV SPEC 2
	October 5, 2017
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