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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	TIFFIN


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The City of Tiffin is proposing to resurface the various State Rout (SR) roadway segments listed below in the City of Tiffin in Seneca County.
1. SR-18 (East Market) from Teakwood Drive (Straight Line Mileage (SLM) 13.00) to Hopewell Avenue (SLM 13.26) 
2. SR-101 (East Market) from Heilman Street (SLM 1.30) to Corp Limit (SLM 1.64) 
3. SR-100 (Washington St) from Tiffin Corporation Limit line (SLM 9.84) to Sandusky Street (SR-53) (SLM 10.45)
These roadway segments are not located within a special flood hazard area and no waterway permits are required for this project.  The section of SR-100 (Washington Street) is within 1000 feet of the Sandusky River; however, is within the limits of the City of Tiffin, where the Ohio Department of Natural Resources (ODNR) does not have jurisdiction.  This project is located within the drinking water source area of effect of two businesses and therefore a plan note will be added to the project plans to protect those drinking water sources. Construction is expected to begin in the summer of 2017. During construction, one lane of vehicular traffic will be maintained at all times. There is no work on sidewalks so pedestrian traffic shall maintained at all times.  
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify the City of Tiffin a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, the City of Tiffin will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
6. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
7. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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8. Pedestrian traffic shall be maintained at all times. 
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Commitments
1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify the City of Tiffin a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, the City of Tiffin will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
6. The intent of this project is to not remove any trees. The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  No trees shall be removed under this project.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
7. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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8. Pedestrian traffic shall be maintained at all times. 
[bookmark: _Toc256000004]Preparers  & Approvals
[bookmark: _Toc256000005]Form Preparer(s)
	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick, Stacy Schimmoeller
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	January 23, 2017

	Stacy Schimmoeller PROGRAM ADMIN 3
	January 23, 2017
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