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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This project proposes to replace the lighting communication equipment for the Veteran's Glass City Skyway (VGCS, Interstate 280) bridge which is partially located within the Craig Street Bridge (the bridge just to the west). Additional work includes replacing lights inside and outside of the center pier of the VGCS and repositioning the lights within the median, which are explained in more detail as Alterative 3 for the tower lighting and Alternative 1 for the cable lighting in the study in the project file. No work will occur below the lowest portion of either bridge; however because this section of the Maumee River is considered a Section 9 and Section 10 water, waterway permitting coordination is being completed with the US Army Corps of Engineers (USACE) and the US Coast Guard (USCG).  The work will occur above a floodplain but will have no impact. Construction is expected to begin in the summer of 2017. During construction, temporary single lane closures on I-280 and the Craig Street Bridge are expected; however pedestrian traffic shall be maintained at all times. A bald eagle nest is shown on the ecological map; however, because it is greater than 1,000 feet from the project area, the project does not require construction date restrictions required when the project is 660 feet or closer to the nest. 
	STIP Reference #
	2016AM08ID0230FDCO 


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	01/04/2017


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Work on the structures shall not be performed between the bridge deck and the water within the navigation channel.  Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.         
4. Pedestrian access shall be maintained at all times on the Craig Street Bridge. 
5. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT or LPA, as required.
6. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge decks during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
7. Coordination with the US Army Corps of Engineers (USACE) and US Coast Guard (USCG) to determine if waterway permitting is required, shall continue.  Should any waterway permits be required, they shall be acquired prior to the start of construction.  
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8. Due to the known presence of Ohio endangered blue spotted salamander within the project area, if any salamander is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
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1. The contractor shall perform all work within the existing right of way. 
2. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
3. Work on the structures shall not be performed between the bridge deck and the water within the navigation channel.  Nothing shall change the vertical clearance height between the lowest portion of the bridge and the surface of the water within the navigational channel.         
4. Pedestrian access shall be maintained at all times on the Craig Street Bridge. 
5. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT or LPA, as required.
6. The contractor shall take all precautions to prevent any and all material from going off the edge of the bridge decks during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
7. Coordination with the US Army Corps of Engineers (USACE) and US Coast Guard (USCG) to determine if waterway permitting is required, shall continue.  Should any waterway permits be required, they shall be acquired prior to the start of construction.  
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Eli Barber, Stacy Schimmoeller
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	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	January 30, 2017

	Stacy Schimmoeller PROGRAM ADMIN 3
	January 30, 2017
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