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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	Bowling Green, City of


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The project proposes to install markedcrosswalks with pedestrian hybrid beacons, lighting, and two-stage crossingmedian refuge islands at the Bowling Green State University Founders Hall and Stroh Center to improve pedestrian safety on the local roadways within theBowling Green State University campus.  PermanentR/W will be needed for the addition of sidewalks and deep excavation is neededfor the beacon pole foundations. All deep excavation is within the existingright of way and has been investigated as shown in the project file.This project will not require any waterway permits and is not located within a special flood hazard area. There is record of the lye-leaved water cress near the project area; however, the habitat part shade/sun, dry sandy or rocky soil, dunes, cliff, prairies, and/or open woods is not within the project area.  Construction is expected to begin in the fall of 2017 and last approximately 60 days. A minimum of one lane of traffic in each direction on Wooster Street will be maintained at all times.  Pedestrian traffic shall be maintained at all times.  
	STIP Reference #
	SLI 15


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Not Present


	Endangered Species:
	No Impacts to Protected Species and Critical Habitat


	100-Year Floodplain:
	No Encroachment Within a Special Flood Hazard Area (SFHA)


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	Minimum Potential to Cause Effect - Appendix B


	Cultural Resources Coordination - ODOT Approval Date:
	01/18/2017


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	


	Hazardous Materials - ESA Screening Conducted
	Yes


	Hazardous Materials - OES Approval Date:
	12/06/2016


	Phase I ESA Warranted Based on Coordination with OES:
	No Further Studies Warranted


	Farmland:
	Urbanized Area; No Impacts in Accordance With the Farmland MOU and 7 CFR 658


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. The contractor shall take all precautions to prevent any and all material from going off the edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
6. Pedestrian traffic shall be maintained at all times.  
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1. The contractor shall notify ODOT a minimum of 18 days prior to beginning work, any major disruptive, time delaying traffic control changes, or detours during construction. Upon receipt of notice from the contractor, ODOT will notify affected agencies including local media outlets, schools, police, fire, emergency services, bus transportation departments, and post offices 15 days prior the work.
2. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and ODOT, as required.
3. Appropriate local detour routes and accommodations shall be made for any local special events or festivals using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be developed and implemented.
5. The contractor shall take all precautions to prevent any and all material from going off the edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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6. Pedestrian traffic shall be maintained at all times.  
[bookmark: _Toc256000004]Preparers  & Approvals
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Stacy Schimmoeller PROGRAM ADMIN 3
	February 28, 2017

	Stacy Schimmoeller PROGRAM ADMIN 3
	February 28, 2017
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Aerial Map.pdf
Schematic Plan.pdf
Stage 2 Design.pdf
USGS Quadrangle Topographical Map.pdf
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Screening Map.png
Screening.pdf
OES Recommendations - Screening.pdf
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Buckeye Assets Mapping.PNG
Project Study Area Map.pdf
Section 106 Request for Review.pdf
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Ecological Review Form - Documentation for an Ecologically Exempt Project .pdf
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