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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	OTTAWA COUNTY ENGINEER


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The Ottawa County Engineer is proposing to resurface and widen approximately1 mile of Krause Rd in Ottawa County to bring the road up to standard width. Approximately 285 feet of roadside stream will be enclosed to allow for the widening of the road. Permanent right of way from a private owner (agricultural land) will be needed to allow for the enclosure of the stream. Utility relocations are expected. The Ottawa County Engineer is in the process of acquiring a waterway permit from the US Army Corp of Engineers for the stream impacts. No work will be started within the stream until the permit has been acquired. This project is located within a floodplain and the local floodplain administrator has reviewed and approved the project. This project has been coordinated with the Ohio Dept. of Natural Resources and the US Fish and Wildlife Service due to the impacts to the stream and location near the Ottawa National Wildlife Refuge. All conditions of the MOA between ODOT and these two agencies will be met and there will be no impacts to any federally or state listed species. There is minimal potential to effect any historic resources. Construction is expected to begin in the summer of 2019 and last approximately 90 days. During construction, one lane of traffic will be maintained at all times. 
This document was approved based on Stage 2 plans. 
	STIP Reference #
	SLI 30


	Select the appropriate project type:
	(26) Modernization of a highway by resurfacing, restoration, rehabilitation, reconstruction, adding shoulders, or adding auxiliary lanes (including parking, weaving, turning, and climbing lanes), if the action meets the constraints in paragraph (e) of this section. Examples include: Joint or limited use of right-of-way where the proposed use would have minimal or no adverse social (including highway safety), economic or environmental impacts; Installation of new noise walls and other new noise mitigation projects; Construction of highway safety and truck escape ramps; Construction of bicycle lanes and pedestrian walkways, sidewalks, shared-use paths, or facilities and trailhead parking that do not otherwise qualify for a C1 designation; Beautification or facility improvement projects (i.e. landscaping, curb and gutter installation and replacement, ADA ramps/curb ramps, installation of park benches, decorative lighting, etc.); Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


In accordance with 23 CFR 771.117(e), the proposed project cannot be processed as a C2 CE, if it involves -
1. a. Acquisition of more than a minor amount of right-of-way
2. b. Residential or non-residential displacements
3. c. A Coast Guard, Individual Section 404 and/or a Section 10 permit
4. d. A Section 106 finding of Adverse Effect
5. e. A Section 4(f) Programmatic or Individual Evaluation
6. f. A finding of May Affect, Likely to Adversely Affect to Threatened and Endangered Species
7. g. Construction of temporary access, or the closure of existing road, bridge, or ramps, that would result in major traffic disruptions
8. h. Changes in access control
9. i. Floodplain encroachment other than functionally dependent uses (e.g., bridges, wetlands) or actions that facilitate open space use (e.g., recreational trails, bicycle and pedestrian paths)
10. j. Construction activities in, across or adjacent to a river component designated or proposed for inclusion in the National System of Wild and Scenic Rivers
11. k. No minor public or agency controversy on environmental grounds (no opposition from any organized groups or agencies and no unresolved environmental coordination)
12. l. If an EJ Analysis Report is required, the project must be processed as a D-level CE or higher level document

For certification purposes, documentation is required to illustrate no significant impacts will occur to the following environmental resources and that no unusual circumstances exist that would warrant a higher level of NEPA document. Upload all supporting documentation to the project file.
	Waterways:
	Present; No Coast Guard, Individual 404, and/or Section 10 Permit required


	Waterways Permit Type:
	Permit Determination and/or Permit Application Approval Pending


	Isolated Wetland Permit
	No


	Endangered Species:
	No Impacts to Protected Species and Critical Habitat


	100-Year Floodplain:
	Encroachment Within the SFHA is a Functionally Dependent Use


	EO 11988/NFIP Coordination and Documentation Completed:
	Yes


	NFIP Local Floodplain Coordinator Notification Date:
	11/02/2017


	Section 4(f):
	Not present


	Section 6(f):
	Not present


	Cultural Resources:
	Present; No Finding of Adverse Effect


	Cultural Resources Coordination:
	Minimum Potential to Cause Effect - Appendix B


	Cultural Resources Coordination - ODOT Approval Date:
	09/11/2017


Projects that meet C2 criteria are not anticipated to have impacts to the following environmental resources. If resources are present, documentation is only required if there is a potential for impacts.
	Air Quality:
	Studies Not Required


	Air Quality - Coordination with OES:
	No


	Noise:
	Studies Not Required


	Noise Coordination - OES Approval Date:
	12/07/2017


	Hazardous Materials - ESA Screening Conducted
	Studies Not Required


	Farmland:
	Non-Urbanized Area; No Impacts in Accordance With the Farmland MOU, 7 CFR 658, and ORC 929.05


	Scenic Rivers
	No National Wild and Scenic River Within 1000 Feet of the Proposed Project Area


Projects that meet C2 criteria must be in accordance with ODOT's EJ Guidance and activities conducted for Public Involvement are commensurate to the project's type and scope of work.
	Environmental Justice:
	Does Not Exceed EJ Guidance Criteria; No EJ Analysis Report Required and No EJ Issues Raised During Public Involvement


	Public Involvement:
	Minimum PI Requirements Met; No Minor Public or Agency Controversy on Environmental Grounds


	Environmental Commitments
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. Notes shall be placed in the plans by the LPA directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-8 and 642-58 to ensure compliance with Federal notification requirements.
2. Appropriate local detour routes and accommodations shall be made by LPA and the Contractor for any local special events or festivals prior to the start of the event using appropriate signage.
3. If required by local ordinance, a construction noise plan note will be added to the plans by LPA and implemented by the contractor during construction.
4. The contractor shall not remove any trees under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. If any snake or turtle is found within the project work limits, the contractor shall wait until the species has moved off of the project site unharmed before work can continue. 
6. The project requires a waterway permit for work within Stream 1. No work below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by Ottawa County Engineer. All conditions of the permit shall be followed throughout construction by the contractor. 
7. The contractor shall not remove any trees under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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1. Notes shall be placed in the plans by the LPA directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-8 and 642-58 to ensure compliance with Federal notification requirements.
2. Appropriate local detour routes and accommodations shall be made by LPA and the Contractor for any local special events or festivals prior to the start of the event using appropriate signage.
3. If required by local ordinance, a construction noise plan note will be added to the plans by LPA and implemented by the contractor during construction.
4. The contractor shall not remove any trees under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. If any snake or turtle is found within the project work limits, the contractor shall wait until the species has moved off of the project site unharmed before work can continue. 
6. The project requires a waterway permit for work within Stream 1. No work below the Ordinary High Water Mark (OHWM) shall take place until the proper permit is obtained by Ottawa County Engineer. All conditions of the permit shall be followed throughout construction by the contractor. 
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7. The contractor shall not remove any trees under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Eli Barber
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Neal ENV SPEC 2
	December 7, 2017

	Phoenix Neal ENV SPEC 2
	December 7, 2017
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Aerial Map.pdf
County Map.pdf
USGS Quadrangle Topographical Map.pdf
Stage 2 Design.pdf
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ESA Screening map.pdf
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OHPO map.pdf
Section 106 Scoping Request Form.pdf
Minimal Potential to Cause Effects - A or B.pdf
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Eco map.pdf
Level 1 ESR OTT-TR76 FLAP PID 104494.pdf
Coordination with ODNR and USFWS.pdf
ODNR Comments.pdf
USFWS Comments.pdf
General MOA Condition Dispositions.pdf
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Water Source Protection Area Map.pdf
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FEMA FIRM.pdf
Permit Determination Request.pdf
Statement of Findings.pdf
OES Permit Determination.pdf
Local Floodplain Administrator Approval.pdf
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