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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	ODOT SPONSORING AGENCY


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This project will upgrade Type A/blunt end guardrailon NHS routes throughout district 2. All work is within right of way and there will be no impacts to utilities. Construction is expected to begin in the spring of 2018 and last approximately 120 days. During construction, traffic will be maintained at all locations with the exception of the US Route 6/20 and State Route 19 interchange in Fremont (Sandusky County) Ohio. This location will be closed for approximately 14 days. All emergency management agencies and school officials have been notified of this closure.
No work at any location will require a permit or coordination with the US Army Corps of Engineers or US Coast Guard since there will be no work below the deck of any bridge. Several locations are within special flood hazard areas, however the District 2 Hydraulics Engineer has determined that there will be no impacts to the floodplain. Records of several State listed species (Blandings Turtle- Threatened and American Badger-Species of Concern) are known to exist within the project area. Plan notes protecting these species will be added to the construction plans.  
	STIP Reference #
	SLI 15


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(1) Activities which do not involve or lead directly to construction, such as planning and technical studies; grants for training; engineering to define the elements of a proposed action or alternatives so that social, economic, and environmental effects can be assessed; and Federal-aid system revisions which establish classes of highways on the Federal-aid highway system. Examples include: Study type projects (i.e. feasibility studies, etc.); Projects that utilize no federal monies or require no federal actions (State-funded actions only); Land donations to ODOT associated with ROW permits (non-NHS/non-Limited Access right-of-way). (Environmental Site Assessment issues will require coordination with ODOT-OES) (State-funded actions only).

	
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. Notes shall be placed in the plans by ODOT directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-8 and 642-58 to ensure compliance with Federal notification requirements.  
2. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should a tree be a safety hazard for the traveling public, the tree should be cut as soon as possible. 
3. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
4. The contractor shall perform all work within the existing right of way. 
5. Due to the known presence of Ohio threatened Blandings Turtle within the project area, if any turtle is found within the project work limits at the locations below, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
1) WOO-420-2.66
2) OTT-51-8.52
6. Due to the known presence of Ohio Species of Concern American Badger within the project area, if any badger is found within the project work limits below, crews shall wait until the species has moved off of the project site unharmed before work can continue. 
1) OTT-53-11.79
2) OTT-163-27.25   
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7. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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Commitments
1. Notes shall be placed in the plans by ODOT directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-8 and 642-58 to ensure compliance with Federal notification requirements.  
2. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. Should a tree be a safety hazard for the traveling public, the tree should be cut as soon as possible. 
3. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
4. The contractor shall perform all work within the existing right of way. 
5. Due to the known presence of Ohio threatened Blandings Turtle within the project area, if any turtle is found within the project work limits at the locations below, crews shall wait until the species has moved off of the project site unharmed before work can continue.    
1) WOO-420-2.66
2) OTT-51-8.52
6. Due to the known presence of Ohio Species of Concern American Badger within the project area, if any badger is found within the project work limits below, crews shall wait until the species has moved off of the project site unharmed before work can continue. 
1) OTT-53-11.79
2) OTT-163-27.25   
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7. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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	Form Preparer
	District 2
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	June 12, 2017

	Phoenix Golnick Neal ENV SPEC 2
	June 12, 2017
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Drinking Water Protection Plan Note.pdf
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Stage 2 Design.pdf
Aerial Map.pdf
County Map.pdf
USGS Quadrangle Topographical Map.pdf
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ESA Screening maps.pdf
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OHPO maps.pdf
Minimum Potential to Cause Effects - A.pdf
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Eco maps.pdf
Ecological Review Form - Documentation for an Ecologically Exempt Project .pdf
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Water Source Protection Area Map.pdf
Community Water System Coordination.pdf
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EMA and School Notification.pdf
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FEMA FIRM.pdf
Floodplain Impacts.pdf
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