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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	OTTAWA COUNTY ENGINEER


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The Ottawa County Engineers Office is proposing to re-align the intersection of Bayshore Rd and Port Clinton Eastern Rd for safety improvements. All work is within the existing right of way. Utility relocations are required. This project does not include impacts to any waterwaysor floodplains, therefore no US Army Corps of Engineers or floodplain permitsare required.There will be no impacts to any ecological orhistorically significant resources. A plan note will be added to the plans to protect any listed species that may be in the area. Construction is expected to begin in the summer of2018 and last approximately 60 days.During construction, Port Clinton Eastern Rd will be closed permanently. Access from the existing properties to Bayshore Rd will be maintained and no detour for Port Clinton Eastern Rd is needed due to the current configuration of the intersection.  A public meeting was held to inform the impacted property owners, public safety agencies, and schools. One comment was received from the public it has been addressed. There were no public controversies brought up as a result of this project. 
This document was approved based on Stage 3 plans.
	STIP Reference #
	SLI 16


	Cultural Resources Coordination:
	Minimal Potential to Cause Effect - Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101 that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,179,656.40 of Federal funds or with a total estimated cost of not more than $31,077,938.40 and with Federal funds that comprise less than 15 percent of the total estimated project cost (each amount adjusted annually by the Secretary to reflect any increases in the Consumer Price Index prepared by the Department of Labor, see www.fhwa.dot.gov or www.fta.dot.gov).


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way. 
2. Notes shall be placed in the plans by the Ottawa County Engineers Office directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-8 and 642-58 to ensure compliance with Federal notification requirements.
3. Appropriate local detour routes and accommodations shall be made by Ottawa County Engineers Office and the Contractor for any local special events or festivals prior to the start of the event using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be added to the plans by Ottawa County Engineers Office and implemented by the contractor during construction.
5. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and Ottawa County Engineers Office, as required.
6. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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7. Due to the known presence of Ohio Species of Concern American Badger within the project area, if Badger is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue. 
[bookmark: _Toc256000002]Environmental Commitments
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1. The contractor shall perform all work within the existing right of way. 
2. Notes shall be placed in the plans by the Ottawa County Engineers Office directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-8 and 642-58 to ensure compliance with Federal notification requirements.
3. Appropriate local detour routes and accommodations shall be made by Ottawa County Engineers Office and the Contractor for any local special events or festivals prior to the start of the event using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be added to the plans by Ottawa County Engineers Office and implemented by the contractor during construction.
5. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and Ottawa County Engineers Office, as required.
6. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
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7. Due to the known presence of Ohio Species of Concern American Badger within the project area, if Badger is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick Neal


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	October 10, 2017

	Phoenix Golnick Neal ENV SPEC 2
	October 10, 2017
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Stage 2 Design.pdf
Aerial Map.pdf
County Map.pdf
USGS Quadrangle Topographical Map.pdf
Stage 3 Design.pdf
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Screening Map.pdf
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Project Study Area Map.pdf
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Eco Map.pdf
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Water Source Protection Area Map.pdf
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Property Owner Notification Letter.pdf
Public Meeting Exhibits.pdf
Public Meeting Presentation.pdf
Public Meeting Sign In Sheet.pdf
Public Notification Mailing List.pdf
EMA and School Notification.pdf
Public Comment Recieved and Response.pdf
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FEMA FIRM.pdf
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