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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	WOOD COUNTY ENGINEER


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This project proposes to replace approximately 0.75 mile of guardrail on Bowling Green Rd E from Napoleon Rd to Housekeeper Rd in Wood County. All work is within the exiting right of way and no utilities will be impacted. There will be no work in any waterways so no permit from the US Army Corps of Engineers is required. This project is not located within a floodplain and will have no impacts to any ecological or historically significant resources. Construction is expected to begin in the spring of 2018 and last approximately 30 days. During construction, one lane of traffic will be maintained at all times.
	STIP Reference #
	SLI 16


	Cultural Resources Coordination:
	(1) Minimum Potential Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101, that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,000,000 of Federal funds or with a total estimated cost of not more than $30,000,000 and with Federal funds that comprise less than 15 percent of the total estimated project cost.


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way. 
2. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. Appropriate local detour routes and accommodations shall be made by the Wood County Engineer and the Contractor for any local special events or festivals prior to the start of the event using appropriate signage.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. If required by local ordinance, a construction noise plan note will be added to the plans by LPA and implemented by the contractor during construction. 
6. No work shall occur below the elevation of 664 feet to ensure that no work (including driving) occurs below the Ordinary High Water Mark (OHWM) of the ditch on the east side of Bowling Green Road.
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7. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and the Wood County Engineer, as required.
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1. The contractor shall perform all work within the existing right of way. 
2. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. Appropriate local detour routes and accommodations shall be made by the Wood County Engineer and the Contractor for any local special events or festivals prior to the start of the event using appropriate signage.
4. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
5. If required by local ordinance, a construction noise plan note will be added to the plans by LPA and implemented by the contractor during construction. 
6. No work shall occur below the elevation of 664 feet to ensure that no work (including driving) occurs below the Ordinary High Water Mark (OHWM) of the ditch on the east side of Bowling Green Road.
	
	 Environmental Document Level: C1
PID 106103 WOO GR FY2018 - Grdral Replac
Approved: August 9, 2017



7. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and the Wood County Engineer, as required.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick Neal
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	August 9, 2017

	Phoenix Golnick Neal ENV SPEC 2
	August 9, 2017
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