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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The Ohio Department of Transportation is proposing to install a left hand turn lane on EB US-20 onto NB SR-163 to improve intersection safety. All work is within the existing right of way, there is no deep excavation and no utility impacts are anticipated. This project does not require any floodplain or US Army Corps of Engineer permits due to no impacts to any floodplains or waters of the US. There will be no impacts to any ecological or historically significant resources. A wetland is located within the right of way in the project area but it will not be impacted by this project. This project is located within a public drinking water protection area. A plan note will be added to the plan to ensure the protection of the drinking water source. Construction is expected to begin in the fall of 2018 and last approximately 60 days. During construction, one lane of traffic on US-20 and SR-163 will be maintained at all times. 
This document was approved using Stage 2 plans.
	STIP Reference #
	2018stipID0084FDCO 


	Cultural Resources Coordination:
	No Historic Properties Affected


	Cultural Resources Coordination Date:
	10/20/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101 that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,179,656.40 of Federal funds or with a total estimated cost of not more than $31,077,938.40 and with Federal funds that comprise less than 15 percent of the total estimated project cost (each amount adjusted annually by the Secretary to reflect any increases in the Consumer Price Index prepared by the Department of Labor, see www.fhwa.dot.gov or www.fta.dot.gov).


	Environmental Commitments:
	Yes
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1. x
2. The contractor shall perform all work within the existing right of way. 
3. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
4. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. Wetland A is located between station 3+20 and 4+40 Lt., and shall not be impacted. 

The contractor shall take all precautions to prevent any and all material from going outside of the construction limits during all construction operations. The contractor shall immediately remove through non-mechanical means any material that falls into the roadside ditches, streams, wetlands, or other waters. through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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6. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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1. x
2. The contractor shall perform all work within the existing right of way. 
3. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
4. No trees shall be removed under this project.  The project is located within the known habitat ranges of the federally listed and protected Indiana bat and northern long-eared bat.  This requirement is necessary to avoid and minimize impacts to these species as required by the Endangered Species Act.  For the purposes of this note, a tree is defined as a live, dying, or dead woody plant, with a trunk three inches or greater in diameter at a height of 4.5 feet above the ground surface, and with a minimum height of 13 feet. 
5. Wetland A is located between station 3+20 and 4+40 Lt., and shall not be impacted. 

The contractor shall take all precautions to prevent any and all material from going outside of the construction limits during all construction operations. The contractor shall immediately remove through non-mechanical means any material that falls into the roadside ditches, streams, wetlands, or other waters. through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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6. A plan note will be added to the construction plans in order to address the project's location in relation to the drinking water source.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Eli Barber, 
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Neal ENV SPEC 2
	November 21, 2017

	Phoenix Neal ENV SPEC 2
	November 21, 2017


	
	 Environmental Document Level: C1
PID 103744 WOO US 20 8.87 Turn Lane Sfty
Approved: November 21, 2017




[bookmark: _Toc256000007]Appendix
[bookmark: _Toc256000008]Uploaded Files by Report Section
[bookmark: _Toc256000009]Environmental Commitments
Drinking Water Protection Plan Note.pdf
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Aerial Map.pdf
Stage 2 Design.pdf
County Map.pdf
USGS Quadrangle Topographical Map.pdf
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RMR Map.pdf
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Project Study Area Map.pdf
Section 106 Scoping Request Form.pdf
OES Section 106 Effect Determination.pdf
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Water Source Protection Area Map.pdf
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FEMA FIRM.pdf
BMP locations.pdf
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