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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.


		Page 8 of 8
Contents
C1	3
Environmental Commitments, 	4
Environmental Commitments	5
C1	5
Preparers  & Approvals	6
Form Preparer(s)	6
Approvals & Electronic Signatures	6
Appendix	7
Uploaded Files by Report Section	7
General	7
ESA	7
Cultural Resources	7
Ecological	7
Other Resources	7
Permits	7

	
	 Environmental Document Level: C1
PID 106624 LUC 280 4.61 SB Drv Lane Ovly
Approved: August 21, 2017




[bookmark: _Toc256000000]C1	PID
	106624


	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Non-Federal


	Private Funding:
	No


	
	


Project Description: 
The Ohio Dept. of Transportation is proposing to overlay the southbound driving lane of the I-280 bridge over the Greenbelt Parkway in Lucas County due to poor pavement conditions. All work is within the existing right of way and there will be no impacts to any utilities. This project does not require any US Army Corps of Engineer permits and does not take place within a floodplain. This project will not impact any historically significant resources. This project is located in an area near known blue spotted salamander populations, however no suitable habitat for this species is within the project limits so there will be no impact. Construction is expected to begin in the fall of 2017 and last approximately 25 days. During construction, there will be lane restrictions on I-280, but it will remain open to traffic. 
	STIP Reference #
	N/A


	Cultural Resources Coordination:
	Minimal Potential to Cause Effect - Appendix A


	Cultural Resources Coordination Date:
	08/29/2012


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(31) Activities that do not utilize federal monies or require federal actions.


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way
2. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
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3. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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1. The contractor shall perform all work within the existing right of way
2. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
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3. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Eli Barber, Phoenix Golnick Neal
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	August 21, 2017

	Phoenix Golnick Neal ENV SPEC 2
	August 21, 2017
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