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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.


		Page 10 of 10
Contents
C1	3
Environmental Commitments, 	4
Environmental Commitments	6
C1	6
Preparers  & Approvals	8
Form Preparer(s)	8
Approvals & Electronic Signatures	8
Appendix	9
Uploaded Files by Report Section	9
General	9
Ecological	9
Permits	9

	
	 Environmental Document Level: C1
PID 106119 HEN PM FY2018
Approved: October 17, 2017




[bookmark: _Toc256000000]C1	PID
	106119


	Project Sponsor
	HENRY COUNTY ENGINEER


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The Henry County Engineer is proposing to paint pavement markings on various roads within Northern Henry County. All work is within the existing right of way and there will be no impacts to utilities. Several locations are within a special flood hazard area. Coordination with the local floodplain administrator determined that no floodplain permit is required. No permits from the US Army Corps of Engineers are required. A portion of Henry County is located within the Oak Openings Region. Plan notes will be added to the plans to protect various plant and animal species that live in this region. Construction is expected to begin in the summer of 2018 and last approximately 60 days. During construction, a minimum of one lane of traffic will be maintained at all times.
This document was approved using a list of location from the Henry County Engineers Office.
	STIP Reference #
	SLI 16


	Cultural Resources Coordination:
	Minimal Potential to Cause Effect - Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(8) Installation of fencing, signs, pavement markings, small passenger shelters, traffic signals, and railroad warning devices where no substantial land acquisition or traffic disruption will occur. Examples include: The installation or maintenance of signs, pavement markings/raised pavement markers/sensors, traffic calming activities, and/or new or replacement fencing (right-of-way, vandal, etc.); General pavement marking or "line painting" projects.


	Environmental Commitments:
	Yes
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1. Notes shall be placed in the plans by the  Henry County Engineers Office directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-58 to ensure compliance with Federal notification requirements.
2. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and the Henry County Engineer, as required.
3. If any animals, snake, turtle, bird, salamander, etc. is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.


4. Due to the location of the following locations within the globally rare Oak Openings region, there shall be no earth disturbance.  No work shall be done off the existing pavement.  Care shall be taken to not disturb the existing vegetation. 
a. CR-3 from CR-U to CR- W
b. CR-4A from CR-U to CR-W
c. CR-7 from Liberty Center Corp to CR-U
d. CR-W from CR-1 to CR-4
e. CR-V from CR-1 to CR-6 

5. x
6. The contractor shall perform all work within the existing right of way.
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7. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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1. Notes shall be placed in the plans by the  Henry County Engineers Office directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-58 to ensure compliance with Federal notification requirements.
2. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and the Henry County Engineer, as required.
3. If any animals, snake, turtle, bird, salamander, etc. is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.


4. Due to the location of the following locations within the globally rare Oak Openings region, there shall be no earth disturbance.  No work shall be done off the existing pavement.  Care shall be taken to not disturb the existing vegetation. 
a. CR-3 from CR-U to CR- W
b. CR-4A from CR-U to CR-W
c. CR-7 from Liberty Center Corp to CR-U
d. CR-W from CR-1 to CR-4
e. CR-V from CR-1 to CR-6 

5. x
6. The contractor shall perform all work within the existing right of way.
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7. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Golnick Neal
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Golnick Neal ENV SPEC 2
	October 17, 2017

	Phoenix Golnick Neal ENV SPEC 2
	October 17, 2017
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