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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.


		Page 11 of 11
Contents
C1	3
Environmental Commitments, 	6
Environmental Commitments	8
C1	8
Preparers  & Approvals	9
Form Preparer(s)	9
Approvals & Electronic Signatures	9
Appendix	10
Uploaded Files by Report Section	10
General	10
Ecological	10
Permits	10

	
	 Environmental Document Level: C1
PID 101073 D02 RPM FY2019
Approved: November 9, 2017




[bookmark: _Toc256000000]C1	PID
	101073


	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This project is an annual contract to replace raised pavement markers throughout the district. All work is within the right of way and there are no utility impacts. Several locations are within special flood hazard areas, however the district 2 hydraulic engineer determined that there would be no impacts to the floodplain. No permits from the US Army Corps of Engineers are required due to ne work within any waters of the US. There will be no impacts to any ecologically or historically significant resources due to this project. A plan note will be added to the plans to ensure that no earth is disturbed within the Oak Openings Region of Fulton and Lucas Counties so there will be no impacts to any state or federally listed plant species. Construction will begin in the spring of 2019 and last through the fall of 2019. During construction, there will be rolling lane restrictions.
This document was approved based on Stage 2 plans.
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	Minimal Potential to Cause Effect - Appendix A


	Cultural Resources Coordination Date:
	06/07/2016


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(8) Installation of fencing, signs, pavement markings, small passenger shelters, traffic signals, and railroad warning devices where no substantial land acquisition or traffic disruption will occur. Examples include: The installation or maintenance of signs, pavement markings/raised pavement markers/sensors, traffic calming activities, and/or new or replacement fencing (right-of-way, vandal, etc.); General pavement marking or "line painting" projects.

	
	(22) Projects, as defined in 23 U.S.C. 101 that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way.
2. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
4. If any animals, snake, turtle, bird, or salamander is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.
5. Due to the location of the project within the globally rare Oak Openings region, there shall be no earth disturbance in these areas: 
a. FUL-109-0.00 to FUL-109-1.00 (FUL-5)
b. LUC-20A-0.48 to LUC-20A-3.47 (LUC-3)
d. LUC-2-2.23 to LUC-2-9.05 (LUC-6)
c. LUC-295-14.47 to LUC-295-16.55 (LUC-9)
d. LUC-20-9.19 to LUC-20-10.16 (LUC-2)
e. LUC-23-9.81 to LUC-23-11.4 (LUC-4)
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No work shall be done off the existing pavement in these areas.  Care shall be taken to not disturb the existing vegetation in these areas. 
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Commitments
1. The contractor shall perform all work within the existing right of way.
2. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
4. If any animals, snake, turtle, bird, or salamander is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.
5. Due to the location of the project within the globally rare Oak Openings region, there shall be no earth disturbance in these areas: 
a. FUL-109-0.00 to FUL-109-1.00 (FUL-5)
b. LUC-20A-0.48 to LUC-20A-3.47 (LUC-3)
d. LUC-2-2.23 to LUC-2-9.05 (LUC-6)
c. LUC-295-14.47 to LUC-295-16.55 (LUC-9)
d. LUC-20-9.19 to LUC-20-10.16 (LUC-2)
e. LUC-23-9.81 to LUC-23-11.4 (LUC-4)
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No work shall be done off the existing pavement in these areas.  Care shall be taken to not disturb the existing vegetation in these areas. 
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Phoenix Neal
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Neal ENV SPEC 2
	November 9, 2017

	Phoenix Neal ENV SPEC 2
	November 9, 2017
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Stage 2 Design.pdf
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Project Related OES Decision - Ecological.pdf
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District Determination - No Floodplain Impacts.pdf
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