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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	DISTRICT 2 PRODUCTION


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
This proposed project includes district wide (Henry, Fulton, Lucas, Ottawa, Sandusky, Seneca, Wood, and Williams County) pavement marking maintenance to re-paint pavement markings. This project will not impact any waters of the US or special flood hazard areas so no permits are required. Some locations are within 1,000 feet of the State Scenic Maumee and Sandusky Rivers however, this activity is an exempt activity and no notifications to the Ohio Department of Natural Resources (ODNR) Scenic Rivers are required. Extra care will be taken to not disturb any plants/animals, especially within the Oak Openings region. This project will not have any impacts on any historically significant resources. Construction is expected to begin in the spring of 2019 and continue throughout the year (winter 2019). The public will be notified of any traffic disruptions. 
This document was approved based on Stage 3 plans.
	STIP Reference #
	SLI 32


	Cultural Resources Coordination:
	Minimal Potential to Cause Effect - Appendix A


	Cultural Resources Coordination Date:
	11/08/2017


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101 that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,179,656.40 of Federal funds or with a total estimated cost of not more than $31,077,938.40 and with Federal funds that comprise less than 15 percent of the total estimated project cost (each amount adjusted annually by the Secretary to reflect any increases in the Consumer Price Index prepared by the Department of Labor, see www.fhwa.dot.gov or www.fta.dot.gov).


	Environmental Commitments:
	Yes
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1. The contractor shall perform all work within the existing right of way.
2. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
4. If any animals, snake, turtle, bird, or salamander is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.
5. The routes listed below in Lucas, Henry, and Fulton Counties are located within the globally rare Oak Openings region. Earth disturbance shall be the very minimum necessary to complete the work.  Care shall be taken to not disturb the existing vegetation as much as possible. 
FUL-20A-26.00 to 26.32
FUL-109-0.00-1.00
HEN-109-23.00 to 23.92
LUC-475-6.30 to 10.60
LUC-20-5.00 to 11.26
LUC-120-10.65 to 11.66
LUC-23-9.63 to 11.00
LUC-20A-0.00 to 6.60 
LUC-2-2.23 to 8.70
LUC-295-6.75 to 16.75
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1. The contractor shall perform all work within the existing right of way.
2. Part 642-58 of the Traffic Engineering Manual shall be placed in the plans by ODOT to ensure compliance with Federal notification requirements.  
3. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove any material that falls into the roadside ditches, streams, wetlands, or other waters through non-mechanical means. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
4. If any animals, snake, turtle, bird, or salamander is found within the project work limits, crews shall wait until the species has moved off of the project site unharmed before work can continue.
5. The routes listed below in Lucas, Henry, and Fulton Counties are located within the globally rare Oak Openings region. Earth disturbance shall be the very minimum necessary to complete the work.  Care shall be taken to not disturb the existing vegetation as much as possible. 
FUL-20A-26.00 to 26.32
FUL-109-0.00-1.00
HEN-109-23.00 to 23.92
LUC-475-6.30 to 10.60
LUC-20-5.00 to 11.26
LUC-120-10.65 to 11.66
LUC-23-9.63 to 11.00
LUC-20A-0.00 to 6.60 
LUC-2-2.23 to 8.70
LUC-295-6.75 to 16.75
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	Form Preparer
	District 2
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	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Neal ENV SPEC 2
	December 7, 2017

	Phoenix Neal ENV SPEC 2
	December 7, 2017
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District Determination - No Floodplain Impacts.pdf
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