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The environmental review, consultation, and other actions required by applicable Federal environmental laws for this project are being, or have been, carried-out by ODOT pursuant to 23 U.S.C. 327 and a Memorandum of Understanding dated December 11, 2015, and executed by FHWA and ODOT.
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	Project Sponsor
	Toledo, City of


	ODOT District
	2


	Funding Source
	Federal


	Private Funding:
	No


	
	


Project Description: 
The City of Toledo is proposing to install a parking bump-out and restripe Glanzman Rd from Byrne Rd to Detroit Ave in Lucas County Ohio. All work is within the existing right of way and there will be no impacts to utilities. There will be no impacts to any waters of the US so no permits from the US Army Corps of Engineers is required. This project does pass through a floodplain. Coordination with the local floodplain admin has been started and if a permit is required, it will be acquired prior to construction. There will be no impacts to any ecologically or historically significant resources as a result of this project. Construction is expected to begin in the summer of 2018 and last approximately 45 days. During construction, one lane of traffic will be maintained at all times. 
This document was approved based on Stage 1 plans. 
	STIP Reference #
	SLI 15


	Cultural Resources Coordination:
	Minimal Potential to Cause Effect - Appendix A


	Cultural Resources Coordination Date:
	11/08/2017


	Supporting documentation has been uploaded to Project File:
	Yes


	Select the appropriate project type (more than one can be selected):
	(22) Projects, as defined in 23 U.S.C. 101 that would take place entirely within the existing operational right-of-way. Existing operational right-of-way refers to right-of-way that has been disturbed for an existing transportation facility or is maintained for a transportation purpose. This area includes the features associated with the physical footprint of the transportation facility (including the roadway, bridges, interchanges, culverts, drainage, fixed guideways, mitigation areas, etc.) and other areas maintained for transportation purposes such as clear zone, traffic control signage, landscaping, any rest areas with direct access to a controlled access highway, areas maintained for safety and security of a transportation facility, parking facilities with direct access to an existing transportation facility, transit power substations, transit venting structures, and transit maintenance facilities. Portions of the right-of-way that have not been disturbed or that are not maintained for transportation purposes are not in the existing operational right-of-way. Examples include: Tower lighting within the existing operational right-of-way; Guardrail installation and replacement (including median cable barriers) where roadway ditches and backslopes will not be relocated; Improvements to existing ODOT/County maintenance facilities; Construction of new ODOT/County maintenance facilities within existing operational right-of-way; Environmental mitigation activities within existing operational right-of-way; Work on pedestrian and vehicle transfer structures and associated utilities, buildings, and terminals within existing operational right-of-way; Construction of alternative energy facilities (fuel tank farms, wind turbines, etc.)

	
	(23) Projects that receive less than $5,179,656.40 of Federal funds or with a total estimated cost of not more than $31,077,938.40 and with Federal funds that comprise less than 15 percent of the total estimated project cost (each amount adjusted annually by the Secretary to reflect any increases in the Consumer Price Index prepared by the Department of Labor, see www.fhwa.dot.gov or www.fta.dot.gov).


	Environmental Commitments:
	Yes


[bookmark: _Toc256000001]Environmental Commitments, 
1. The contractor shall perform all work within the existing right of way. 
2. Notes shall be placed in the plans by the City of Toledo directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-58 to ensure compliance with Federal notification requirements.
3. Appropriate local detour routes and accommodations shall be made by the City of Toledo and the Contractor for any local special events or festivals prior to the start of the event using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be added to the plans by the City of Toledo and implemented by the contractor during construction.
5. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and the City of Toledo, as required.
6. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove through non-mechanical means any material that falls into the roadside ditches, streams, wetlands, or other waters. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
7. If a floodplain permit is required, the City of Toledo shall acquire the permit prior to any work within the floodplain and the conditions shall be followed throughout construction by the contractor
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8. The City of Toledo and the contractor shall ensure that all pedestrian access is maintained through the construction zone at all times.
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Commitments
1. The contractor shall perform all work within the existing right of way. 
2. Notes shall be placed in the plans by the City of Toledo directing the contractor to comply with the notification requirement timeframes outlined in the Traffic Engineering Manual Part 642-58 to ensure compliance with Federal notification requirements.
3. Appropriate local detour routes and accommodations shall be made by the City of Toledo and the Contractor for any local special events or festivals prior to the start of the event using appropriate signage.
4. If required by local ordinance, a construction noise plan note will be added to the plans by the City of Toledo and implemented by the contractor during construction.
5. Adequate erosion and sediment controls shall be implemented and maintained throughout construction by the contractor and the City of Toledo, as required.
6. The contractor shall take all precautions to prevent any and all material from going off the edge of bridge deck(s) and edge of culvert(s) during all construction operations. The contractor shall immediately remove through non-mechanical means any material that falls into the roadside ditches, streams, wetlands, or other waters. Under no circumstances shall the contractor work in or store equipment and/or materials in any wetlands, streams, or other waters. No work or staging is permitted below the top of bank of any stream and/or within a wetland.
7. If a floodplain permit is required, the City of Toledo shall acquire the permit prior to any work within the floodplain and the conditions shall be followed throughout construction by the contractor
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8. The City of Toledo and the contractor shall ensure that all pedestrian access is maintained through the construction zone at all times.
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	Form Preparer
	District 2


	Supporting Form Preparer(s)
	Eli Barber, Phoenix Neal


[bookmark: _Toc256000006]Approvals & Electronic Signatures
	Approved & Electronically Signed By:
	Approval Date:


	Phoenix Neal ENV SPEC 2
	November 29, 2017

	Phoenix Neal ENV SPEC 2
	November 29, 2017
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USGS Quadrangle Topographical Map.pdf
Stage 1 Design.pdf
Aerial Map.pdf
County Map.pdf
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RMR Map.pdf
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Buckeye Assets Mapping.pdf
Project Study Area Map.pdf
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Eco map.pdf
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Water Source Protection Area Map.pdf
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FEMA FIRM.pdf
Coordination with Local Floodplain Administrator.pdf
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